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UPDATED FEB 2014
STATEMENT

IN LINE WITH THE CONDITIONS SET OUT WITHIN THE LICENCE

 (EAWML 100188)

BLAENAU GWENT COUNCIL HAS SET OUT THE FOLLOWING PLANS AND RISK ASSESSMENTS TO DEAL WITH THE DAY TO DAY OPERATION OF THE SITE, PLUS SAFEGUARD THE SITE FROM ANY POTENTIAL HAZARDS.
Dave Stevens
(COTC LICENCE HOLDER)
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Driver log/Incident report sheet

LOADING BAY – CENTRAL DEPOT, BARLEYFIELD IND EST, BRYNMAWR, NP23 4YF

Name




____________________________

Vehicle Reg


______________________

Date of tip off  

_____/_____/_____

Time of tip off 

____:_____(AM/PM)



PLEASE TICK AS APPROPRIATE.


Contamination in Bay





Bay is full and needs emptying      


Waste needs compacting

Skip is full (Needs emptying)


(Please indicate below any problems you have encountered)






Signed ________________________ 

Copy to Depot Manager and Operations Manager

SITE INSPECTION LOG

LOADING BAY – CENTRAL DEPOT, BARLEYFIELD IND EST, BRYNMAWR, NP23 4YF

Name

____________________________________

Date of inspection   
_____/_____/_____

Time of inspection 

____:_____(AM/PM)



PLEASE TICK AS APPROPRIATE.


Contamination in Bay





Bay is full and needs emptying      


Waste needs compacting

Skip is full (Needs emptying)


Action Required 






Signed ________________________ 

Copy to Depot Manager and Operations Manager


Please follow the instructions below in conjunction with your risk assessments for the safe deposit of gully and mechanical sweeper waste.

1) Upon arrival to the bay please check for any contamination or fly tipping.  If there are any problems please record in your ‘Incident Report Sheet’.

2) Please ensure you dewater as much as possible to prevent spillage over the road.

3) Only when the bay is clear, then you can reverse ensuring safety for passing cars and people.

4) Once the vehicle is stationary please eject the load safely.

5) At all times please be aware of the hazards within the waste such as syringes, glass and other sharp objects.

6) Upon successfully depositing the waste, please leave bay ready for next operative.

Street cleansing department, Central Depot, Barleyfield Ind Est, Brynmawr, NP23 4YF


Site Maintenance Schedule

1) fortnightly checks carried out by COTC officer and daily checks by driver to identify any problems such as contamination and fly tipping.

2) Regular cleansing of the drainage channel to avoid blockages is required.

3) Ensure waste is compacted to the rear of the drying bay to ensure maximum capacity.

4) Before leaving the area ensure signs and cones are left in front of bay to prevent any fly tipping.

5) If necessary wash down the bay ready for the next operative.

6) Periodic emptying of the interceptor and drains will be required through the use of the gully machine.

7) All staff should have the appropriate high viz, industrial gloves and safety footwear.

In accordance with the above maintenance schedule and the Driver’s instruction sheet there will be a duty for all drivers to inform the correct personnel if any problems arise.


Copy to All staff


	
	Environmental

Awareness
	Maintenance/Operations
	Accidents and Emergency
	

	
	COTC  LICENCE
	SUPERVISION OF SITE
	DUTY OF CARE
	WASTE STORAGE
	
	MAINTENANCE OF PLANT
	DRYING BAY
	
	
	
	FIRE PROCEDURE
	FLOOD PROCEDURE
	FAILURE OF SERVICES
	
	
	

	Transport/depot Manager
	
	√
	√
	√
	
	√
	
	
	
	
	√
	√
	√
	
	
	

	Security (Peter George)
	
	√
	
	√
	
	√
	√
	
	
	
	√
	√
	√
	
	
	

	Operations Manager
	√
	
	√
	√
	
	
	
	
	
	
	√
	√
	√
	
	
	

	Operator 1
	
	
	
	
	
	
	√
	
	
	
	
	
	√
	
	
	

	Operator 2
	
	
	
	
	
	
	√
	
	
	
	
	
	√
	
	
	

	Operator 3
	
	
	
	
	
	
	√
	
	
	
	
	
	√
	
	
	

	Contractor
	
	
	
	
	
	
	√
	
	
	
	
	
	√
	
	
	



	SITE DETAILS

	LOCATION: central Depot, Barleyfield Ind Est, Brynmawr

	POSTCODE: NP23 4YF

	SITE ACCESS GRID REFERENCE: S01911SW

	

	SITE CONTACTS
	OFFICE HOURS
	OUT OF HOURS

	TRANSPORT & DEPOT MANAGER
SECURITY

OPERATIONS MANAGER
	01495-355629
07977-893-377

07967-341-748

07977-491-073

01495-370125
	01495-311556
07977-893-377

07967-341-748

07977-491-073

01495-311556

	EMERGENCY SERVICES
	OFFICE HOURS
	OUT OF HOURS

	ALL EMERGENCY SERVICES
	999
	999

	REGULATORS
	OFFICE HOURS
	OUT OF HOURS

	NATURAL RESOURCES WALES
	02920-245-396
	08708-506-506

	UTILITIES
	OFFICE HOURS
	OUT OF HOURS

	WELSH WATER
	0800-085-3968


	0800-085-3968




	POSSIBLE ACCIDENT
	WHAT WOULD THE HARM BE
	HOW DO WE REDUCE THE CHANCES OF IT HAPPENING?
	WHAT TO DO IF IT HAPPENS

	Litter problems
	Blocked drains and flooding
	Ensure regular inspection of site and regular maintenance of the area.  Ensure appropriate grids are placed over drains.
	Clear the blockage immediately where possible, failing that, Close the area and lift all drain covers to identify root cause.  Clear blockage and put drain covers back.  Surplus surface water to be directed into drainage system.   Re-evaluate the current control measures and implement new risk plan.

	Odour Problems
	Nuisance to workers and businesses on site
	Ensure regular inspections and visibly make people aware of a contact number to report if problem is persistent.
	Get the site totally cleared of waste.  Wash down and disinfect entire area, followed by power wash.  If odour still persists then contact APT 01495 308048 who will deep clean entire area.

	Scavenging birds/animals
	Nuisance to local businesses and risk of disease.
	Ensure regular monitoring from Pest control.  
	Contract in place with P&P Pest control.  If situation is getting worse, then contact P&P on 01873 268123.  


	Waste is set on fire
	Harm to humans and buildings from fire and smoke damage.
	Regular movements of waste from site to prevent it being set on fire.  Ensure 24/7 CCTV is in operation.
	Immediately contact 999 for the fire service.  Re-evaluate the current control measures and implement new risk plan.

	Hazardous waste dumped
	Potential harm to humans/wildlife 
	Regular monitoring of site plus recorded CCTV of the area 24/7.
	Identify the nature of the waste and dispose of in the correct manner.  If in doubt contact the environment Agency 08708-506-506


Rejected waste loads – If the waste is rejected at landfill then a hazardous waste contractor will be notified to collect it.





Breakdowns – All vehicles are fitted with radios or mobile phones.  If a breakdown occurs the driver will note in the drivers defect book and call our transport department.  





Spillages – Any oil spillages will be logged by the driver, so the waste can then be picked up by a Hazardous waste carrier.





There is 24 hour CCTV in operation, which will help alleviate any fly tipping.





Working Plan





ACCIDENT MANAGEMENT PLAN





Weighbridge tickets and tracking information will be logged by the COTC officer.





In addition Driver will also fill out, Drivers defect book daily, and Drivers operators handbook





Driver fills out log/Incident report sheet’ – Name, Date, Time, Vehicle reg, Description of what is in bay, and notes for contamination.(Form A)





COTC officer checks the bay periodically each fortnight and fills in ‘Site Inspection log’, which consists of Date, Time, Name, Amount of waste in bay, Drain Inspection, and log of any contamination.(Form B)





When waste is suitably dry on the bay, it will be transferred to skip for disposal





Water from interceptor flows into foul sewer





Small Solids contained within interceptor





Small solids are sucked out of the interceptor once it is full





Waste is tipped at the top end of bay





Vehicle tips out waste (20-03-03)





Water drains from the waste into interceptor





Driver reverses vehicle into drying bay





Driver checks drying bay for any contaminants





Other issues





Treatment





Record Keeping





Waste Acceptance





Road Sweeper/ Gully Machine comes into depot





(





(





Records








FORM A





FORM B





TRAINING & AWARENESS





KEY SITE & EMERGENCY CONTACTS








