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	Issue
	Risk Assessment (High, Medium, Low)
	Prevention Measures
	Mitigation Measures

	Spillage of Cleaning Agents
	LOW
	· Correct storage, usage and disposal are ensured through our COSHH Assessment.
	· Minimum quantity of chemical stored and correct storage
· Regularly update COSHH folder by carrying out assessment and staff training.

	Spillage of waste fluids & Drainage mechanisms
	Medium
	· Waste fluids are stored in an appropriate bunded area.

· Relevant staff are trained in how to handle the various waste fluids correctly.

· Initially remove all/as much fluid from vehicles during the de-pollution process as possible.
	· Oil spill kits and materials have been installed at appropriate locations around the site.
· Oil interceptors have been installed as part of the drainage system. Processing areas are made of impermeable surface and sealed drainage. 
· Oil Spill Kits on site and on vehicle pick-up lorries.

	Spillage of Battery Acid
	Low
	· After removal from vehicles the batteries are placed directly into purpose built acid – proof containers. There are +100 special battery boxes available. Ensure sufficient quantities in each yard.
	· Box integrity checks included on weekly maintenance checklist.

	Fire on Site
	High
	· Processes involving the use of naked flames, such as oxygen fuelled cutting, are carried out only in well ventilated places away from flammable substances and by fully trained staff.
· Presence of flammable substances on site, such as recovered petrol.

· Ensure Cardiff site has had a comprehensive fire risk assessment. 
	· A fire Assessment has been carried out and the recommendations for improvement implemented.
· The correct fire extinguishers have been installed and serviced and a contract has been set up to ensure they are regularly maintained. 
· Correct fire safety signage has been set up around the site.

· Staff have received appropriate training. 

	Flood on Site
	Low
	· Suitable regularly maintained drainage system in place.
· Regularly check that stop valve on Cardiff drainage system is accessible and in working order. 
	· Ensure drainage system is maintained.
· Checks included on weekly checklist.

	Diesel Spillage
	Med
	· The diesel tanks are regularly checked and maintained.

· They are situated in a suitable sheltered bunded area.
· Ensure red diesel is stored correctly
	· Spillage absorbent has been installed at appropriate locations around the site so that any waste fluids can be cleaned up.

· Two oil interceptors have been installed in the yard to prevent spilt/leaked waste fluids from entering watercourses.

	BOC gas Leakage/Fire
	Med 
	· Processes involving the use of naked flames, oxygen fuelled cutting, are carried out only in well-ventilated places away from flammable substances and by fully trained staff.

· There is a purpose built storage area for the storage of BOC gas canisters when not in use.
	· A fire Assessment has been carried out.
· The correct fire extinguishers have been installed and serviced and a contract has been set up to ensure they are regularly maintained.
· All staff who carry out cutting are appropriately trained and licensed by external trainers. 
· Correct fire safety signage has been set up around the site.

· Oxygen and Propane gas canisters are stored in separate secure areas in the yard.

	Spillage & Storage of Antifreeze
	Low
	· Correct storage, usage and disposal are ensured through our COSHH Assessment.
	· Spill kits have been installed at appropriate locations around the site so that any waste fluids can be cleaned up.

	Noise
	High
	· Noise management plan (Ogmore Only)
	· As per noise management plan a number are imposed

· Operating hours

· Opening of new site

· Training

· Maintenance of equipment

· Operating & processing methods and techniques

· Checks on noise barrier included on checklist


