Environmental Risk assessment – Lamby Way IBA screening process 2015
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	Noise from delivery vehicle movements onsite and offloading
	Local residents (nearest dwelling 450m from operations)
	Air
	Traffic movements to be kept to working hours. Deliveries will be between 07:00 and 18:00. Driver will make every effort to minimise door slam noise, especially in windy weather.
	Medium
	Low
	Low

	Vibration from site
	Local residents (nearest dwelling 450m from operations)
	Land
	Any plant vibrations will be monitored on a daily bases and controlled via a preventative maintenance schedule
	Low
	Low
	Low

	Dust from deliveries, processing and handling
	Local residents (nearest dwelling 450m from operations) Wentloog flats SSSI (400m distant)                   Cors Crochydd Reen (350m distant)          River Runmey (650m distant)
	Air
	IBA arrives at Lamby Way already saturated with water from the cooling process and the Trident Park ERF in lorry's that are fully netted. This Ash is then loaded into the screener whilst still wet. The stockpile is outside so any rainfall also soaks into the stockpile and reduces the possibility or dust becoming airborne. This will be the case for all winter and spring months. If the summer weather causes the stockpile to dry out, CCC will bring in additional rescores to thoroughly damp down the stockpile. This will include but is not limited to parking a water bowser on top of the stockpile, and the possible use of water cannon/hoses to make sure that no dust leaves the site. The size of the stockpile will also be kept to a minimum to reduce the possible footprint of dust origin. 
	High
	Medium
	Low

	Run off from stockpile
	Wentloog flats SSSI (400m distant)                   Cors Crochydd Reen (350m distant)          River Runmey (650m distant)              Estury via surface water drainage (650m distant)
	Land/water
	The current screening operation is located within a natural "low" point on top of the landfill, bound by the operational are to the South and West, with the Cell 1 & 2 capping depth to the north an East providing a bunded area that will not allow any surface water to escape. The operation is located on uncapped Landfill so any water percolation will drain into the active landfill drainage system to be treated by the sites Leachate treatment plant.
	High
	Medium
	Low

	Run off/spillage of fuel/oil from screening machines
	Wentloog flats SSSI (400m distant)                   Cors Crochydd Reen (350m distant)          River Runmey (650m distant)              Estury via surface water drainage (650m distant)
	Land/water
	No fuel or oil stores are kept on site overnight. A minimum of three spill kits are kept on site in the event that an oil pipe bursts or fuel is spilt when fuelling up in the mornings.
	Medium
	Medium
	Low


