	Permit Number:
	EPR/PP3993VS
	
	Operator:
	Atlantic Recycling
	
	

	
	
	
	
	
	
	
	

	Facility:
	Atlantic Recycling
	Form Number:
	Surfacewater1 
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	Reporting of surface water monitoring for the period from November 2014 to December 2014


	Monitoring Point
	Substance / Parameter
	Trigger level
	Reference Period
	Result(1)
	Test

Method(2)
	Sample

Date and Times(3)
	Uncertainty (4)

	Outfall
	Suspended Solids, Total
	>250 mg/l (1 occasion)

>100 mg/l (3 consecutive occasions)

>60 mg/l (4 consecutive occasions)
	Monthly
	149 mg/l
	TM022
	12/12/2014  15:30
	Lab: Precision 1.48%, Bias -3.40%, Expanded Uncertainty 6.36%. Sampling: Immeasurable

	Outfall
	BOD, unfiltered
	>18 mg/l (1 occasion)

>10 mg/l (3 consecutive occasions)
	Monthly
	5.17 mg/l
	TM045
	12/12/2014  15:30
	Lab: Precision 8.52%, Bias -5.91%, Expanded Uncertainty 22.95%. Sampling: Immeasurable

	Outfall
	Ammoniacal Nitrogen as N
	>1 mg/l (1 occasion)

>0.5 mg/l (4 consecutive occasions)
	Monthly
	1.04 mg/l
	TM099
	12/12/2014  15:30
	Lab: Precision 2.40%, Bias 0.38%, Expanded Uncertainty 5.18%. Sampling: Immeasurable

	Outfall
	Conductivity
	>2000 µS/cm
	Monthly
	1.09 mS/cm
	TM120
	12/12/2014  15:30
	Lab: Precision 1.24%, Bias 3.07%, Expanded Uncertainty 5.56%. Sampling: Immeasurable

	Outfall
	Lead (diss.filt)
	>0.25 mg/l
	Monthly
	0.789 µg/l
	TM152
	12/12/2014  15:30
	Lab: Precision 2.40%, Bias -0.35%, Expanded Uncertainty 5.14%. Sampling: Immeasurable

	Outfall
	Nickel (diss.filt)
	>0.1 mg/l
	Monthly
	5.86 µg/l
	TM152
	12/12/2014  15:30
	Lab: Precision 3.74%, Bias -0.39%, Expanded Uncertainty 7.86%. Sampling: Immeasurable

	Outfall
	EPH Range >C10-C40 (aq)
	>2 mg/l
	Monthly
	600 µg/l
	TM172
	12/12/2014  15:30
	Lab: Precision 8.72%, Bias -13.34%, Expanded Uncertainty 30.79%. Sampling: Immeasurable

	Outfall
	EPH Range >C10-C20 (aq)
	>2 mg/l
	Monthly
	94.6 µg/l
	TM172
	12/12/2014  15:30
	Lab: Precision 8.72%, Bias -13.34%, Expanded Uncertainty 30.79%. Sampling: Immeasurable

	Outfall
	EPH Range >C20-C30 (aq)
	>2 mg/l
	Monthly
	266 µg/l
	TM172
	12/12/2014  15:30
	Lab: Precision 8.72%, Bias -13.34%, Expanded Uncertainty 30.79%. Sampling: Immeasurable

	Outfall
	EPH Range >C30-C40 (aq)
	>2 mg/l
	Monthly
	238 µg/l
	TM172
	12/12/2014  15:30
	Lab: Precision 8.72%, Bias -13.34%, Expanded Uncertainty 30.79%. Sampling: Immeasurable

	Outfall
	Sulphate
	>300 mg/l
	Monthly
	288 mg/l
	TM184
	12/12/2014  15:30
	Lab: Precision 6.67%, Bias 0.41%, Expanded Uncertainty 13.75%. Sampling: Immeasurable

	Outfall
	Chloride
	>300 mg/l
	Monthly
	87.3 mg/l
	TM184
	12/12/2014  15:30
	Lab: Precision 1.67%, Bias 1.28%, Expanded Uncertainty 4.63%. Sampling: Immeasurable

	Outfall
	Nitrite as N
	>1 mg/l
	Monthly
	0.0478 mg/l
	TM184
	12/12/2014  15:30
	Lab: Precision 0.74%, Bias 0.75%, Expanded Uncertainty 2.23%. Sampling: Immeasurable

	Outfall
	Phosphate (ortho) as PO4
	>1 mg/l
	Monthly
	0.335 mg/l
	TM184
	12/12/2014  15:30
	Lab: Precision 1.68%, Bias 0.12%, Expanded Uncertainty 3.48%. Sampling: Immeasurable

	Outfall
	Nitrate as N
	>1 mg/l
	Monthly
	0.618 mg/l
	TM184
	12/12/2014  15:30
	Lab: As per TON and Nitrite. Sampling: Immeasurable

	Outfall
	Total Oxidised Nitrogen as N
	>2 mg/l
	Monthly
	0.666 mg/l
	TM184
	12/12/2014  15:30
	Lab: Precision 3%, Bias 1.81%, Expanded Uncertainty 7.29% Sampling: Immeasurable

	Outfall
	Oxygen, dissolved
	<2 mg/l (1 occasion)

<5 mg/l (3 consecutive occasions)
	Monthly
	5.26 mg/l
	TM187
	12/12/2014  15:30
	Lab: Unknown. Sampling: Immeasurable

	Outfall
	Cadmium (tot.unfilt)
	>0.005 mg/l
	Monthly
	0.606 µg/l
	TM191
	12/12/2014  15:30
	Lab: Precision 3.38%, Bias -1.58%, Expanded Uncertainty 8.34%. Sampling: Immeasurable

	Outfall
	Zinc (tot.unfilt)
	>1 mg/l
	Monthly
	170 µg/l
	TM191
	12/12/2014  15:30
	Lab: Precision 6.18%, Bias -1.77%, Expanded Uncertainty 14.12%. Sampling: Immeasurable

	Outfall
	Calcium (tot.unfilt)
	>300 mg/l
	Monthly
	203 mg/l
	TM228
	12/12/2014  15:30
	Lab: Precision 4.64%, Bias -5.75%, Expanded Uncertainty 15.02%. Sampling: Immeasurable

	Outfall
	pH
	6.8 – 8.5
	Monthly
	8.11 pH Units
	TM256
	12/12/2014  15:30
	Lab: Precision 0.53%, Bias 0.88%, Expanded Uncertainty 1.95%. Sampling: Immeasurable

	Outfall
	GRO >C5-C12
	>2 mg/l
	Monthly
	<50 µg/l 
	TM245
	12/12/2014  15:30
	Lab: Precision 8.29%, Bias -0.37%, Expanded Uncertainty 16.95%. Sampling: Immeasurable

	Outfall
	GRO >C7-C8
	>2 mg/l
	Monthly
	<10 µg/l
	TM245
	12/12/2014  15:30
	Lab: Precision 8.29%, Bias -0.37%, Expanded Uncertainty 16.95%. Sampling: Immeasurable

	Outfall
	GRO >C5-C6
	>2 mg/l
	Monthly
	<10 µg/l
	TM245
	12/12/2014  15:30
	Lab: Precision 8.29%, Bias -0.37%, Expanded Uncertainty 16.95%. Sampling: Immeasurable

	Outfall
	GRO >C6-C7
	>2 mg/l
	Monthly
	<10 µg/l
	TM245
	12/12/2014  15:30
	Lab: Precision 8.29%, Bias -0.37%, Expanded Uncertainty 16.95%. Sampling: Immeasurable

	Outfall
	GRO >C8-C10
	>2 mg/l
	Monthly
	<10 µg/l
	TM245
	12/12/2014  15:30
	Lab: Precision 8.29%, Bias -0.37%, Expanded Uncertainty 16.95%. Sampling: Immeasurable

	Outfall
	GRO >C10-C12
	>2 mg/l
	Monthly
	<10 µg/l
	TM245
	12/12/2014  15:30
	Lab: Precision 8.29%, Bias -0.37%, Expanded Uncertainty 16.95%. Sampling: Immeasurable

	Outfall
	GRO >C5-C10
	>2 mg/l
	Monthly
	<10 µg/l
	TM245
	12/12/2014  15:30
	Lab: Precision 8.29%, Bias -0.37%, Expanded Uncertainty 16.95%. Sampling: Immeasurable

	SW09
	Suspended Solids, Total
	>250 mg/l (1 occasion)

>100 mg/l (3 consecutive occasions)

>60 mg/l (4 consecutive occasions)
	Monthly
	111 mg/l
	TM022
	12/12/2014  15:45
	Lab: Precision 1.48%, Bias -3.40%, Expanded Uncertainty 6.36%. Sampling: Immeasurable

	SW09
	BOD, unfiltered
	>18 mg/l (1 occasion)

>10 mg/l (3 consecutive occasions)
	Monthly
	3.22 mg/l
	TM045
	12/12/2014  15:45
	Lab: Precision 8.52%, Bias -5.91%, Expanded Uncertainty 22.95%. Sampling: Immeasurable

	SW09
	Ammoniacal Nitrogen as N
	>1 mg/l (1 occasion)

>0.5 mg/l (4 consecutive occasions)
	Monthly
	0.1 mg/l
	TM099
	12/12/2014  15:45
	Lab: Precision 2.40%, Bias 0.38%, Expanded Uncertainty 5.18%. Sampling: Immeasurable

	SW09
	Conductivity
	>2000 µS/cm
	Monthly
	0.543 mS/cm
	TM120
	12/12/2014  15:45
	Lab: Precision 1.24%, Bias 3.07%, Expanded Uncertainty 5.56%. Sampling: Immeasurable

	SW09
	Lead (diss.filt)
	>0.25 mg/l
	Monthly
	0.133 µg/l
	TM152
	12/12/2014  15:45
	Lab: Precision 2.40%, Bias -0.35%, Expanded Uncertainty 5.14%. Sampling: Immeasurable

	SW09
	Nickel (diss.filt)
	>0.1 mg/l
	Monthly
	3.31 µg/l
	TM152
	12/12/2014  15:45
	Lab: Precision 3.74%, Bias -0.39%, Expanded Uncertainty 7.86%. Sampling: Immeasurable

	SW09
	EPH Range >C10-C40 (aq)
	>2 mg/l
	Monthly
	178 µg/l
	TM172
	12/12/2014  15:45
	Lab: Precision 8.72%, Bias -13.34%, Expanded Uncertainty 30.79%. Sampling: Immeasurable

	SW09
	EPH Range >C10-C20 (aq)
	>2 mg/l
	Monthly
	<10 µg/l
	TM172
	12/12/2014  15:45
	Lab: Precision 8.72%, Bias -13.34%, Expanded Uncertainty 30.79%. Sampling: Immeasurable

	SW09
	EPH Range >C20-C30 (aq)
	>2 mg/l
	Monthly
	81.6 µg/l
	TM172
	12/12/2014  15:45
	Lab: Precision 8.72%, Bias -13.34%, Expanded Uncertainty 30.79%. Sampling: Immeasurable

	SW09
	EPH Range >C30-C40 (aq)
	>2 mg/l
	Monthly
	90.3 µg/l
	TM172
	12/12/2014  15:45
	Lab: Precision 8.72%, Bias -13.34%, Expanded Uncertainty 30.79%. Sampling: Immeasurable

	SW09
	Sulphate
	>300 mg/l
	Monthly
	118 mg/l
	TM184
	12/12/2014  15:45
	Lab: Precision 6.67%, Bias 0.41%, Expanded Uncertainty 13.75%. Sampling: Immeasurable

	SW09
	Chloride
	>300 mg/l
	Monthly
	30.4 mg/l
	TM184
	12/12/2014  15:45
	Lab: Precision 1.67%, Bias 1.28%, Expanded Uncertainty 4.63%. Sampling: Immeasurable

	SW09
	Nitrite as N
	>1 mg/l
	Monthly
	0.0313 mg/l
	TM184
	12/12/2014  15:45
	Lab: Precision 0.74%, Bias 0.75%, Expanded Uncertainty 2.23%. Sampling: Immeasurable

	SW09
	Phosphate (ortho) as PO4
	>1 mg/l
	Monthly
	0.163 mg/l
	TM184
	12/12/2014  15:45
	Lab: Precision 1.68%, Bias 0.12%, Expanded Uncertainty 3.48%. Sampling: Immeasurable

	SW09
	Nitrate as N
	>1 mg/l
	Monthly
	1.16 mg/l
	TM184
	12/12/2014  15:45
	Lab: As per TON and Nitrite. Sampling: Immeasurable

	SW09
	Total Oxidised Nitrogen as N
	>2 mg/l
	Monthly
	1.19 mg/l
	TM184
	12/12/2014  15:45
	Lab: Precision 3%, Bias 1.81%, Expanded Uncertainty 7.29% Sampling: Immeasurable

	SW09
	Oxygen, dissolved
	<2 mg/l (1 occasion)

<5 mg/l (3 consecutive occasions)
	Monthly
	7.89 mg/l
	TM187
	12/12/2014  15:45
	Lab: Unknown. Sampling: Immeasurable

	SW09
	Cadmium (tot.unfilt)
	>0.005 mg/l
	Monthly
	<0.5 µg/l
	TM191
	12/12/2014  15:45
	Lab: Precision 3.38%, Bias -1.58%, Expanded Uncertainty 8.34%. Sampling: Immeasurable

	SW09
	Zinc (tot.unfilt)
	>1 mg/l
	Monthly
	63 µg/l
	TM191
	12/12/2014  15:45
	Lab: Precision 6.18%, Bias -1.77%, Expanded Uncertainty 14.12%. Sampling: Immeasurable

	SW09
	Calcium (tot.unfilt)
	>300 mg/l
	Monthly
	87.9 mg/l
	TM228
	12/12/2014  15:45
	Lab: Precision 4.64%, Bias -5.75%, Expanded Uncertainty 15.02%. Sampling: Immeasurable

	SW09
	pH
	6.8 – 8.5
	Monthly
	7.85 pH Units
	TM256
	12/12/2014  15:45
	Lab: Precision 0.53%, Bias 0.88%, Expanded Uncertainty 1.95%. Sampling: Immeasurable

	SW09
	GRO >C5-C12
	>2 mg/l
	Monthly
	<50 µg/l 
	TM245
	12/12/2014  15:45
	Lab: Precision 8.29%, Bias -0.37%, Expanded Uncertainty 16.95%. Sampling: Immeasurable

	SW09
	GRO >C7-C8
	>2 mg/l
	Monthly
	<10 µg/l
	TM245
	12/12/2014  15:45
	Lab: Precision 8.29%, Bias -0.37%, Expanded Uncertainty 16.95%. Sampling: Immeasurable

	SW09
	GRO >C5-C6
	>2 mg/l
	Monthly
	<10 µg/l
	TM245
	12/12/2014  15:45
	Lab: Precision 8.29%, Bias -0.37%, Expanded Uncertainty 16.95%. Sampling: Immeasurable

	SW09
	GRO >C6-C7
	>2 mg/l
	Monthly
	<10 µg/l
	TM245
	12/12/2014  15:45
	Lab: Precision 8.29%, Bias -0.37%, Expanded Uncertainty 16.95%. Sampling: Immeasurable

	SW09
	GRO >C8-C10
	>2 mg/l
	Monthly
	<10 µg/l
	TM245
	12/12/2014  15:45
	Lab: Precision 8.29%, Bias -0.37%, Expanded Uncertainty 16.95%. Sampling: Immeasurable

	SW09
	GRO >C10-C12
	>2 mg/l
	Monthly
	<10 µg/l
	TM245
	12/12/2014  15:45
	Lab: Precision 8.29%, Bias -0.37%, Expanded Uncertainty 16.95%. Sampling: Immeasurable

	SW09
	GRO >C5-C10
	>2 mg/l
	Monthly
	<10 µg/l
	TM245
	12/12/2014  15:45
	Lab: Precision 8.29%, Bias -0.37%, Expanded Uncertainty 16.95%. Sampling: Immeasurable


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the 'minimum - maximum' measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Environment Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.

[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
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	Signed……………………………………………………………
	Date: January 2015.

	(Authorised to sign as representative of Operator)


	


Ahlim Hashm on behalf of Atlantic Recycling
Permit Number EPR/PP3993VS
