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HR:

Hazard Rating

	
	CATEGORY OR TASK
	WHO AT RISK
	HAZARD IDENTIFICATION
	H.R


	CURRENT RISK CONTROL MEASURES
	FURTHER ACTION TO CONTROL RISK
	H.R



	A
	Deposit of wastes/recyclates & materials


	Operatives

Sub-contractors

Site users
	Slips/falls 

Contact-damage

Injury
	H


	Specific areas designated for disposal/storage.

Personal protective clothing
Site management plan
	Ensure careful transfer/movement to waste receptacles.

Management to monitor
	L



	B
	Movement of waste containers
	Operatives

Sub-contractors

Site users


	Contact with people

Contact with plant/vehicles


	H


	Site operatives to supervise unloading/loading operations.

Limit movement during lifting operations.

Keep pedestrians/vehicles away from plant/lorry
	Maintain safety zone around area 

Management to monitor
	M

	C
	Lighting
	Operatives

Sub-contractors

Site users
	Slips, trips, falls

Contact with plant etc.
	H
	Sufficient natural/artificial lighting maintained
	Back-up light units to be sourced as required

Report failure ASAP
	L

	D


	Movement of wastes/recyclates products & materials 
	Operatives


	Injury due to carrying/lifting


	H


	Good manual handling techniques

Use of site plant by authorised/competent users

Awareness of Manual Handling Operations Regulations
	Management to monitor
HSE guidance displayed on notice board
	L

	E
F
	Manual handling operations (MHO)
General site operations & processing of wood
	Operatives(take due account of individual capabilities)
Operatives

Sub-contractors

Neighbouring properties


	Injury/damage to back/muscles etc.
Injury, crushing,

Entrapment,

Fall from height,
Struck by plant,

Burn from hot surfaces,

Electrocution,

Contact with hazardous materials.

Dust inhalation
	M
H
	Manual handling awareness

Guidance on maximum lifting e.g. 25 kg man or 16 kg woman

Use of lifting aids e.g. trolleys, site plant
Awareness of weight of loads, distance to be moved and underfoot conditions
Competent/Authorised users only.

Safety instructions in use

Daily check of safety operating systems i.e. guards, interlocks, emergency stops, supply, hydraulic leaks etc.

Use of appropriate PPE – HV, eye protection, gloves, helmet etc.  

Noise protection zones, assessments performed

Use of safety harness to secure point.

Maintain safety zone around loading operations.
Use of dust suppression, water sprays, use of PPE e.g. dust masks

Trained & authorised repairers only for breakdown/servicing/maintenance operations.

Isolate energy source prior to maintenance/service.

Use impervious gloves and overalls on fuelling/contact with diesel.

Use authorised method of use, access and structures to move around plant/equipment.
	Training/signage/notices

Assistance with 2 man lift 
Management to monitor.
Management to monitor.
No loose clothing in use or loose hair.

Erect warning signage.

Follow operators manual.

Maintain equipment and monitor emissions on and off site

Maintain access to emergency stops at all times.

Refer to COSHH data.
	L
M




	
	CATEGORY OR TASK
	WHO AT RISK
	HAZARD IDENTIFICATION
	H.R

	CURRENT RISK CONTROL MEASURES
	FURTHER ACTION TO CONTROL RISK
	HR


	G
	Recycling Area 


	Operatives

Sub-contractors

Site users
	Contact with falling objects

Contact with moving vehicles etc.

Movement of materials


	H

	Ensure regular pick-up/emptying of recyclate containers skips etc.

Supervision of container movement. 

Traffic management e.g. Banksman/reversing assistant (RA) to organise.

Personal protective clothing (PPE/HV) e.g. Suitable gloves to be used

Inspection/recording PPE use and issue
	Management to monitor

HSE Guidance displayed on notice board

	L


	H
	General site operations
	Operatives

Sub-contractors

Site users
	Contact with plant/vehicles

Hazardous wastes


	H

	Personal Protective Equipment/clothing/HV to be used.

Ensure non-standard wastes are brought to the attention of site management prior to moving.
	Follow emergency procedures/plans.

Management to monitor
Maintain vigilance by site staff.


	L


	 I
	Use of site plant/equipment
	    Operatives
	              Injury
	H
	Authorised/certificated users only 
	Management to monitor
	L

	
	
	
	Overturning

Contact

Contact with hazardous materials

Noise
	
	Maintain plant reversing aids, lights, horn etc. via schedule
Use of PPE while using fuels/diesel.

Noise protection zones, assessments performed
	Review COSHH information


	

	J

	Lone working


	Operatives


	Injury

Violence 


	M

	Use of telephone for communication.

Operative awareness/training.

Limited work activities.

Shortened periods of lone work.

Operators told to inform management of any site difficulties.  
	Management to monitor

	L


	K

	Waste container condition 

e.g. skip/bin
	Operatives

Site users

Sub-contractors
	Injury

Damage
	H

	Monitor for:

i. correct operation of door locking/opening        mechanism.

ii. Rust/corrosion

iii. Hooking points

iv.   Runners
Defect recording system
	Inform site management of all occurrences.

Inform waste carrier of all occurrences

Identification scheme to be organised

Management to monitor
	L

	L
	Use of conveyor & picking line system


	Operatives

Sub-contractors
	Injury

Entrapment

Falling objects

Noise
	H

	Trained operatives, instructions/toolbox talks
Warning signage, Emergency stop controls

Personnel protective equipment issued

Do not use with loose clothing/long hair
Hearing protection zones, signage, assessment
	Management to monitor 


	L


	M
N
	Fire
Work at Height
	
	
	
	SEE SPECIFIC RISK ASSESSMENT
SEE SPECIFIC RISK ASSESSMENT
	
	

	O
	Reversing Vehicles 

and 

Waste discharge


	Operatives

Drivers

Site users


	Struck by moving vehicles.

Falling from vehicles.

Vehicles colliding. 

Vehicle damage.

Traffic management

Speeding.

Vehicle condition.

Safe waste discharge.

Noise


	H


	No un-authorised pedestrians allowed during discharge operation. Safety Instructions issued via site rules.

Safety equipment (PPE/HV) to be used.

All drivers to take care when alighting.

Banksman/reversing assistant to be used. 

Competent operatives/drivers. 

No waste vehicles to use designated parking areas.

Traffic routes to be maintained, free from obstructions. Any damage to be repaired ASAP.  Dedicated pedestrian routes
Traffic to be monitored by site personnel/banksman.

Damage to be recorded and reported by site personnel e.g. reversing aids, mirrors.

As directed by site operatives.

Loads to be secure on entry and on exit.

Safe unloading practices to be followed.

Vehicle to be braked, on level ground and secure – stabilisers to be used.

Signage placed on items of plant etc.
	Management to monitor
Site signs to be in use as appropriate.


	M








Action: 1. Nominated personnel:








2. Target date:




