Permit Number: 
EPR/BV3715IL

Operator: 
SCA Hygiene Products UK Limited

Facility:

Oakenholt Paper Mill
Form Number: 
Water1 / 12.07.2013
Reporting of emissions to water (other than to sewer) and land for the period from 01.09.15 to 31.12.15
	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Uncertainty[4]

	W1
	Biochemical Oxygen Demand (BOD)
	50 mg/l
	24-hour flow proportional composite sample
	170 mg/L
	In accordance with TGN M18
	09/12/15 at 09:00
	LOD – 1 mg/L

	
	Chemical Oxygen Demand (COD)
	No limit set
	24-hour flow proportional composite sample
	390 mg/L
	In accordance with TGN M18
	26/11/15 at 09:00
	LOD – 10 mg/L

	
	Suspended Solids
	50 mg/l
	24-hour flow proportional composite sample
	120 mg/L
	In accordance with TGN M18
	17/11/15 at 09:00
	LOD – 5mg/L

	
	Temperature
	No limit set
	Instantaneous
	24.7°C
	Standard temperature sensor
	09/12/15 at 09:00
	In house

	
	Flow
	2200 m3/day
	Instantaneous
	2006 m3/day
	MCERTS self monitoring of effluent flow scheme
	24/12/15 at 04:00
	In house

	
	Flow (maximum instantaneous)
	30 l/sec
	Instantaneous
	87.72m3
	MCERTS self monitoring of effluent flow scheme
	20/12/15 at 04:00
	In house

	
	PH
	5 - 9
	Instantaneous
	Max: 7.71
Min: 6.63
	MCERTS approved instrumentation
	Max: 13/11/15 at 04:00
Min: 12/12/15 at 04:00
	In house

	
	Total Nitrogen
	16 mg/l
	24-hour flow proportional composite sample
	59 mg/L
	In accordance with TGN M18
	17/11/15 at 09:00
	LOD – 1mg/L

	
	Total Phosphorus
	No limit set
	24-hour flow proportional composite sample
	8.90 mg/L
	In accordance with TGN M18
	04/11/15 at 09:00
	LOD - 18µg/L

	
	Metals Zn, As, Cu, Cr, Ni, Pb
	No limit set
	24-hour flow proportional composite sample
	Zn = 93.1µg/l
As = 0.42 µg/l
Cu = 0.8 µg/l
Cr = <0.25 µg/l
Ni = <0.5 µg/l
Pb = <0.09 µg/l

	In accordance with TGN M18
	17/11/15 at 09:00 (All)
	LOD – 1.25 µg/l
LOD – 0.16 µg/l
LOD – 0.4 µg/l
LOD – 0.25 µg/l
LOD – 0.5 µg/l
LOD – 0.09 µg/l

	W2
	Suspended Solids
	50 mg/l
	Spot sample
	9 mg/L
	In accordance with TGN M18
	17/12/15
	In house

	
	PH
	5 - 9
	Spot sample
	Max: 7.60
Min: 6.88
	MCERTS approved instrumentation
	Max: 04/12/15
Min: 04/11/15
	In house

	
	Hydrocarbon oil
	15 mg/l
	Spot sample 
	0.13 mg/L
	In accordance with TGN M18
	21/10/15 at 09:00
	0.13 mg/l


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Environment Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed…………MIKE KING…..……………….  

Date 08/01/16

(Authorised to sign as representative of Operator)

Permit Number: 
EPR/BV3715IL


Operator: 
SCA Hygiene Products UK Limited


Facility:

Oakenholt Paper Mill

Form Number: 
Performance1 / 12.07.2013
Reporting of other performance indicators for the period 01.09.15 to 31.12.15
	Parameter
	Units

	
	

	NOx/ADT
	0.077 Tonnes/ADT 

	CO2/ADT
	0.36 Tonnes/ADT

	BOD/ADT
	0.27 Kg/ADT 

	Suspended Solids/ADT
	0.25 Kg/ADT

	Total Nitrogen
	0.18 Kg/ADT

	Total Phosphorus
	0.0049 Kg/ADT


	


Signed …… …………………Mike King…………………….  

Date…………08/01/16……………..   



(Authorised to sign as representative of Operator)

