[bookmark: _GoBack]Permit Number: 	EPR/BJ9681IX				Operator: 	SCA Hygiene Products UK Limited

Facility:		Oakenholt Paper Mill			Form Number: 	Performance 1 


Reporting of other performance indicators for the period……01 / 04 / 2019 ….. to ……30 / 06 / 2019 …….…

	Parameter
	
	Units 
	

	
	
	
	

	BOD
	0.110 Kg / Tonne
	

	Suspended solids
	0.180 Kg / Tonne
	

	Total Nitrogen
	0.0552 Kg / Tonne
	

	Total Phosphorous
	0.00969 Kg / Tonne
	

	NOx 
	4.884 Tonnes
	

	CO2
	6404.788 Tonnes
	

	AOX
	0.00335 Kg / Tonne 
	

	Total Energy Used
	43662.50 MWh
	

	Effluent Discharged
	147763 m3
	

	Water input to installation
	160574 Tonnes
	

	Water Discharged from installation
	147763 Tonnes
	



	Operator’s comments :
1m3 = 1 tonne for water input to installation
1m3 = 1 tonne for water discharge from installation 
Water discharge from installation = Effluent Discharged.
Total energy = Gas & Electricity consumption 






Signed ………Mike King………….  		Date…….08 / 07 /2019……	
	(Authorised to sign as representative of Operator)









Permit Number: 	EPR/BJ9681IX				Operator: 	SCA Hygiene Products UK Limited

Facility:		Oakenholt Paper Mill			Form Number: 	 Water 1 
Reporting of emissions to water (other than to sewer) and land for the period from …01 / 04 / 2019…. to …30 / 06 / 2019…...
	Emission
Point
	Substance /
Parameter
	Emission/
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	W1
	Biological Oxygen Demand (BOD)
	50 mg/l
	24-hour flow proportional composite sample
	33.1 mgL-1
	MCERTS self-monitoring of effluent flow scheme
	24/04/2019 04:00
	1 mgL-1

	W1
	Chemical Oxygen Demand (COD)
	--
	Spot Sample
	364 mgL-1
	MCERTS self-monitoring of effluent flow scheme
	24/04/2019 04:00
	10 mgL-1

	W1
	Total Suspended Solids
	50 mg/l
	24-hour flow proportional composite sample
	94.1 mgL-1
	MCERTS self-monitoring of effluent flow scheme
	24/04/2019 04:00
	5 mgL-1

	W1
	Total Mercury and its compounds
	--
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	-

	W1
	Total Cadmium and its compounds
	--
	24-hour flow proportional composite sample
	
	BS EN ISO5961:1995
	
	-

	W1
	pH
	5-9
	Instantaneous
	Maximum: 8.25 
Minimum: 6.79
	MCERTS self-monitoring of effluent flow scheme
	Maximum: 02/04/2019 07:00
Minimum: 28/05/2019     09:45
	-

	W1
	Dangerous Substances Screen
	--
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	-

	W1
	Temperature
	Maximum 25oC
	Instantaneous
	23.88°C
	MCERTS self-monitoring of effluent flow scheme
	29/06/2019 15:00
	
-


	W1
	Flow rate
	108 m3/hour
	Instantaneous
	102.69 m3 hr-1
	MCERTS self-monitoring of effluent flow scheme
	28/06/2019 14:30
	Less than +/- 8%

	W1
	Ammonia
	16mg/l
	24-hour flow proportional composite sample
	9.34 mgL-1
	BS EN ISO 11732 
or
ISBN 0117516139
	22/05/2019 09:00
	0.015 mgL-1

	W1
	Total Nitrogen
	--
	24-hour flow proportional composite sample
	11.4 mgL-1
	MCERTS self-monitoring of effluent flow scheme
	01/05/2019 09:00
	1 mgL-1

	W1
	Total Phosphorus
	--
	24-hour flow proportional composite sample
	2.32 mgL-1
	MCERTS self-monitoring of effluent flow scheme
	03/04/2019 09:00
	1.5 mgL-1

	W1
	AOx
	--
	24-hour flow proportional composite sample
	0.549 mgL-1
	MCERTS self-monitoring of effluent flow scheme
	24/04/2019 09:00
	0.01 mgL-1

	W1
	Pb
	--
	24-hour flow proportional composite sample
	<1 μgL-1
	MCERTS self-monitoring of effluent flow scheme
	10/04/2019 09:00
	1 μg/l

	W1
	Zn
	--
	24-hour flow proportional composite sample
	24 μgL-1
	MCERTS self-monitoring of effluent flow scheme
	10/04/2019 09:00
	5 μgL-1

	W1
	As
	--
	24-hour flow proportional composite sample
	<2 μgL-1
	MCERTS self-monitoring of effluent flow scheme
	10/04/2019 09:00
	2 μgL-1

	W1
	Cu
	--
	24-hour flow proportional composite sample
	<1 μgL-1
	MCERTS self-monitoring of effluent flow scheme
	10/04/2019 09:00
	1 μgL-1

	W1
	Cr
	--
	24-hour flow proportional composite sample
	<3 μgL-1
	MCERTS self-monitoring of effluent flow scheme
	10/04/2019 09:00
	3 μgL-1

	W1
	Ni
	--
	24-hour flow proportional composite sample
	1.87 μgL-1
	MCERTS self-monitoring of effluent flow scheme
	10/04/2019 09:00
	2 μgL-1







[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.


Signed …Mike King….….  		Date…… 08 / 07 / 2019 ….






















Essity Internal



