[bookmark: _GoBack]Permit Number: 	EPR/BJ9681IX				Operator: 	SCA Hygiene Products UK Limited

Facility:		Oakenholt Paper Mill			Form Number: 	Performance 1 


Reporting of other performance indicators for the period 01/09/16 to 31/12/16

	Parameter
	
	Units 
	

	
	
	
	

	BOD
	2896.87 Kg
	

	Suspended solids
	3327.97 Kg
	

	Total Nitrogen
	4561.69 Kg
	

	Total Phosphorous
	210.57 Kg
	

	NOx 
	4779.56 kg
	

	CO2
	6340 Tonne
	

	AOX
	Not measured
	

	Total Energy Used
	45,922.1317 Mwh
	

	Effluent Discharged
	137022 m3
	

	Water input to installation
	194 353 m3
	

	Water Discharged from installation
	137022 tonnes
	



	Operator’s comments :
Total energy used made up of total gas used and site electricity for time period.
Water input to installation is from fresh water useage for time period (assumed 1m3 =1tonne)
Water discharged from installation is the effluent sent out to estuary (assumed 1m3= 1 tonne)





Signed ………Mike King…………….  		Date………12/01/2017…..…..   	
	(Authorised to sign as representative of Operator)









Permit Number: 	EPR/BJ9681IX				Operator: 	SCA Hygiene Products UK Limited

Facility:		Oakenholt Paper Mill			Form Number: 	 Water 1 
Reporting of emissions to water (other than to sewer) and land for the period from 01/09/16 to 31/12/16
	Emission
Point
	Substance /
Parameter
	Emission/
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	W1
	Biological Oxygen Demand (BOD)
	50 mg/l
	24-hour flow proportional composite sample
	65 mg L-1
	MCERTS self-monitoring of effluent flow scheme
	04/10/2016
09:00

	LOD 1 mg/l

	W1
	Chemical Oxygen Demand (COD)
	--
	Spot Sample
	249 mg L-1
	MCERTS self-monitoring of effluent flow scheme
	04/10/2016 04:00
	In house 

	W1
	Total Suspended Solids
	50 mg/l
	24-hour flow proportional composite sample
	58 mg L-1
	MCERTS self-monitoring of effluent flow scheme
	18/10/16
	LOD 5 mg/l

	W1
	Total Mercury and its compounds
	--
	24-hour flow proportional composite sample
	<0.01 µg/l
	MCERTS self-monitoring of effluent flow scheme
	05/10/2016 09:00
	LOD <0.01 µg/l

	W1
	Total Cadmium and its compounds
	--
	24-hour flow proportional composite sample
	0.03 µg/l
	BS EN ISO5961:1995
	05/10/2016 09:00
	LOD < 0.03 µg / l

	W1
	pH
	5-9
	Instantaneous
	MAX - 8
MIN – 7
	MCERTS self-monitoring of effluent flow scheme
	MAX – 26/10/2016 04:00
MIN – 07/11/2016 04:00
	In house

	W1
	Dangerous Substances Screen
	--
	24-hour flow proportional composite sample
	-
	MCERTS self-monitoring of effluent flow scheme
	-
	-

	W1
	Temperature
	Maximum 40oC
	Instantaneous
	24.6°C
	MCERTS self-monitoring of effluent flow scheme
	24/11/2016
	In house

	W1
	Flow rate
	108 m3/hour
	Instantaneous
	108 m3 hr-1
	MCERTS self-monitoring of effluent flow scheme
	14/12/2016 04:00
	In house

	W1
	Ammonia
	16mg/l
	24-hour flow proportional composite sample
	7.9 mg L-1
	BS EN ISO 11732 
or
ISBN 0117516139
	04/10/2016 09:00
	LOD 0.015 mg/l

	W1
	Total Nitrogen
	--
	24-hour flow proportional composite sample
	230 mg L-1
	MCERTS self-monitoring of effluent flow scheme
	30/11/2016 09:00
	LOD 1 mg/l

	W1
	Total Phosphorus
	--
	24-hour flow proportional composite sample
	4.6 mg L-1
	MCERTS self-monitoring of effluent flow scheme
	01/11/2016 09:00
	LOD 0.18 mg/l 

	W1
	Pb
	--
	24-hour flow proportional composite sample
	0.41mg L-1

	MCERTS self-monitoring of effluent flow scheme
	01/10/2016 09:00
	LOG 0.09 µg/l

	W1
	Zn
	--
	24-hour flow proportional composite sample
	11 mg L-1
	MCERTS self-monitoring of effluent flow scheme
	01/10/2016 09:00
	LOD 1.3 µg/l

	W1
	As
	--
	24-hour flow proportional composite sample
	0.98 mg L-1
	MCERTS self-monitoring of effluent flow scheme
	01/10/2016 09:00
	LOD 0.16 µg/l

	W1
	Cu
	--
	24-hour flow proportional composite sample
	1.9 mg L-1
	MCERTS self-monitoring of effluent flow scheme
	01/10/2016 09:00
	LOD 0.4 µg/l

	W1
	Cr
	--
	24-hour flow proportional composite sample
	0.33 mg L-1
	MCERTS self-monitoring of effluent flow scheme
	01/10/2016 09:00
	 LOD 0.25 µg/l

	W1
	Ni
	--
	24-hour flow proportional composite sample
	1.8 mg L-1
	MCERTS self-monitoring of effluent flow scheme
	01/10/2016 09:00
	LOD 0.5 µg/l







[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.


Signed ………Mike King…….. ….  		Date……12/01/17…..

















Permit Number: 	EPR/BJ9681IX			Operator: 	SCA Hygiene Products UK Limited

Facility:		Oakenholt Paper Mill		Form Number: 	 Air 1 
Reporting of emissions to air for the period from DD/MM/2016 to DD/MM/2016 
	Emission
Point
	Substance /
Parameter
	Emission/
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1
	Oxides of Nitrogen
	250 mg/m3
	Hourly average
	
	
	
	

	
	
	
	
	
	
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …MIKE KING….  		Date……..
	
	(Authorised to sign as representative of Operator)


