Permit Number: 
EPR/BV3715IL

Operator: 
SCA Hygiene Products UK Limited

Facility:

Oakenholt Paper Mill
Form Number: 
Water1 / 12/07/2013
Reporting of emissions to water (other than to sewer) and land for the period from 01/01/2016 to 31/03/2016
	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Uncertainty[4]

	W1
	Biochemical Oxygen Demand (BOD)
	50 mg/l
	24-hour flow proportional composite sample
	80 mg/l
	In accordance with TGN M18
	12/01/2016 09:00
	LOD 1 mg/l

	
	Chemical Oxygen Demand (COD)
	No limit set
	24-hour flow proportional composite sample
	490 mg/l
	In accordance with TGN M18
	09/02/2016 04:00
	In house

	
	Suspended Solids
	50 mg/l
	24-hour flow proportional composite sample
	120 mg/l
	In accordance with TGN M18
	06/01/2016 04:00
	In house

	
	Temperature
	No limit set
	Instantaneous
	30°C
	Standard temperature sensor
	19/01/2016 04:00
	In house

	
	Flow
	2200 m3/day
	Instantaneous
	2115 m3/day
	MCERTS self monitoring of effluent flow scheme
	24/01/2016 04:00
	In house

	
	Flow (maximum instantaneous)
	108m3/hour
	Instantaneous
	94.7m3/hour
	MCERTS self monitoring of effluent flow scheme
	22/01/2016 04:00
	In house

	
	PH
	5 - 9
	Instantaneous
	MIN:  6.60

MAX: 7.96
	MCERTS approved instrumentation
	22/03/2016 04:00

30/01/2016 04:00
	In house

	
	Total Nitrogen
	16 mg/l
	24-hour flow proportional composite sample
	45 mg/l
	In accordance with TGN M18
	15/03/2016 04:00
	LOD 1 mg/l

	
	Total Phosphorus
	No limit set
	24-hour flow proportional composite sample
	2.2 mg/l
	In accordance with TGN M18
	15/03/2016 04:00
	LOD 18 ug/l

	
	Metals Zn, As, Cu, Cr, Ni, Pb
	No limit set
	24-hour flow proportional composite sample
	Zn 15 µg/l

As 0.60 µg/l

Cu 1.9 µg/l

Cr 0.52 µg/l

Ni 2.5 µg/l

Pb 0.36 µg/l
	In accordance with TGN M18
	09/02/2016 09:00
	LOD

Zn - 1.25 ug/l

As - 0.16 ug/l

Cu - 0.4 ug/l

CR - 0.25 ug/l

Ni - 0.5 ug/l

PB – 0.09 ug/l

	W2
	Suspended Solids
	50 mg/l
	Spot sample 
	5.8 mg/l
	In accordance with TGN M18
	13/01/2016 09:00
	In house

	
	PH
	5 - 9
	Spot sample 
	MIN: 6.52

MAX:7.3
	MCERTS approved instrumentation
	10/02/2016 09:00

04/03/2016 09:00
	In house

	
	Hydrocarbon oil
	15 mg/l
	Spot sample 
	0.11 mg/l
	In accordance with TGN M18
	13/01/2016 09:00
	LOD – 10 ug/l


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Environment Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …………MIKE KING………………….  

Date…11/04/16…..


(Authorised to sign as representative of Operator)

Permit Number: 
EPR/BV3715IL


Operator: 
SCA Hygiene Products UK Limited


Facility:

Oakenholt Paper Mill

Form Number: 
Performance1 / 12/07/2013
Reporting of other performance indicators for the period 01/01/2016 to 31/03/2016
	Parameter
	Units

	
	

	NOx/ADT
	0.28 Tonnes/ADT

	CO2/ADT
	0.36 Tonnes/ADT

	BOD/ADT
	0.29 Kg/ADT

	Suspended Solids/ADT
	0.22 Kg/ADT

	Total Nitrogen
	0.14 Kg/ADT

	Total Phosphorus
	0.007 Kg/ADT


	Operator’s comments :




Signed ……………MIKE KING……………………….  

Date………11/04/16………..   



(Authorised to sign as representative of Operator)

