Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.

Part A 
	Permit Number
	BG9681IX

	Name of operator
	SCA Hygiene UK Ltd

	Location of Facility
	Chester Road, Oakenholt, Flintshire, CH6 5PU

	Time and date of the detection 
	July 8th 2016


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	July 8th 2016

	Reference or description of the location of the event 
	This report is to support our notification by telephone of a near miss with the potential of release to estuary. During this week we have experienced two high results for suspended solids (83 & 59ppm).

	Description of where any release into the environment took place
	PM2 machine hall

	Substances(s) potentially released
	Dye

	Best estimate of the quantity or rate of  release of substances
	Best estimate would be 20 litres.

	Measures taken, or intended to be taken, to stop any emission
	· ETP was put into recirculation in order to contain, treat and further dilute the contents.
·  Both paper machines were closed whilst resolution was sought.
· MSDS checked.

· Advice sought from manufacturer.

· Testing carried out on Ph. / COD and suspended solids (all results were within limits)

· Monitoring frequency increased to six hourly

	Description of the failure or accident.
	Potential to release to estuary.


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	ETP

	Parameter(s)
	Suspended solids

	Limit
	50ppm

	Measured value and uncertainty
	83 & 59ppm

	Date and time of monitoring
	July 8th 2016

	Measures taken, or intended to be taken, to stop the emission
	· ETP was put into recirculation in order to contain, treat and further dilute the contents.

·  Both paper machines were closed whilst resolution was sought.

· MSDS checked.

· Advice sought from manufacturer.

· Testing carried out on Ph. / COD and suspended solids (all results were within limits)

· Monitoring frequency increased to six hourly


	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	None known / anticipated

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	


	Name*
	Mike King

	Post
	Environmental Leader

	Signature
	

	Date
	July 15th 2016


* authorised to sign on behalf of the operator

