Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.

Part A 
	Permit Number
	BJ9681IX

	Name of operator
	Essity UK Ltd Oakenholt Mill.

	Location of Facility
	Chester Road, Oakenholt, Flintshire, CH6 5PU

	Time and date of the detection 
	January 17th, 2018.


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	January 17th, 2018.

	Reference or description of the location of the event 
	Suspended solids test result from external laboratory showed 110mg/l against the permit limit of 50mg/l.

	Description of where any release into the environment took place
	None

	Substances(s) potentially released
	None

	Best estimate of the quantity or rate of release of substances
	None

	Measures taken, or intended to be taken, to stop any emission
	Checked for cleanliness and hygiene of sampling equipment, and all were re-cleaned.

	Description of the failure or accident.
	Potential to release out of consent suspended solids


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	W1

	Parameter(s)
	Suspended solids

	Limit
	50mg/l

	Measured value and uncertainty
	110mg/l

	Date and time of monitoring
	January 17th, 2018.

	Measures taken, or intended to be taken, to stop the emission
	ETP would have gone into recirculation mode, which would have added dilution water to the system. This would have lowered PPM levels before discharge.


	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	None known / anticipated

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	Suspended solids test result from external laboratory showed 110mg/l against the permit limit of 50mg/l.

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	ETP would have gone into recirculation mode, which would have added dilution water to the system. This would have lowered PPM levels before discharge. Results of internal monitoring did not indicate any out of consent results during this period.

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	Full investigation will be carried out.

	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	07/01/16, 19/01/16, 26/01/16, 17/03/16, 15/04/16, 16/05/16, 08/07/16, 19/08/16, 21/09/16, 18/10/16, 01/11/16, 06/02/17, 03/04/17, 26/04/17, 11/07/17, 11/08/17


	Name*
	Mike King

	Post
	Safety Specialist & Environmental Leader

	Signature
	

	Date
	26/01/2018


* authorised to sign on behalf of the operator



