Permit Number: 	EPR/BJ9681IX				Operator: 	SCA Hygiene Products UK Limited

Facility:		Oakenholt Paper Mill			Form Number: 	Performance 1 


Reporting of other performance indicators for the period DD/MM/2016 to DD/MM/2016

	Parameter
	
	Units 
	

	
	
	
	

	BOD
	kg
	

	Suspended solids
	kg
	

	Total Nitrogen
	kg
	

	Total Phosphorous
	kg
	

	NOx 
	Tonnes
	

	CO2
	Tonnes
	

	AOX
	Tonnes
	

	Total Energy Used
	MWh
	

	Effluent Discharged
	M3
	

	Water input to installation
	Tonnes
	

	Water Discharged from installation
	Tonnes
	



	Operator’s comments :








Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)









Permit Number: 	EPR/BJ9681IX				Operator: 	SCA Hygiene Products UK Limited

Facility:		Oakenholt Paper Mill			Form Number: 	 Water 1 
Reporting of emissions to water (other than to sewer) and land for the period from DD/MM/2016 to DD/MM/2016
	Emission
Point
	Substance /
Parameter
	Emission/
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	W1
	Biological Oxygen Demand (BOD)
	50 mg/l
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Chemical Oxygen Demand (COD)
	--
	Spot Sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Total Suspended Solids
	100 mg/l
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Total Mercury and its compounds
	--
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Total Cadmium and its compounds
	--
	24-hour flow proportional composite sample
	
	BS EN ISO5961:1995
	
	

	W1
	pH
	9
	Instantaneous
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Dangerous Substances Screen
	--
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Temperature
	Maximum 40oC
	Instantaneous
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Flow rate
	108 m3/hour
	Instantaneous
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Ammonia
	16mg/l
	24-hour flow proportional composite sample
	
	BS EN ISO 11732 
or
ISBN 0117516139
	
	

	W1
	Total Nitrogen
	--
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Total Phosphorus
	--
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	AOx
	--
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Pb
	--
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Zn
	--
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	As
	--
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Cu
	--
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Cr
	--
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	

	W1
	Ni
	--
	24-hour flow proportional composite sample
	
	MCERTS self-monitoring of effluent flow scheme
	
	







[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.


Signed …………………………………………………………….  		Date………………………..

















Permit Number: 	EPR/BJ9681IX			Operator: 	SCA Hygiene Products UK Limited

Facility:		Oakenholt Paper Mill		Form Number: 	 Air 1 
Reporting of emissions to air for the period from DD/MM/2016 to DD/MM/2016 
	Emission
Point
	Substance /
Parameter
	Emission/
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1
	Oxides of Nitrogen
	250 mg/m3
	Hourly average
	
	
	
	

	
	
	
	
	[bookmark: _GoBack]
	
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


