Schedule 6 – Notification

This page outlines the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.
Part A 

	Permit Number
	BV 7273

	Name of Operator
	Flintshire County Council 

Waste Management Service

	Location of Installation
	Brookhill Landfill Site, Pinfold Way, Buckley. CH7 3PL.

	
	

	Time and date of the detection
	11am August 2015 – Breaches in monthly groundwater / pond results. 
 


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, fugitive emission which as caused, is causing or may cause significant pollution.


	To be notified within 24 hours of detection

	Date and Time of the event
	11am August 2015

	Reference or description of the location of the event
	GW 2A, GW3A, GW4, P2

	Description of where any release into the environment took place 
	Brookhill perimeter  groundwater boreholes and pond 2

	Substances(s) potentially 
released 
	Ammoniacal Nitrogen, Chloride, COD, 

	Best estimate of the quantity or rate of release of substances
	Unknown

	Measures taken, or intended to be taken, to stop any emission 
	Ongoing GW investigation to discover cause. 

Pond 2 water retained and being treated through leachate plant.

	Description of failure or 

accident

	Breach in trigger levels

	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	GW 2A, GW3A, GW4, P2,

	Parameter(s) 
	(Ammoniacal Nitrogen), (Chloride), (COD) (SS)

	Limit
	(GW =1.7mg/l, P2 =1.6 mg/l), (GW = 60mg/l, P2 = 250mg/l) (P2= 100mg/l)  (P2=100mg/l) respectively

	Measured value and uncertainty 
	(<0.2mg/l, <0.07mg/l,<7mg/l , )respectively

	Date and time of monitoring 
	11am August 2015

	Measures taken, or intended to

be taken, to stop the emission  
	Ongoing GW investigation to discover cause. 

Pond 2 water retained and being treated through leachate plant.


	Time periods for notification following detection of a breach of a limit 

	Parameter 
	Notification period

	None
	

	
	


	( c )  Notification requirements for the detection of any significant adverse environmental effect 

	To be notified within 24 hours of detection

	Description of where the effect on
the environment was detected
	Notification period

	Substances(s) detected 
	Ammoniacal Nitrogen, Chloride, COD,SS 



	Concentrations of the substances

detected  
	Ammoniacal Nitrogen: GW2A = 16.4 mg/l.
GW 3A = 49.1 mg/l.

GW4 = 46 mg/l.
Chloride: GW2A = 137 mg/l. 
GW3A = 195 mg/l.
GW4 = 151 mg/l.
P2 = 3.05 mg/l

COD: P2 = 594 mg/l.
Suspended Solids: P2 = 1550 mg/l.

	Date of monitoring / sampling
	11am August 2015


Part B to be supplied as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment or harm which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	


	Name*
	Paul Murphy  

	Post
	Technical

	Signature
	

	Date
	


* authorised to sign on behalf of FCC
