Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1b
Reporting of emissions to air for the period from 01/07/14 to 31/12/14 

	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result 
	Test Method 
	Sample Date and Times 
	Uncertainty

	A1
	Particulates
	-
	
	(annual sampling for calibration of CEM completed 01/07/14)
	
	
	

	A1
	Sulphur Dioxide
	25 mg/m3
	2 hour average
	0.21 mg/m3
	BS EN 14791
	20/11/14, 08:55 – 10:55
	0.03 mg/m3

	A1
	Volatile Organic Compounds
	20 mg/m3
	Hourly average
	4.1 mg/m3
	BS EN 13526
	18/11/14, 11:30 – 15:30
	1.3 mg/m3

	A1
	Gaseous Fluorides (as HF)
	1 mg/m3
	Hourly average
	0.062 mg/m3
	BS ISO 15713
	18/11/14, 11:50 – 13:50
	0.008 mg/m3

	A1
	Hydrogen Chloride
	10 mg/m3
	Hourly average
	0.08 mg/m3
	BS EN 1911
	18/11/14, 09:20 – 11:20
	0.01 mg/m3

	A1
	Dioxins
	0.1 ng/m3
	4 hour average
	0.0043 ng/m3
	BS EN 1948
	30/06/14, 11:30 – 15:30
	0.0007 ng/m3

	
	
	
	
	
	
	
	

	A1
	Carbon Monoxide
	100 mg/m3
	Hourly average
	25.5 mg/m3
	BS EN 15058
	18/11/14, 11:30 – 15:30
	2.5 mg/m3

	
	
	
	
	
	
	
	

	A1
	Oxides of Nitrogen
	60 mg/m3
	Hourly average
	7.0 mg/m3
	BS EN 14792
	18/11/14, 11:30 – 15:30
	4.0 mg/m3


Signed …Joel Priest ……………………………………………………….  

Date……28/01/15………

(Authorised to sign as representative of Operator)

Results have been corrected as per condition 3.1.4

Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1c
Reporting of emissions to air for the period from 01/07/14 to 31/12/14
	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result 
	Test Method 
	Sample Date and Times 
	Uncertainty

	A12
	Particulates
	-
	
	(annual sampling for calibration of CEM completed 01/07/14)
	
	
	

	A12
	Sulphur Dioxide
	25 mg/m3
	2 hour average
	1.94 mg/m3
	BS EN 14791
	20/11/14, 08:55 – 10:55
	0.26 mg/m3

	A12
	Volatile Organic Compounds
	20 mg/m3
	Hourly average
	10 mg/m3 

(actual result given – result minus uncertainty is -1.3 mg/m3)
	BS EN 13526
	18/11/14, 11:30 – 15:30
	11.3 mg/m3

	A12
	Gaseous Fluorides (as HF)
	1 mg/m3
	Hourly average
	0.48 mg/m3
	BS ISO 15713
	18/11/14, 11:50 – 13:50
	0.07 mg/m3

	A12
	Hydrogen Chloride
	10 mg/m3
	Hourly average
	0.19 mg/m3
	BS EN 1911
	18/11/14, 09:20 – 11:20
	0.03 mg/m3

	A12
	Dioxins
	0.1 ng/m3
	4 hour average
	0.008 ng/m3
	BS EN 1948
	18/11/14, 11:30 – 15:30
	0.002 ng/m3

	
	
	
	
	
	
	
	

	A12
	Carbon Monoxide
	100 mg/m3
	Hourly average
	28.9 mg/m3
	BS EN 15058
	18/11/14, 11:30 – 15:30
	2.1 mg/m3

	
	
	
	
	
	
	
	

	A12
	Oxides of Nitrogen
	60 mg/m3
	Hourly average
	7.9 mg/m3
	BS EN 14792
	18/11/14, 11:30 – 15:30
	4.1 mg/m3


Signed …Joel Priest………………………………………………………….  

Date……28/01/15………

(Authorised to sign as representative of Operator)

Results have been corrected as per condition 3.1.4

Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1d
Reporting of emissions to air for the year ……2014……
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Reference Period
	Result 
	Test

Method 
	Sample

Date and Times 
	Uncertainty



	A13
	Particulates
	-
	4 hour average
	0.28 mg/m3
(actual result given – result minus uncertainty is -0.02 mg/m3) mg/m3
	BS EN 13284
	02/07/14, 09:03 – 13:32
	0.30 mg/m3

	A13
	Carbon monoxide
	150mg/m3
	Hourly average
	3.2 mg/m3
	BS EN 15058
	02/07/14, 09:08 – 13:08
	2.6 mg/m3

	
	
	
	
	
	
	
	

	A13
	Oxides of nitrogen
	60mg/m3
	Hourly average
	9.8 mg/m3
	BS EN 14792
	02/07/14, 09:08 – 13:08
	4.2 mg/m3


Signed …Joel Priest………………………………………………………….  

Date……04/08/14……………

(Authorised to sign as representative of Operator)
Results have been corrected as per condition 3.1.4

