Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1b
Reporting of emissions to air for the period from 01/01/15 to 30/06/15 

	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result 
	Test Method 
	Sample Date and Times 
	Uncertainty

	A1
	Particulates
	-
	4 hour average
	3.10 mg/m3
	BS EN 13284
	23/06/15, 10:00 – 15:32
	0.40 mg/m3

	A1
	Sulphur Dioxide
	25 mg/m3
	2 hour average
	0.43 mg/m3
	BS EN 14791
	24/06/15, 11:05 – 13:05
	0.06 mg/m3

	A1
	Volatile Organic Compounds
	20 mg/m3
	Hourly average
	5.1 mg/m3
	BS EN 13526
	23/06/15, 16:30 – 20:30
	1.3 mg/m3

	A1
	Gaseous Fluorides (as HF)
	1 mg/m3
	Hourly average
	0.68 mg/m3
	BS ISO 15713
	23/06/15, 10:41 – 12:41
	0.09 mg/m3

	A1
	Hydrogen Chloride
	10 mg/m3
	Hourly average
	0.008 mg/m3
	BS EN 1911
	23/06/15, 12:50 – 14:50
	0.002 mg/m3

	A1
	Dioxins
	0.1 ng/m3
	4 hour average
	0.0007 ng/m3
	BS EN 1948
	24/06/15, 10:04 – 14:04
	0.0003 ng/m3

	
	
	
	
	
	
	
	

	A1
	Carbon Monoxide
	100 mg/m3
	Hourly average
	61.4 mg/m3
	BS EN 15058
	23/06/15, 16:30 – 20:30
	2.6 mg/m3

	
	
	
	
	
	
	
	

	A1
	Oxides of Nitrogen
	60 mg/m3
	Hourly average
	4.7 mg/m3
	BS EN 14792
	23/06/15, 16:30 – 20:30
	4.1 mg/m3


Signed …Joel Priest ……………………………………………………….  

Date……07/08/15………

(Authorised to sign as representative of Operator)

Results have been corrected as per condition 3.1.4

Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1c
Reporting of emissions to air for the period from 01/01/15 to 30/06/15
	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result 
	Test Method 
	Sample Date and Times 
	Uncertainty

	A12
	Particulates
	-
	4 hour average
	0.67 mg/m3
	BS EN 13284
	23/06/15, 10:00 – 15:32
	0.24 mg/m3

	A12
	Sulphur Dioxide
	25 mg/m3
	2 hour average
	10.6 mg/m3
	BS EN 14791
	24/06/15, 11:05 – 13:05
	1.4 mg/m3

	A12
	Volatile Organic Compounds
	20 mg/m3
	Hourly average
	16.6 mg/m3
	BS EN 13526
	23/06/15, 16:30 – 20:30
	1.4 mg/m3

	A12
	Gaseous Fluorides (as HF)
	1 mg/m3
	Hourly average
	0.07 mg/m3
	BS ISO 15713
	23/06/15, 10:42 – 12:42
	0.01 mg/m3

	A12
	Hydrogen Chloride
	10 mg/m3
	Hourly average
	0.017 mg/m3
	BS EN 1911
	23/06/15, 12:50 – 14:50
	0.003 mg/m3

	A12
	Dioxins
	0.1 ng/m3
	4 hour average
	0.06 ng/m3
	BS EN 1948
	24/06/15, 10:04 – 14:04
	0.02 ng/m3

	
	
	
	
	
	
	
	

	A12
	Carbon Monoxide
	100 mg/m3
	Hourly average
	27.0 mg/m3
	BS EN 15058
	23/06/15, 16:30 – 20:30
	2.0 mg/m3

	
	
	
	
	
	
	
	

	A12
	Oxides of Nitrogen
	60 mg/m3
	Hourly average
	3.5 mg/m3 

(actual result given as result minus uncertainty = -0.6 mg/m3)
	BS EN 14792
	23/06/15, 16:30 – 20:30
	4.1 mg/m3


Signed …Joel Priest………………………………………………………….  

Date……07/08/15………

(Authorised to sign as representative of Operator)

Results have been corrected as per condition 3.1.4

Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1d
Reporting of emissions to air for the year ……2015……
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Reference Period
	Result 
	Test

Method 
	Sample

Date and Times 
	Uncertainty



	A13
	Particulates
	-
	4 hour average
	2.16 mg/m3
	BS EN 13284
	02/07/14, 09:03 – 13:32
	0.34 mg/m3

	A13
	Carbon monoxide
	150mg/m3
	Hourly average
	3.6 mg/m3
	BS EN 15058
	02/07/14, 09:08 – 13:08
	2.0 mg/m3

	
	
	
	
	
	
	
	

	A13
	Oxides of nitrogen
	60mg/m3
	Hourly average
	13.9 mg/m3
	BS EN 14792
	02/07/14, 09:08 – 13:08
	4.1 mg/m3


Signed …Joel Priest………………………………………………………….  

Date……07/08/15……………

(Authorised to sign as representative of Operator)
Results have been corrected as per condition 3.1.4

