Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1b
Reporting of emissions to air for the period from 01/01/16 to 30/06/16 

	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result 
	Test Method 
	Sample Date and Times 
	Uncertainty

	A1
	Particulates
	-
	
	(annual sampling for calibration of CEM completed 29/06/16)
	
	
	

	A1
	Sulphur Dioxide
	25 mg/m3
	2 hour average
	0.09 mg/m3
	BS EN 14791
	29/06/16, 08:35 – 10:35
	0.01 mg/m3

	A1
	Volatile Organic Compounds
	20 mg/m3
	Hourly average
	12.7 mg/m3
	BS EN 13526
	28/06/16, 20:00 – 00:00
	1.3 mg/m3

	A1
	Gaseous Fluorides (as HF)
	1 mg/m3
	Hourly average
	0.025 mg/m3
	BS ISO 15713
	28/06/16, 12:08 – 12:08
	0.005 mg/m3

	A1
	Hydrogen Chloride
	10 mg/m3
	Hourly average
	0.12 mg/m3
	BS EN 1911
	28/06/16, 12:28 – 14:28
	0.02 mg/m3

	A1
	Dioxins
	0.1 ng/m3
	4 hour average
	0.031 ng/m3
	BS EN 1948
	28/06/16, 10:08 – 14:08
	0.009 ng/m3

	
	
	
	
	
	
	
	

	A1
	Carbon Monoxide
	100 mg/m3
	Hourly average
	51.4 mg/m3
	BS EN 15058
	28/06/16, 20:00 – 00:00
	2.6 mg/m3

	
	
	
	
	
	
	
	

	A1
	Oxides of Nitrogen
	60 mg/m3
	Hourly average
	9.9 mg/m3
	BS EN 14792
	28/06/16, 20:00 – 00:00
	4.1 mg/m3


Signed …Joel Priest ……………………………………………………….  

Date……27/07/16………

(Authorised to sign as representative of Operator)

Results have been corrected as per condition 3.1.4

Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1c
Reporting of emissions to air for the period from 01/01/16 to 30/06/16
	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result 
	Test Method 
	Sample Date and Times 
	Uncertainty

	A12
	Particulates
	-
	
	(annual sampling for calibration of CEM completed 30/06/16)
	
	
	

	A12
	Sulphur Dioxide
	25 mg/m3
	2 hour average
	1.05 mg/m3
	BS EN 14791
	30/06/16, 08:35 – 10:35
	0.15 mg/m3

	A12
	Volatile Organic Compounds
	20 mg/m3
	Hourly average
	10.7 mg/m3
	BS EN 13526
	29-30/06/16, 21:40 – 01:40
	1.3 mg/m3

	A12
	Gaseous Fluorides (as HF)
	1 mg/m3
	Hourly average
	0.11 mg/m3
	BS ISO 15713
	30/06/16, 11:00 – 13:00
	0.02 mg/m3

	A12
	Hydrogen Chloride
	10 mg/m3
	Hourly average
	0.12 mg/m3
	BS EN 1911
	01/07/16, 08:30 – 10:30
	0.02 mg/m3

	A12
	Dioxins
	0.1 ng/m3
	4 hour average
	0.00 ng/m3
	BS EN 1948
	30/06/16, 08:35 – 12:35
	0.02 ng/m3

	
	
	
	
	
	
	
	

	A12
	Carbon Monoxide
	100 mg/m3
	Hourly average
	49.0 mg/m3
	BS EN 15058
	29-30/06/16, 21:40 – 01:40
	10.0 mg/m3

	
	
	
	
	
	
	
	

	A12
	Oxides of Nitrogen
	60 mg/m3
	Hourly average
	8.9 mg/m3 
	BS EN 14792
	29-30/06/16, 21:40 – 01:40
	4.1 mg/m3


Signed …Joel Priest………………………………………………………….  

Date……27/07/16………

(Authorised to sign as representative of Operator)

Results have been corrected as per condition 3.1.4

Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1d
Reporting of emissions to air for the year ……2016……
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Reference Period
	Result 
	Test

Method 
	Sample

Date and Times 
	Uncertainty



	A13
	Particulates
	-
	
	(annual sampling for calibration of CEM completed 27/06/16)
	
	
	

	A13
	Carbon monoxide
	150mg/m3
	Hourly average
	13.5 mg/m3
	BS EN 15058
	27/06/16, 10:41 – 14:41
	2.5 mg/m3

	
	
	
	
	
	
	
	

	A13
	Oxides of nitrogen
	60mg/m3
	Hourly average
	14.8 mg/m3
	BS EN 14792
	27/06/16, 10:41 – 14:41
	4.2 mg/m3


Signed …Joel Priest………………………………………………………….  

Date……27/07/16……………

(Authorised to sign as representative of Operator)
Results have been corrected as per condition 3.1.4

