Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1b
Reporting of emissions to air for the period from 01/07/15 to 31/12/15 

	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result 
	Test Method 
	Sample Date and Times 
	Uncertainty

	A1
	Particulates
	-
	
	(annual sampling for calibration of CEM completed 23/06/15)
	
	
	

	A1
	Sulphur Dioxide
	25 mg/m3
	2 hour average
	0.37 mg/m3
	BS EN 14791
	10/11/15, 12:00 – 14:00
	0.05 mg/m3

	A1
	Volatile Organic Compounds
	20 mg/m3
	Hourly average
	11.3 mg/m3
	BS EN 13526
	10/11/15, 09:45 – 13:45
	2.7 mg/m3

	A1
	Gaseous Fluorides (as HF)
	1 mg/m3
	Hourly average
	0.03 mg/m3
	BS ISO 15713
	09/11/15, 12:50 – 14:50
	0.01 mg/m3

	A1
	Hydrogen Chloride
	10 mg/m3
	Hourly average
	0.53 mg/m3
	BS EN 1911
	10/11/15, 09:45 – 11:45
	0.07 mg/m3

	A1
	Dioxins
	0.1 ng/m3
	4 hour average
	0.01 ng/m3
	BS EN 1948
	09/11/15, 11:15 – 15:15
	0.0003 ng/m3

	
	
	
	
	
	
	
	

	A1
	Carbon Monoxide
	100 mg/m3
	Hourly average
	72.9 mg/m3
	BS EN 15058
	10/11/15, 09:45 – 13:45
	5.1 mg/m3

	
	
	
	
	
	
	
	

	A1
	Oxides of Nitrogen
	60 mg/m3
	Hourly average
	2.8 mg/m3
	BS EN 14792
	10/11/15, 09:45 – 13:45
	8.2 mg/m3


Signed …Joel Priest ……………………………………………………….  

Date……05/01/16………

(Authorised to sign as representative of Operator)

Results have been corrected as per condition 3.1.4

Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1c
Reporting of emissions to air for the period from 01/07/15 to 31/12/15
	Emission Point
	Substance / Parameter
	Emission Limit Value
	Reference Period
	Result 
	Test Method 
	Sample Date and Times 
	Uncertainty

	A12
	Particulates
	-
	
	(annual sampling for calibration of CEM completed 23/06/15)
	
	
	

	A12
	Sulphur Dioxide
	25 mg/m3
	2 hour average
	0.14 mg/m3
	BS EN 14791
	10/11/15, 12:00 – 14:00
	0.02 mg/m3

	A12
	Volatile Organic Compounds
	20 mg/m3
	Hourly average
	1.8 mg/m3
	BS EN 13526
	09/11/15, 16:00 – 20:00
	2.7 mg/m3

	A12
	Gaseous Fluorides (as HF)
	1 mg/m3
	Hourly average
	0.08 mg/m3
	BS ISO 15713
	09/11/15, 12:50 – 14:50
	0.01 mg/m3

	A12
	Hydrogen Chloride
	10 mg/m3
	Hourly average
	0.11 mg/m3
	BS EN 1911
	10/11/15, 09:45 – 11:45
	0.02 mg/m3

	A12
	Dioxins
	0.1 ng/m3
	4 hour average
	0.024 ng/m3
	BS EN 1948
	09/11/15, 11:15 – 15:15
	0.006 ng/m3

	
	
	
	
	
	
	
	

	A12
	Carbon Monoxide
	100 mg/m3
	Hourly average
	28.0 mg/m3
	BS EN 15058
	09/11/15, 16:00 – 20:00
	5.0 mg/m3

	
	
	
	
	
	
	
	

	A12
	Oxides of Nitrogen
	60 mg/m3
	Hourly average
	0.9 mg/m3 
	BS EN 14792
	09/11/15, 16:00 – 20:00
	8.2 mg/m3


Signed …Joel Priest………………………………………………………….  

Date……05/01/16………

(Authorised to sign as representative of Operator)

Results have been corrected as per condition 3.1.4

Permit Number: 
EA/EPR/BK3638IF/V002


Operator: 

Hydro Aluminium Deeside

Facility:

Wrexham Aluminium Works

Form Number: 
 Air1d
Reporting of emissions to air for the year ……2015……
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Reference Period
	Result 
	Test

Method 
	Sample

Date and Times 
	Uncertainty



	A13
	Particulates
	-
	4 hour average
	2.16 mg/m3
	BS EN 13284
	25/06/14, 08:58 – 13:21
	0.34 mg/m3

	A13
	Carbon monoxide
	150mg/m3
	Hourly average
	3.6 mg/m3
	BS EN 15058
	25/06/14, 09:15 – 13:15
	2.0 mg/m3

	
	
	
	
	
	
	
	

	A13
	Oxides of nitrogen
	60mg/m3
	Hourly average
	13.9 mg/m3
	BS EN 14792
	25/06/14, 09:15 – 13:15
	4.1 mg/m3


Signed …Joel Priest………………………………………………………….  

Date……07/08/15……………

(Authorised to sign as representative of Operator)
Results have been corrected as per condition 3.1.4

