[bookmark: _GoBack]Permit Number: 	EPR/BK6483IU					Operator: 		Toyota Motor manufacturing (UK) Limited

Facility:		Deeside Engine Casting Plant			Form Number: 	Sewer1 / 18/12/17
Reporting of emissions to sewer for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	S1
	Suspended solids
	200 mg/l
	Composite of continuous sampling in a 24 hour period
	
	BS EN 872
	
	

	
	Chemical oxygen demand
	1500 mg/l
	Composite of continuous sampling in a 24 hour period
	
	BS 6068-2.34
	
	

	
	Hydrocarbon oils
	150 mg/l
	Composite of continuous sampling in a 24 hour period
	
	SCA blue book 77 ISBN0117517283
	
	

	
	Copper and its compounds expressed as Cu
	1 mg/l
	Composite of continuous sampling in a 24 hour period
	
	BS EN ISO 11885
	
	

	
	Zinc and its compounds expressed as Zn 
	2 mg/l
	Composite of continuous sampling in a 24 hour period
	
	BS EN ISO 11885
	
	

	
	Lead and its compounds expressed as Pb
	1 mg/l
	Composite of continuous sampling in a 24 hour period
	
	BS EN ISO 11885
	
	

	
	Nickel and its compounds expressed as Ni
	1 mg/l
	Composite of continuous sampling in a 24 hour period
	
	BS EN ISO 11885
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)

