Permit Reference Number: BL1096IB/V012                






Operator: Castle Cement Ltd

Installation: Padeswood Works                                          






Form Number: S4 / A1

Six-monthly Reporting of Emissions to Air from Emission Point A8 for the period 1st January 2015 to 31st December 2015
	Substance / Parameter
	Emission Limit Level / Unit
	Result (1)
	Test Method2
	Sample Date & Times(3)
	Accreditation/ Certification (4)
	Uncertainty

(5)

	
	
	First 6 Months
	Second 6 Months
	
	
	
	

	Hydrogen Fluoride
	1mg/m3 over minimum 1 hour period / mg/Nm3
	0.027
	
	ISO 15713
	05-May-15

15:50 - 18:28
	MCERTS
	26

	Cadmium & thallium and their compounds (total)
	0.05mg/m3 over minimum 30 min, max 8 hr period / mg/Nm3
	0.0012
	
	BS EN 14385
	28-Apr-15

15:10 - 19:14
	MCERTS
	16

	Mercury and its compounds
	0.05mg/m3 over minimum 30 min, max 8 hr period / mg/Nm3
	0.011
	
	BS EN 13211
	29-Apr-15

14:50 - 18:54
	MCERTS
	14

	Sb, As, Pb, Cr, Co, Cu, Mn, Ni, and V and their compounds (total)
	0.5mg/m3 over minimum 30 min, max 8 hr period / mg/Nm3
	0.0051
	
	BS EN 14385
	28-Apr-15

15:10 - 19:14
	MCERTS
	15

	Dioxins / Furans 

(I-TEQ)6
	0.1ng/m3 over minimum 6hr, max 8 hr period / ng/Nm3
	0.011/0.011
	
	BS EN 1948
	28-Apr-15

08:30 - 14:54
	MCERTS
	13

	Dioxins / Furans (WHO – TEQ Humans/ Mammals)6
	No Limit / ng/Nm3
	0.0096/0.0098
	
	BS EN 1948
	28-Apr-15

08:30 - 14:54
	MCERTS
	13

	Dioxins / Furans (WHO – TEQ Fish)6
	No Limit / ng/Nm3
	0.011/0.011
	
	BS EN 1948
	28-Apr-15

08:30 - 14:54
	MCERTS
	13

	Dioxins / Furans (WHO – TEQ Birds)6
	No Limit / ng/Nm3
	0.027/0.027
	
	BS EN 1948
	28-Apr-15

08:30 - 14:54
	MCERTS
	13

	Dioxin – like PCBs (WHO – TEQ Humans/ Mammals)6
	No Limit / ng/Nm3
	0.011/0.011
	
	BS EN 1948
	28-Apr-15

08:30 - 14:54
	MCERTS
	18

	Dioxin – like PCBs (WHO – TEQ Fish)6
	No Limit / ng/Nm3
	0.000061/0.000061
	
	BS EN 1948
	28-Apr-15

08:30 - 14:54
	MCERTS
	18

	Dioxin – like PCBs (WHO – TEQ Birds)6
	No Limit / ng/Nm3
	0.0038/0.0038
	
	BS EN 1948
	28-Apr-15

08:30 - 14:54
	MCERTS
	18

	Poly-cyclic aromatic hydrocarbons Total
	No Limit / mg/Nm3
	0.043
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Anthanthrene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Benzo(a)anthracene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Benzo(b)fluoranthene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Benzo(k)fluoranthene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Benzo(b)napth(2,1-d)thiophene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Benzo(c)phenathrene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Benzo(g,h,i)perylene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Benzo(a)pyrene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Cholanthrene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Chrysene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Cyclopenta(c,d)pyrene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Dibenzo(a,h)anthracene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Dibenzo(a,i)pyrene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Fluoranthene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Indo(1,2,3-cd)pyrene
	No Limit / mg/Nm3
	<0.000064
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Naphthalene
	No Limit / mg/Nm3
	0.042
	
	BS 1SO 11338-1
	29-Apr-15

08:33 - 14:37
	MCERTS
	49

	Zinc and its compounds
	No Limit / mg/Nm3
	0.0031
	
	BS EN 14385
	28-Apr-15

15:10 - 19:14
	MCERTS
	12

	Benzene
	No Limit / mg/Nm3
	1.8/2.3
	
	BS EN 13649
	29-Apr-15

12:00-13:00, 13:10-14:10
	MCERTS
	19

	1,3-butadiene
	No Limit / mg/Nm3
	0.50
	
	BS EN 13649
	29-Apr-15

12:00-12:10, 12:20-12:30
	MCERTS
	16


1. The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reported period, expressed in the same terms as the emission limit value. Where the emission limit is expressed as a range, the result given as the minimum – maximum’ measured values. 

2. Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the agency is used then the appropriate identifier is given. In other cases the principal technique is stated e.g. gas chromatography

3. For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.

4. The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis. 

5. The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. 

6. The result to be reported as a range based on: All congeners less than the detection limit assumed to be zero as a minimum, and all congeners less than the detection limit assumed to be at the detection limit as a maximum. 

7. Due to a contaminated batch of filter papers the Zinc result is un-accredited and the result reported is a worse case result.
Signed 
   








Date   15th July 2015
Victoria Smith, Quality and Environment Manager
(Authorised to sign as representative of Castle Cement Ltd)

