Permit Number: EPR/BL1096IB                





Operator: Castle Cement Limited
Installation: Padeswood Cement Works                                          

Form Number: Air 1

Date: 26/07/18
Six-monthly Reporting of Emissions to Air from Emission Point A8 for the period from
1st January to 30th June 2018 
	Substance / Parameter
	Emission Limit Level
	Result (1)
	Test Method(2)
	Sample Date & Times(3)
	Accreditation/ Certification (4)
	Uncertainty

(5)

	
	
	First 6 Months
	Second 6 Months
	
	
	
	

	Hydrogen Fluoride
	1mg/Nm3 over minimum 1 hour period
	<0.026 mg/Nm3
	
	ISO 15713
	2nd May 2018 08:40 – 10:40
	MCERTS
	40%

	Cadmium & thallium and their compounds (total)
	0.05mg/Nm3 over minimum 30 min, max 8 hr period
	0.0015 mg/Nm3
	
	EN 14385
	14th June 2018 12:10 – 16:14
	MCERTS
	14%

	Mercury and its compounds
	0.05mg/Nm3 over minimum 30 min, max 8 hr period
	0.034 mg/Nm3
	
	EN 13211
	15th June 2018 06:40 – 11:10
	MCERTS
	15%

	Sb, As, Pb, Cr, Co, Cu, Mn, Ni, and V and their compounds (total)
	0.5mg/Nm3 over minimum 30 min, max 8 hr period
	0.0038 mg/Nm3
	
	EN 14385
	14th June 2018 12:10 – 16:14
	MCERTS
	15%

	Dioxins / Furans (I-TEQ)6
	0.1ng/Nm3 over minimum 6hr, max 8 hr period
	0.0073 ng/Nm3
	
	EN 1948
	2nd May 2018 10:55 – 17:10
	MCERTS
	15%

	Dioxins / Furans (WHO – TEQ Humans/ Mammals)6
	No Limit
	0.0070 ng/Nm3
	
	EN 1948
	2nd May 2018 10:55 – 17:10
	MCERTS
	15%

	Dioxins / Furans (WHO – TEQ Fish)6
	No Limit
	0.0074 ng/Nm3
	
	EN 1948
	2nd May 2018 10:55 – 17:10
	MCERTS
	15%

	Dioxins / Furans (WHO – TEQ Birds)6
	No Limit
	0.024 ng/Nm3
	
	EN 1948
	2nd May 2018 10:55 – 17:10
	MCERTS
	15%


1. The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reported period, expressed in the same terms as the emission limit value. Where the emission limit is expressed as a range, the result given as the minimum – maximum’ measured values. 

2. Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the agency is used then the appropriate identifier is given. In other cases the principal technique is stated e.g. gas chromatography

3. For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.

4. The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis. 

5. The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. 

6. The result to be reported as a range based on: All congeners less than the detection limit assumed to be zero as a minimum, and all congeners less than the detection limit assumed to be at the detection limit as a maximum. 

Signed ……………Robert Keough……………….        



Date……26/07/18..      
(Authorised to sign as representative of Castle Cement Limited)
