Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	Permit Number
	EPR/BL1096IB/V011

	Name of operator
	Castle Cement Limited

	Location of Installation
	Padeswood Works, Padeswood, Mold.

	Time and date of the detection 
	02/09/2014  05:55


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	02/09/2014  05:55

	Reference or description of the location of the event 
	Raw mill outlet air slide

	Description of where any release into the environment took place
	Directly below the raw mill outlet air slide and a quantity of dust released into the air. 

	Substances(s) potentially released
	Raw Meal

	Best estimate of the quantity or rate of  release of substances
	100KG

	Measures taken, or intended to be taken, to stop any emission
	Both Raw Mill and kiln brought to an immediate controlled stop upon detection of the release.

	Description of the failure or accident.
	A blockage in the raw mill outlet air slide caused material to back up and push a lid off.


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	A dust release was noted on the camera in the control room, the controller contact the Shift Manager and it was quickly realised that it was coming from the raw mill outlet air slide. Both the raw mill and kiln were crash stopped to stop the flow of materials and allow for investigation of the exact cause.



	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	On investigation a hole was found in the cloth that was preventing it from conveying product effectively. This had led to a build-up of material that lifted the lids allow material to escape.
This cloth was repaired and the rest of the airslide cleaned out and checked and the lids resecured. A 3 monthly PM was added to SAP.


	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	The dust release quickly dispersed and stopped at source immediately after the raw mill was shut down. 

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
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	Name* 
	Victoria Smith

	Post 
	Quality and Environment Manager

	Signature 
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	Date 
	01/10/2015


* authorised to sign on behalf of Castle Cement Limited
