Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	Permit Number
	EPR/BL1096IB/V011

	Name of operator
	Castle Cement Limited

	Location of Installation
	Padeswood Works, Padeswood, Mold.

	Time and date of the detection 
	00.05 – 06/07/15


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	

	Reference or description of the location of the event 
	

	Description of where any release into the environment took place
	

	Substances(s) potentially released
	

	Best estimate of the quantity or rate of  release of substances
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	A5 Mill 3 Filter 

	Parameter(s)
	Particulates

	Limit
	Daily average Limit 30mg/Nm3

	Measured value and uncertainty
	Actual – 35.6 mg/Nm3

	Date and time of monitoring
	05/07/15 00:00 to 06/07/15 00:00

	Measures taken, or intended to be taken, to stop the emission
	Mill down for filter bag change.

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	Mill 3 filter was being run for stock prior to being taken out of service for a planned filter bag change. A number of trips on dust average took the mill out of service in the previous 24hrs. The mill was restarted after midnight to run out the mill and filter as requested for the filter works. It ran for 45 minutes and was then taken off by the 45minute internal high level system. It was then left off for the planned stop. 

This gives an over for the 24hrs but only pertains to 45minutes of run time. 

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	Planned filter changes underway. This are scheduled via emission reviews.

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	Total dust emission below 1kg for time period would have dissipated rapidly.

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	07/07/2013
16/11/2013

11/07/2013
13/04/2014

18/07/2013
02/09/2014

25/07/2013
06/09/2014

19/09/2013
21/01/2015

27/09/2013
06/02/2015

10/10/2013
01/04/2015


	Name*
	Victoria Smith

	Post
	Quality and Environment Manager

	Signature
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	Date
	06/07/2015


* authorised to sign on behalf of Castle Cement Limited
