Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	Permit Number
	EPR/BL1096IB/V012

	Name of operator
	Castle Cement Limited

	Location of Installation
	Padeswood Works, Padeswood, Mold.

	Time and date of the detection 
	03:00 10/9/15


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	01:06 10/9/15

	Reference or description of the location of the event 
	Kiln system over pressurisation.

	Description of where any release into the environment took place
	Kiln outlet seal.

	Substances(s) potentially released
	Dust and fumes.

	Best estimate of the quantity or rate of  release of substances
	Less than 50Kg.

	Measures taken, or intended to be taken, to stop any emission
	Clearing cooler filter hoppers out during the incident.
  

	Description of the failure or accident.
	Running out main bag filter and kiln feed system overwhelmed.


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	The kiln was off for most of the previous day, and kiln feed re-introduced at 00.30 10/09. Feed to the preheater tower was then run for around 40 minutes at 140t/h when the kiln became very unstable.
Investigations traced the route cause to filter dust entering the top of the top of the tower, increasing the feed rate and overwhelming the PHT. After 30mins the Kiln Burner reduced the raw meal feed to 120t/h to the tower to reduce the total material flow and the risk of further overwhelming the system.
This situation occurred because under normal operation we empty the bag filter to the tower, through a screw to the raw meal elevator. This is the only outlet from the filter for the collected dust and can only be used whilst the kiln in operation.  
If the kiln trips this system continues to operate collecting dust but with no outlet. This can lead to a significant backlog of material being introduced from the bag filter hopper at restart of kiln operation.
This return feed is in equilibrium when kiln in stable operation, hence we don’t see this as an ongoing issue.

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	As part of the continuous improvement program we are investigating amending the material flows by installing a blowing line to a silo, this system will be able to run when the kiln is off emptying the filter system of collected dust before feed re-starts. The transfer on material from the silo can then be managed along with the normal return from the filter system.

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	The dust release quickly dispersed with minimal environmental impact.

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	19/09/13

13/04/14

06/02/15

17/07/15

27/09/13

02/09/14

01/04/15

23/08/15

10/10/13

06/09/14

06/07/15

16/11/13

21/01/15

15/07/15




	Name* 
	Victoria Smith

	Post 
	Quality and Environment Manager

	Signature 
	

	Date 
	11/11/15


* authorised to sign on behalf of Castle Cement Limited
