Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	Permit Number
	EPR/BL1096IB/V012

	Name of operator
	Castle Cement Limited

	Location of Installation
	Padeswood Works, Padeswood, Mold.

	Time and date of the detection 
	18/7/15 00:01 hrs


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	

	Reference or description of the location of the event 
	

	Description of where any release into the environment took place
	

	Substances(s) potentially released
	

	Best estimate of the quantity or rate of  release of substances
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	Cement Mill 4 DCE

	Parameter(s)
	Particulates mg/Nm3

	Limit
	30 mg/Nm3

	Measured value and uncertainty
	30.88 mg/Nm3

	Date and time of monitoring
	00.01 17/07/15 – 00.01 18/07/15  (24 hour period)

	Measures taken, or intended to be taken, to stop the emission
	Mill was stopped to investigate high dust readings. Further work is being carried out.

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	Cement Mill 4 DCE stack 
	24hrs

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	The DCE on mill 4 prior to this event was slowly trending up as is normal under constant operation against the daily average but was not showing a significant raise in emissions levels and had not triggered the internal warning level. (See Appendix 1) On the evening of the 16th July after a short mill stop the dust reading rose over a 2hr period to above the emission limit, the flow of air and material in the mill circuit was adjusted to bring this down and this was initially successful. 
Running on into the morning of the 17th the dust results again rose significantly. The internal control sequence took the mill off serval times for reaching the emission limit. 
The mill feed was temporarily stopped while investigations were carried out into the cause and the sluice under the filter was changed as it was passing material back in to the filter. The mill system was then restarted. The emissions were improved for several hours but not sufficiently so to bring the daily average back under the limit for the 17th July. (Appendix 2)
For the following few days the mill system was then managed with products with less impact on the filter being manufactured until the following week when a bag change was carried out to a section of the DCE filter reducing the emissions further.


	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	Continued monitoring of trends through the CEM’s and reporting of mill circuit issues that may lead to poor filter operation. Following visioliting (pigment dust into filter, viewed under UV light) in January, 30 bags were changed, 400 were changed out in April. The rest are due to be changed later in the year.
Trends will continue to be monitored and issues highlighted to allow bags to be changed.


	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	Very small additional dust to atmosphere would have dissipated rapidly.

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	18/07/13

16/11/13

06/02/15

25/07/13

13/04/14

01/04/15

19/09/13

02/09/14

06/07/15

27/09/13

06/09/14

15/07/15

10/10/13

21/01/15



	Name* 
	Victoria Smith

	Post  
	Quality and Environment Manager

	Signature 
	

	Date 
	09/11/15


* authorised to sign on behalf of Castle Cement Limited
Appendix 1 DCE Mill 4 Trend
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Appendix 2 DCE CEMS for 17/07/15
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