Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	Permit Number
	EPR/BL1096IB/V012

	Name of operator
	Hanson Cement Limited

	Location of Installation
	Padeswood Works, Padeswood, Mold.

	Time and date of the detection 
	12:30 07/12/15


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	12:38 07/12/15

	Reference or description of the location of the event 
	Pre Heater Tower,  Level 6

	Description of where any release into the environment took place
	As above, through the cladding, west side of tower, blowing north towards Buckley.

	Substances(s) potentially released
	Fumes and fine particles of Kiln feed.

	Best estimate of the quantity or rate of  release of substances
	Release occurred over 10 minutes but was mostly visible due to fumes. Dust release estimated 50kg

	Measures taken, or intended to be taken, to stop any emission
	Increased suction on the tower until the emission subsided.

	Description of the failure or accident.
	Worn refractory on inlet to cyclone 5 allowed fumes to pass when positive pressure occurred through the PHT following a planned kiln stop. This area had been inspected 24hrs previously and had not shown signs of deterioration. 


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	


	Name* 
	Victoria Smith

	Post 
	Quality and Environment Manager

	Signature 
	

	Date 
	07/12/15


* authorised to sign on behalf of Castle Cement Limited
