
Schedule 5 - Notification 

These pages outline the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the PPC Regulations.

Part A 
	Permit Number
	EPR/BL1096IB/V013

	Name of operator
	Castle Cement Limited

	Location of Installation
	Padeswood Works, Padeswood, Mold.

	Time and date of the detection 
	04/05/2018  23:59HRS


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	

	Reference or description of the location of the event 
	

	Description of where any release into the environment took place
	

	Substances(s) potentially released
	

	Best estimate of the quantity or rate of  release of substances
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	Main stack Kiln 4

	Parameter(s)
	Hcl

	Limit
	10 Mg/Nm3

	Measured value and uncertainty
	13 Mg/Nm3

	Date and time of monitoring
	04/05/2018 to 04/05/2018 -  0000hrs to 23:59hrs

	Measures taken, or intended to be taken, to stop the emission
	We had a raw mill belt failure on BC03,  this was caused by a lump that entered the system and wedged under the mag belt on BC03,  Resulting in the belt slowing and tracking to one side in turn causing small spillage of material to the return side of the belt.  The material built up at the tail end drum causing the belt to lift away from the tail drum, as the belt lifted the belt became snagged on the bottom corner of the steel vertical skirts at the back end of the transfer chute.  This cut the belt approximately 40 meters.  The belt was off for approximately 12hours until repaired.  The kiln was for 4hours also during the same period due to lack of raw material to produce the clinker.  This caused a short run on the kiln systems resulting in the breach of Hcl.

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	


	Name*
	P Durkin

	Post
	Duty Shift Manager

	Signature
	Paul Durkin

	Date
	04/05/2018


* authorised to sign on behalf of Castle Cement Limited
