Schedule 6 Notification

Part A

	Permit Number
	BU0800IZ

	Name of Operator
	3C Waste Limited

	Location of Installation
	Llanddulas Landfill Site

	Time and date of the detection
	14th April 2015 (sampled) – lab report received 1stth May 2015


(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

To be notified within 24 hours of detection

	Date and time of the event
	n/a

	Reference or description of the     

Location of the event
	n/a

	Description of where any release into 

The environment took place
	n/a

	Substance(s) potentially released
	n/a


	Best estimate of the quantity or rate

Of release substances
	n/a

	Measures taken or intended to be taken,

To stop any emission
	n/a

	Description of the failure or accident
	n/a


(b) Notification requirements for the breach of a limit

To be notified within 24 hours unless otherwise specified below

	Emission point reference/ source
	Groundwater borehole – GWBH36

	Parameters(s)
	Potassium & Tributyl Tin

	Limit
	See below


	Measured value and uncertainty


	Sample ID

Determinand

Trigger

Value

GWBH36
Potassium
12mg/l
36mg/l
GWBH36
Tributyl Tin
0.001ug/l
0.00322ug/l


	Date and time of monitoring


	Sampling took place on 14th April 2015 and was reported to FCC by the laboratory on 1st May 2015.


	Measures taken or intended to be taken,

to stop any emission


	Groundwater borehole GWBH36 reported a value above the trigger limit for Potassium previously in January 2015 with a value of 39mg/l whilst the trigger limit for Tributyl Tin has never been exceeded in any groundwater borehole.  There appear to be no other determinands exceeding their trigger limits or showing elevated levels.  For example Ammoniacal Nitrogen is at <0.01mg/l and the Chloride concentration is 78mg/l which is well below the 250mg/l limit. Both Potassium and Chloride concentrations show a reducing trend since January 2015 and historical data shows that there have been occasional spikes of Potassium in borehole GWBH36 previously but levels have returned to background concentrations within a few months.

We have requested that our contract laboratory retest the sample for both substances and we will report the result once received.



Time periods for notification following detection of a breach of a limit 

Parameter  







               Notification period

(c} Notification requirements for the detection of any significant adverse environmental effect

To be notified within 24 hours of detection

	Description of where the effect on 

The environment was detected
	n/a

	Substance(s) detected
	n/a

	Concentrations of substances

Detected
	n/a

	Date of monitoring/sampling 
	n/a


Part B
	Any more accurate information on the matters for notification under Part A.
	To be completed once the retests have been carried out.

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	n/a

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment or harm which has been or may be caused by the emission
	n/a

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	As previously reported via Schedule 6.


	Name:               Peter Taberner

	Post:                Site Manager

	Signature:  [image: image1.png]




	Date:                05/05/15


