Schedule 5 - Notification 

This page outlines the information that the operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.

Part A 
	Permit Number
	CB3432AA

	Name of operator
	3C Waste Ltd

	Location of Installation
	Llanddulas Composting Facility

	Time and date of the detection 
	8th September  2015


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and Time of the event
	N/A

	Reference or description of the location of the event 
	N/A

	Description of where any release into the environment took place
	N/A

	Substances(s) potentially released
	N/A

	Best estimate of the quantity or rate of  release of substances
	N/A

	Measures taken, or intended to be taken, to stop any emission
	N/A

	Description of the failure or accident.
	N/A


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	Sample Point 1 50-75m west of the composting pad on the track that surrounds the quarry surface. Grid ref SH 90164 77150

	Parameter(s)
	Asperigillus Fumigatus

	Limit
	Aspergillus Fumigatus = 500 cfu/m3 (Table S3.2 of Permit)

	Measured value and uncertainty
	SP1 Asperigillus Fumigatus = 28278 cfu/m3

	Date and time of monitoring
	8th September  2015

	Measures taken, or intended to be taken, to stop the emission
	Highly variable wind directions were recorded at the sampling points on the day of the monitoring. The predominant wind direction at SP1, the sensitive receptor (Plas Farm and Plas yn Llysfaen) was from the north, northeast which should have placed SP2 downwind of composting operations. However the mean wind direction at SP2 was from the east. Shredding of green waste and bagging of it was in progress during the monitoring. Total Bacteria was below the permit level at <833 cfu/m3.

Aspergillus Fumigatus is predominantly produced from the composting process, but as this is done in closed ECO pods it is unlikely that this was the source of the breach. There is some potential for Aspergillus Fumigatus to be produced from fresh green waste being shredded.

Shredding and bagging was being done during monitoring and it was noted that the feed material had an unusually large amount of grass cuttings which had started to decompose due to a delay in the waste being collected because of the extended bank holiday weekend. This resulted in material being stored for longer than usual before shredding and might have increased the potential for an increase in Aspergillus Fumigatus. Considering the results and variable wind direction this potential might be open to debate.
The highly variable wind directions resulted in difficult monitoring conditions and debris and particles from the surrounding area circulating around the monitoring point, SP1 might have influenced the results. Such swirling air movement within the quarry might have caused Aspergillus Fumigatus to become trapped in pockets around the quarry walls above the composting pad. Sudden changes of wind direction might have caused concentrations of it to escape off site towards the sensitive receptor monitoring point SP1. 
We plan to undertake the next quarterly monitoring in December


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	N/A

	Substances(s) detected
	N/A

	Concentrations of substances detected
	N/A

	Date of monitoring/sampling
	N/A


Part B to be supplied as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	N/A

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	The effects of wind swirling and types of activity being undertaken at the time of monitoring would suggest that the site might not be the only source of the elevated readings. However the escape of concentrations of Aspergillus Fumigatis trapped in pockets below the rim of the quarry wall and released by sudden changes in wind direction cannot be discounted. The composting process will continue to be operated in accordance with the sites working plan, odour management plan and site specific bioaerosol risk assessment. The positioning of monitoring equipment  will be reviewed to represent more accurately the effects on the sensitive receptor of emissions from the composting operation. Delays between receipt of green waste & shredding of it will be avoided whenever possible with allowances for Bank Holidays being taken into account.

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	N/A

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	12/12/14 and 09/06/15

	Name*
	Peter Taberner

	Post
	Unit Manager

	Signature
	[image: image1.png]






	Date
	28 September 2015


*authorised to sign on behalf of 3C Waste Ltd
