Permit Reference Number: BR7321





Operator: Tata Steel UK Limited

Installation: Tata Steel Colors Shotton Works




Form Number: W1 (Page 1 of 3)

Reporting of Emissions to Water (other than to Sewer) for the period from …01/07/16….to…30/09/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	W1
	Flow
	15,000 m3/day
	Mean
	1079
	Magnetic flow meter
	100%
	UKAS Lab
	3.7%

	
	
	
	Max
	2465
	Magnetic flow meter
	
	UKAS Lab
	3.7%

	
	pH
	5 - 9
	Min
	6.9
	Glass electrode laboratory pH meter
	8am Every morning
	UKAS Lab
	+/- 0.12

	
	
	
	Max
	7.7
	
	
	UKAS Lab
	

	
	Suspended solids
	100 mg/l
	Mean
	6.75
	Gravimetric /Filtering/Balance
	8am Every morning
	UKAS Lab
	+/- 2.1mg/l

	
	
	
	Max
	28
	
	
	UKAS Lab
	

	
	Chemical Oxygen Demand
	200 mg/l
	Mean
	26.38
	Colorimetric - Hach Spectrophotometer
	8am Every morning
	UKAS Lab
	+/- 1.2mg/l

	
	
	
	Max
	67
	
	
	UKAS Lab
	

	
	Iron
	10 mg/l
	Mean
	0.69
	Laboratory ICP
	8am Every morning
	UKAS Lab
	+/- 0.1mg/l

	
	
	
	Max
	1
	
	
	UKAS Lab
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed …… P. Shephard ……………………………………………………….  

Date………17/10/16………………..



(authorised to sign as representative of the Operator)
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Reporting of Emissions to Water (other than to Sewer) for the period from …01/07/16….to…30/09/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	W1
	Chromium
	0.3 mg/l
	Mean
	0.1
	Laboratory ICP
	8am Every morning
	UKAS Lab
	+/- 0.1mg/l

	
	
	
	Max
	0.1
	
	
	UKAS Lab
	

	
	Mercury
	10 (g/l
	
	0.26
	Laboratory ICP
	
	UKAS Lab
	+/- 0.1µg/l

	
	Nickel
	0.6 mg/l
	Mean
	0.1
	Laboratory ICP
	8am Every morning
	UKAS Lab
	+/- 0.1mg/l

	
	
	
	Max
	0.1
	
	
	UKAS Lab
	

	
	Zinc
	0.8 mg/l
	Mean
	0.1
	Laboratory ICP
	8am Every morning
	UKAS Lab
	+/- 0.1mg/l

	
	
	
	Max
	0.1
	
	
	UKAS Lab
	

	
	Ammoniacal Nitrogen (mg/l)
	
	Mean
	2.86
	Colorimetric - Hach Spectrophotometer
	8am Every morning
	UKAS Lab
	+/- 0.1mg/l

	
	
	
	Max
	4
	
	
	UKAS Lab
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ……………………… P. Shephard ……………………………………………………….  

Date………17/10/16……..




(authorised to sign as representative of the Operator)
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Operator: Tata Steel UK Limited
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Reporting of Emissions to Water (other than to Sewer) for the period from …01/07/16….to…30/09/16

	Emission

Point
	Substance /

Parameter
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	Effluent Plant Discharge

A41
	pH
	Min
	7.2
	Glass electrode laboratory pH meter
	8am Every morning
	UKAS Lab
	+/- 0.12

	
	
	Max
	8.4
	
	8am Every morning
	UKAS Lab
	

	
	Iron (mg/l)
	Mean
	0.53
	Laboratory ICP
	8am Every morning
	UKAS Lab
	+/- 0.1mg/l

	
	
	Max
	1.1
	
	8am Every morning
	UKAS Lab
	

	
	Mercury ((g/l)
	
	3.83
	Laboratory ICP
	
	UKAS Lab
	+/- 0.1µg/l

	
	Chromium (mg/l)
	Mean
	0.1
	Laboratory ICP
	8am Every morning
	UKAS Lab
	+/- 0.1mg/l

	
	
	Max
	0.1
	
	8am Every morning
	UKAS Lab
	

	
	Nickel (mg/l)
	Mean
	0.1
	Laboratory ICP
	8am Every morning
	UKAS Lab
	+/- 0.1mg/l

	
	
	Max
	0.1
	
	8am Every morning
	UKAS Lab
	

	
	Zinc (mg/l)
	Mean
	0.11
	Laboratory ICP
	8am Every morning
	UKAS Lab
	+/- 0.1mg/l

	
	
	Max
	0.3
	
	8am Every morning
	UKAS Lab
	


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed …………………… P. Shephard ……………………………………………………….  

Date………17/10/16……..




(authorised to sign as representative of the Operator)

