Permit Reference Number: BR7321





Operator: Corus UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 1 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A1(gas firing conditions) NOT OPERATED
	Oxides of Nitrogen (as NO2)
	300 mg/m3
	
	
	
	
	

	
	Carbon  monoxide (mg/m3)
	
	
	
	
	
	

	A1(oil firing conditions)

NOT OPERATED


	Oxides of Nitrogen (as NO2)
	450 mg/m3
	
	
	
	
	

	
	Particulates
	50 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	
	Sulphur dioxide (Kg)
	
	
	
	
	
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Corus UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 2 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A2(gas firing conditions) NOT OPERATED
	Oxides of Nitrogen (as NO2)
	300 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	A2(oil firing conditions) NOT OPERATED
	Oxides of Nitrogen (as NO2)
	450 mg/m3
	
	
	
	
	

	
	Particulates
	50 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	
	Sulphur dioxide (Kg)
	
	
	
	
	
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Corus UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 3 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A3(gas firing conditions) NOT OPERATED 
	Oxides of Nitrogen (as NO2)
	300 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	A3(oil firing conditions) NOT OPERATED
	Oxides of Nitrogen (as NO2)
	450 mg/m3
	
	
	
	
	

	
	Particulates
	50 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	
	Sulphur dioxide (Kg)
	
	
	
	
	
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Corus UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 4 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A4(gas firing conditions)

NOT OPERATED
	Oxides of Nitrogen (as NO2)
	300 mg/m3
	
	
	
	
	

	
	Particulates 
	5 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	A4(oil firing conditions) NOT OPERATED
	Oxides of Nitrogen (as NO2)
	450 mg/m3
	
	
	
	
	

	
	Particulates
	50 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	
	Sulphur dioxide (Kg)
	
	
	
	
	
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Corus UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 5 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A5(gas firing conditions) 
	Oxides of Nitrogen (as NO2)
	300 mg/m3
	136.65 mg/Nm³
	Electrochemical cell
	16/11/16 10:04 Hrs
	None
	+10.4mg/Nm³

	
	Carbon monoxide (mg/m3)
	
	13.32 mg/Nm³
	Electrochemical cell
	16/11/16 10:04 Hrs
	None
	+2.9mg/Nm³

	A5(oil firing conditions) NOT OPERATED
	Oxides of Nitrogen (as NO2)
	450 mg/m3
	
	
	
	
	

	
	Particulates
	50 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	
	Sulphur dioxide (Kg)
	
	
	
	
	
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Corus UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 6 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A6(gas firing conditions) 
	Oxides of Nitrogen (as NO2)
	300 mg/m3
	147.54 mg/Nm³
	Electrochemical cell
	11/11/16 09:52 Hrs
	None
	+10.7mg/Nm³

	
	Carbon monoxide (mg/m3)
	
	10.62

mg/Nm³
	Electrochemical cell
	11/11/16 09:52 Hrs
	None
	+2.9mg/Nm³

	A6(oil firing conditions) NOT OPERATED
	Oxides of Nitrogen (as NO2)
	450 mg/m3
	
	
	
	
	

	
	Particulates
	50 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	
	Sulphur dioxide (Kg)
	
	
	
	
	
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Corus UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 7 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A7(gas firing conditions)


	Oxides of Nitrogen (as NO2)
	300 mg/m3
	147.05 mg/Nm³
	Electrochemical cell
	10/11/2016 14:59 Hrs
	None
	+10.7mg/Nm³

	
	Carbon monoxide (mg/m3)
	
	5.28 mg/Nm³
	Electrochemical cell
	10/11/2016 14:59 Hrs
	None
	+2.9mg/Nm³

	A7(oil firing conditions) NOT OPERATED 


	Oxides of Nitrogen (as NO2)
	450 mg/m3
	
	
	
	
	

	
	Particulates
	50 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	
	Sulphur dioxide (Kg)
	
	
	
	
	
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.}

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Corus UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 8 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A8(gas firing conditions) 
	Oxides of Nitrogen (as NO2)
	300 mg/m3
	217.47 mg/Nm³
	Electrochemical cell
	14/11/16 13:51 Hrs
	None
	+13.1g/Nm³

	
	Carbon monoxide (mg/m3)
	
	<1 mg/Nm³
	Electrochemical cell
	14/11/16 13:51 Hrs
	None
	+2.9mg/Nm³

	A8(oil firing conditions) NOT OPERATED
	Oxides of Nitrogen (as NO2)
	450 mg/m3
	
	
	
	
	

	
	Particulates
	50 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	
	Sulphur dioxide (Kg)
	
	
	
	
	
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Corus UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 9 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A9(gas firing conditions) NOT OPERATED
	Oxides of Nitrogen (as NO2)
	300 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	A9(oil firing conditions) NOT OPERATED
	Oxides of Nitrogen (as NO2)
	450 mg/m3
	
	
	
	
	

	
	Particulates
	50 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	
	Sulphur dioxide (Kg)
	
	
	
	
	
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Corus UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 10 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A10(gas firing conditions)

NOT OPERATED
	Oxides of Nitrogen (as NO2)
	300 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	A10(oil firing conditions) NOT OPERATED
	Oxides of Nitrogen (as NO2)
	450 mg/m3
	
	
	
	
	

	
	Particulates
	50 mg/m3
	
	
	
	
	

	
	Carbon monoxide (mg/m3)
	
	
	
	
	
	

	
	Sulphur dioxide (Kg)
	
	
	
	
	
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.}

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Corus UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 11 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A11

NO LONGER IN USE
	Oxides of Nitrogen (as NO2)
	
	
	
	
	
	

	
	Carbon monoxide
	
	
	
	
	
	

	
	Volatile Organic Carbon (as C)
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	A12

1 colorcoat old RTO
	Oxides of Nitrogen (as NO2)
	100 mg/m3
	16.85

mg/Nm³
	Electrochemical cell
	23/09/16 09:38Hrs
	None
	+8.4mg/Nm³

	
	Carbon monoxide
	100 mg/m3
	33.02 mg/Nm³
	Electrochemical cell
	23/09/16 09:38Hrs
	None
	+3.2mg/Nm³

	
	Volatile Organic Carbon (as C)
	50 mg/m3
	2.43

mgC/m³
	BS EN 13526
	23/09/16 09:43Hrs
	None
	+2.7mgC/m³

	
	
	
	
	
	
	
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Corus UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 12 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A12A

1 colorcoat new RTO
	Oxides of Nitrogen (as NO2)
	100 mg/m3
	9.2 mg/Nm³
	Electrochemical cell
	22/09/16 10:00Hrs
	None
	+8.3mg/Nm³

	
	Carbon monoxide


	100 mg/m3
	9.07

mg/Nm³
	Electrochemical cell
	22/09/16 10:00Hrs
	None
	+2.9mg/Nm³

	
	Volatile Organic Carbon as C
	50 mg/m3
	43.6

mgC/m³
	BS EN 13526
	22/09/16 10:30Hrs
	None
	+2.7mgC/m³

	A21

2 colorcoat new RTO
	Oxides of Nitrogen (as NO2)
	100 mg/m3
	26.33 mg/Nm³
	Electrochemical cell
	06/10/16 12:00Hrs
	None
	+8.8mg/Nm³

	
	Carbon monoxide


	100 mg/m3
	11.8 mg/Nm³
	Electrochemical cell
	06/10/16 12:00Hrs
	None
	+2.8mg/Nm³

	
	Volatile Organic Carbon as C
	20 mg/m3
	18.44

mgC/m³
	BS EN 13526
	06/10/16 12:47Hrs
	None
	+2.8mgC/m³

	
	Isocyanates as NCO
	Test no longer required
	
	
	
	
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Corus UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 13 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A31

5 galv DF furnace.NOT OPERATED
	Oxides of Nitrogen (as NO2) (mg/m3)
	
	
	
	
	
	

	
	Carbon monoxide 

(mg/m3)
	
	
	
	
	
	

	A32 5 galv DF furnace with boiler.NOT OPERATED 
	Oxides of Nitrogen (as NO2) (mg/m3)
	
	
	
	
	
	

	
	Carbon monoxide 

(mg/m3)
	
	
	
	
	
	


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Corus UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 14 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A33

5 Galv RT furnace.

NOT OPERATED
	Oxides of Nitrogen (as NO2) (mg/m3)
	
	
	Electrochemical cell
	
	None
	

	
	Carbon monoxide 

(mg/m3)
	
	
	Electrochemical cell
	
	None
	

	A35

6 galv furnace
	Oxides of Nitrogen (as NO2) (mg/m3)
	
	88.23mg/Nm³
	Electrochemical cell
	17/11/16 09:40Hrs
	None
	+9.3mg/m³

	
	Carbon monoxide 

(mg/m3)
	
	214.18mg/Nm³
	Electrochemical cell
	17/11/16 09:40Hrs
	None
	+10.3mg/m³


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Tatasteel UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 15 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A13

1 colorcoat Coater house extraction
	Volatile Organic Carbon (as C)
	None
	34.78

mgC/m³
	BS EN 13526
	23/11/16 13:06Hrs
	None
	+2.7mgC/m³

	A14

1 colorcoat washtank extraction
	Volatile Organic Carbon (as C)
	None
	47.99

mgC/m³
	BS EN 13526
	23/11/16 10:51Hrs
	None
	+2.7mgC/m³


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

Permit Reference Number: BR7321





Operator: Tatasteel UK Ltd

Installation: Corus Colors Shotton Works




Form Number: A1 (Page 16 of 16)

Reporting of Emissions to Air for the period from 01/01/16 to 31/12/16

	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	A15

1 colorcoat paint kitchen extraction
	Volatile Organic Carbon as C
	None
	13.5

mgC/m³
	BS EN 13526
	21/11/16 12:17Hrs
	None
	+2.8mgC/m³


[1] 
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] 
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] 
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] 
The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] 
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 

Signed ………………………… P. Shephard ………………………………………….  

Date………23.1.17………………..    



(authorised to sign as representative of the Operator)

