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	Matthew Kelk

	Natural Resource Wales

	Chester Road

	Buckley

	Flintshire

	CH7 3AJ
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Attn: Matthew Kelk

Re: Shotton Works Permit BR7321 Condition 4.14 Fugitive emission

Dear Matthew,

In response to Reporting Condition 4.1.4, we have reviewed fugitive emissions from the installation and can report on these releases and measures taken to reduce them with due regard to the application of BAT.

Fugitive releases are based on total volumes of solvents used in the processes and their corresponding Volatile Organic Compound (VOCs) emissions: -

No.2 Colorcoat 

Total Solvent consumed = 




1284.636 tonnes

Average Fugitive VOC emissions for the year = 


0.64%

Calculated Fugitive VOC emissions for the year = 

8.165 tonnes
No.1 Colorcoat

Total Solvent consumed = 




1267.243 tonnes

Average Fugitive VOC emissions for the year = 


3.94%

Calculated Fugitive VOC emissions for the year = 

49.878 tonnes

Total Fugitive VOC emissions for 2014 = 


58.043 tonnes
Based on 2014 Colorcoat production of 263,063 tonnes = 
0.221 kg/tonne total VOCs
Yours sincerely

Peter Shephard

Senior Energy & Environment Officer
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