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	Potential source of land Pollution.
	Above or below ground.
	Monitoring
	Frequency
	Responsibility

	Waste oil storage tank. (Top filled).
(Chemical Store)
	Above ground.

	Visual inspection and recording of the integrity of the tank. 
(As per the weekly checklist)
	Weekly 
	Safety officer
(To be completed by the Security Staff) 

	Waste oil emulsion tank.
(Machine Shop)
	Above ground.


	Measurement and recording of the fill level from the external site glass.  
(As per the weekly checklist)
	Weekly
	Safety officer

(To be completed by the Security Staff)

	Holography waste tanks.
(West Side)
	Above ground.


	Measurement and recording of the fill level from the external site glass. 
(As per the weekly checklist)
	Weekly
	Safety officer

(To be completed by the Security Staff)

	Process effluent settling weir tanks. 
	Below ground.
	Measurement and recording of the fill level from the top of the tank.
	Quarterly 
	Works Engineering Manager.

	Drains to the point of entry to the public sewer. 
	Below ground.
	Closed circuit television survey. 
	Annual 
	Works Engineering  Manager

	Drains, roadways and hard standings used for chemical passage, usage or storage. 
	Above ground.
	Visual inspection and recording of the integrity. (MEPI) Monthly Environmental Premises Inspection.

	Monthly 
	Site Services Manager &

Environmental Engineer
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