Schedule 6 - Notification 

Part A 
	Permit Number
	GP3030BE

	Name of Operator
	Tata Steel UK Limited

	Location of Installation
	Shotton Works Landfill 

	
	

	Time and date of the detection 
	17/10/2016


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and Time of the event
	N/A

	Reference or description of the location of the event 
	N/A

	Description of where any release into the environment took place
	N/A

	Substances(s) potentially released
	N/A

	Best estimate of the quantity or rate of release of substances
	N/A

	Measures taken, or intended to be taken, to stop any emission
	N/A

	Description of the failure or accident.
	N/A


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	BH10 – Zinc 3-Point moving average (Q3 2016)

BH9 – CO2 level (July 2016)
BH2 – CO2 level (August & September 2016)

BH10 – CO2 level (August & September 2016)

	Parameter(s)
	3-Point moving average limit for Zinc

CO2 limit (spot sample) 

	Limit
	Zinc limit of 0.04ppm @ BH10

CO2 limit of 1.5% @BH2, 10

	Measured value and uncertainty
	Q3 BH10 3-Point moving average
0.06ppm

BH9 (July) – 1.7% CO2

BH2 (August) – 1.9% CO2

BH10 (August) – 3% CO2

BH2 (September) – 1.8% CO2

BH10 (September) – 1.7% CO2

	Date and time of monitoring
	04/07/16 (CO2)

03/08/16 (CO2)

08/09/16 (CO2)

17/08/16 (Zinc)

	Measures taken, or intended to be taken, to stop the emission
	As noted previously, BH10 (zinc) may be showing some of the traits of the land reclamation material used in construction/reclamation. It should also be noted that the actual measured value on May was 0.03ppm (i.e. below the limit – however as the permit states a 3 point moving average, the average value constituted a breach).

CO2 levels are generally stable, and it should be noted that althought BH2 and BH10 are elevated, apart from one result the Leachate well levels (L1-4 do not show elevated CO2, strongly suggested (an) off-site source(s) for the CO2 levels 


	Time periods for notification following detection of a breach of a limit 

	Parameter
	Notification period 24 h

	c) Notification requirements for the detection of any significant adverse environmental effect 

To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	N/A

	Substances(s) detected
	N/A

	Concentrations of substances detected
	N/A

	Date of monitoring/sampling
	N/A


Part B to be supplied as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	No further information 

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	Continue to monitor all boreholes; check monthly returns when received to determine whether this reoccurs so that local environmental factors or changes can be monitored and evaluated. 
It should be noted that the Permit for the landfill is going to be varied to take into account the HRA produced for the landfill, which will include adjusting the emissions limit values

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	None – due to the age of the landfill and the material used for land reclamation, ascertaining the source of the breach of limits would be virtually impossible.

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	Zinc limit for BH10 (3 month average) was breached in Q1, Q2, Q3 & Q4 2015, and Q1 & Q2 2016. 
CO2 limits in boreholes were breached in Q1, Q2, Q3 & Q4 2015, and Q1 2016. 


	Name*
	Peter Shephard

	Post
	Senior Energy & Environment Officer

	Signature
	

	Date
	17/10/2016


* authorised to sign on behalf of Tata Steel UK Limited

