Permit Number: 
EPR/PP3834CB





Operator: 
Morgan Technical Ceramics Limited 

Facility:

Ruabon Electroceramics




Form Number: Air 1 
Date : 7th January ’15.
Reporting of Emissions to Air for the period from January 2014 to December 2014.
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	B6
	Lead
	0.2 mg/m3
	0.4123 mg/m3
	BS EN 14385: 2004
	01/10/2014
12:20 - 13:20
	UKAS MCERTS
	± 0.0451

	B6
	Particulates
	3 mg/m3
	1.4 mg/m3
	BS EN 13284:2002
	01/10/2014
13:38 - 15:38
	UKAS MCERTS
	± 0.2

	B7
	Lead
	0.2 mg/m3
	0.0206 mg/m3
	BS EN 14385: 2004
	01/10/2014

10:31 - 11:34
	UKAS MCERTS
	± 0.0022

	B7
	Particulates
	2 mg/m3
	0.2 mg/m3
	BS EN 13284:2002
	02/10/2014
09:22 - 12:04
	UKAS MCERTS
	± 0.02

	B24
	Lead
	0.2 mg/m3
	0.11mg/m3
	BS EN 14385: 2004
	04/12/2014
11:40 – 12:40
	UKAS MCERTS
	± 0.0462

	B24
	Particulates
	2 mg/m3
	14.6 mg/m3
	BS EN 13284:2002
	04/12/2014
12:57 – 14:57
	UKAS MCERTS
	± 1.6


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. 

Signed:  T J Lunt (electronic submission)








Date: 7th January ’15. 



(authorised to sign as representative of the Operator)

Permit Number: 
EPR/PP3834CB





Operator: 
Morgan Technical Ceramics Limited 

Facility:

Ruabon Electroceramics



Form Number: Sewer 1 
 
Date:  7th January ’15.
Reporting of Emissions to Sewer for the period from July 2014 to December 2014.
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	S1
	Lead
	0.5 mg/l
	0.8 mg/l
	UKAS approved method
	10/11/14 11.05am
	UKAS Welsh water
	TBA

	S1
	Zinc
	2 mg/l
	0.1 mg/l
	UKAS approved method
	10/11/14 11.05am
	UKAS Welsh water
	TBA


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.  Welsh Water queried on this figure 10th December ’14, and 6th January ’15 for definitive information, but no positive response received.
Signed:  T J Lunt (electronic submission).







  
Date:   
7th January ’15.

(authorised to sign as representative of the Operator)

Permit Number: 
EPR/PP3834CB





Operator: 
Morgan Technical Ceramics Limited 

Facility:

Ruabon Electroceramics



Form Number: Sewer 1 

Date:  7th January ’15.
Reporting of Emissions to Sewer for the period from January 2014 to June 2014.
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Accreditation/Certification [4]
	Uncertainty

[5]

	S1
	Lead
	0.5 mg/l
	0.5 mg/l
	UKAS approved method
	05/06/14 11.10 am
	UKAS Welsh water
	TBA

	S1
	Zinc
	2 mg/l
	0.1 mg/l
	UKAS approved method
	05/06/13 11.10 am
	UKAS Welsh water
	TBA


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. 

Signed:  T J Lunt (electronic submission).


 




Date:   
7th January ’15.

(authorised to sign as representative of the Operator)

Permit Number: 
EPR/PP3834CB





Operator: 
Morgan Technical Ceramics Limited 

Facility:

Ruabon Electroceramics



Form Number: Waste 1 

Date:  7th January ’15.
Reporting of Waste Disposal and Recovery for the year 2014.
	Waste

Description
	Disposal
	Recovery
	
	Trends in Waste Disposal and Recovery

	
	Route
	Tonnes
	Tonnes
	
	Year
	Parameter

	
	
	
	
	
	
	Hazardous

waste (t) / PVC compound (t)
	Non hazardous

waste (t) / PVC compound (t)
	Total waste (t) /  PVC compound (t)

	1) Hazardous Wastes
	
	
	
	
	2009
	1.07
	1.35
	2.42

	Named haz. Waste
	
	
	
	
	2010
	1.56
	1.60
	3.16

	Other hazardous wastes
	
	
	
	
	2011
	1.22
	1.696
	2.91

	Total hazardous waste
	
	214.08
	8.68
	
	2012
	3.73
	1.397
	5.14

	
	
	
	
	
	2013
	4.03
	1.397
	5.39

	2) Non-Hazardous Wastes
	
	
	
	
	2014
	1.33
	0.26
	1.59

	Named non-haz. Waste
	
	
	
	
	2015
	
	
	

	Other non-hazardous wastes
	
	
	
	
	
	
	
	

	Total non-hazardous waste
	
	42.4
	29.91
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	TOTAL WASTE
	-
	256.48
	38.59
	
	
	
	
	


	Operator’s comments :

Waste disposed of was down on previous year, but in line with 2009, 2010 & 2011.



Signed:  T J Lunt (electronic submission).


 




Date:   
7th January ’15.

(authorised to sign as representative of the Operator)

Permit Number: 
EPR/PP3834CB





Operator: 
Morgan Technical Ceramics Limited 

Facility:

Ruabon Electroceramics




Form Number: Water Use 1 
Date: 7th January ’15.
Reporting of Water Usage for the year 2014
	Water Source
	Usage

(m3)
	Specific Usage

(m3/t)
	
	Trends in Water Usage

	
	
	
	
	Year
	Parameter

	
	
	
	
	
	
	Total

Water usage
	Water per tonne electroceramic product

	Mains water
	7,734
	48.01
	
	
	
	
	

	
	
	
	
	2009
	
	8233m3
	46.34m3/T

	
	
	
	
	2010
	
	7997m3
	50.81m3/T

	
	
	
	
	2011
	
	7989m3
	41.39m3/T

	
	
	
	
	2012
	
	5146m3
	35.61m3/T

	
	
	
	
	2013
	
	13916m3
	159.3m3/T

	
	
	
	
	2014
	
	7,734 m3
	48.01 m3/tonne

	TOTAL WATER USAGE
	
	
	
	2015
	
	
	


	Operator’s comments :

Water usage was down on previous year but in line with 2009, 2010, 2011 & 2012.




Signed:  T J Lunt (electronic submission).


 




Date:   
7th January ’15.
(authorised to sign as representative of the Operator)

Permit Number: 
EPR/PP3834CB





Operator: 
Morgan Technical Ceramics Limited 

Facility:

Ruabon Electroceramics




Form Number: Energy 1 

Date: 7th January ’15.
Reporting of Energy Usage for the year 2014
	Energy Source
	Energy Usage
	CO2
Produced

(tonnes)
	
	Trends in Energy Usage

	
	Quantity
	Primary Energy

(MWh)
	
	
	Year
	Parameter

	
	
	
	
	
	
	Primary Energy usage
	CO2

 produced
	CO2 per tonne Electroceramic product

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	2009
	6743
	6550
	36.87

	Electricity *
	4,890 MWh
	1,2714 MWh
	5,779
	
	2010
	18075
	7117
	45.21

	Gas 
	1,858 MWh
	1,858 MWh
	343
	
	2011
	18060
	7125
	37.29

	
	
	
	
	
	2012
	16733
	6604
	45.70

	
	
	
	
	
	2013
	15732
	6327
	72.44

	
	
	
	
	
	2014
	14,572
	6,122
	38.00

	TOTAL
	6,748 MWh
	14,572 MWh
	6,122
	
	2015
	
	
	

	
	
	
	
	
	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.6
	Operator’s comments :

Electricity conversion factor of 0.45453 kgs CO2/kWh utilised.  Source – 2012 Guidelines to Defra/DECC’s GHG Conversion Factors for Company Reporting.
Gas conversion factor of 0.18483 kgs CO2/kWh utilised.  Source – 2012 Guidelines to Defra/DECC’s GHG Conversion Factors for Company Reporting.

Energy usage down by 8% on 2013 because of product mix.



Signed:  T J Lunt (electronic submission).


 




Date:   
7th January ’15.

(authorised to sign as representative of the Operator)

Permit Number: 
EPR/PP3834CB





Operator: 
Morgan Technical Ceramics Limited 

Facility:

Ruabon Electroceramics




Form Number: Performance 1 
Date: 7th January ’15.
Environmental Performance Indicators 
	Parameter
	Annual Average
	Units
	
	Trends in Environmental Performance

	
	
	
	
	Year
	Parameter

	Hazardous waste disposal
	214.08
	T/yr
	
	
	Hazardous waste disposal (t) / Electroceramic product (t)
	Non hazardous waste disposal (t) / Electroceramic product (t)

	Non hazardous waste disposal
	42.4
	T/yr
	
	
	
	

	
	
	
	
	2009
	1.07
	1.35

	
	
	
	
	2010
	1.56
	1.60

	
	
	
	
	2011
	1.22
	1.696

	
	
	
	
	2012
	3.73
	1.397

	
	
	
	
	2013
	4.03
	1.397

	
	
	
	
	2014
	1.33
	0.26

	
	
	
	
	2015
	
	


	Operator’s comments :




Signed:  T J Lunt (electronic submission).


 




Date:   
7th January ’15.

(authorised to sign as representative of the Operator)

EPR/PP3834CB  Reporting Forms  05/07/2012

EPR/PP3834CB  Reporting Forms  05/07/2012
EPR/PP3834CB  Reporting Forms  05/07/2012

