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	IN-RAMS-GI-014-A-Cable Percussion (Over Water)
	


	Contract Name
	Tawe Riverside West SUP
	Contract Number
	TBC
	Date
	20/09/22



	General Overview
	SOCOTEC UK has been appointed by the City and County of Swansea Council to attend a number of drilling sites located in The River Tawe along its western bank situated between the White Rock Bridge (Hafod Copper Works) and The Council Buildings. 
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SOCOTEC



 

Works cannot proceed until the necessary approved documents are in place, they could include NRW fisheries licence / agreement, NRW FRAP (Flood Risk Activity Permit) or marine licences. 

Necessary documents to be confirmed by CCSC. 


	Overview
	A set down point for the establishment, construction and loading out of the floating plant (e.g. barge / pontoon is yet to be agreed). A crane may be required to facilitate the establishment.

The project is expected to comprise four to five number Cable percussive boreholes over water to depths of up to 20mBgl. 

The Pontoon will be built and maintained by a floatation company (Sea Lift, Pontoon Works Ltd, TPA, Red Severn or similar tbc). The business employed to deliver the Pontoon or Barge will be responsible for providing a safe over water working environment, access and safety boat as deemed necessary. The company will provide their own Rams and Method statements

Borehole coordinates are to be provided by Client / Engineer. Boreholes will be set out using a GPS on the Pontoon. 

Contact with buried services and UXO are deemed a significant safety hazards. It is expected that the employer will remain responsible for provision of service plans and UXO desk study providing a permit to dig prior to breaking ground.

Cable avoidance tool (CAT) and generator (“genny”) cannot be used to clear the location therefore all responsibility for service avoidance rests with the client. To limit risk full up to date service plans must be provided by CCSC, Socotec will agree safe stand off to avoid suspected service runs. 

The employer will provide a UXO safety assessment detailing the necessary measures to avoid buried ordnance.

It is expected that the river bed will be classified moderate to high risk and will require clearance prior to any penetration works into the river bed (barge foot or borehole). It is envisaged that the clearance will be undertaken with an on board hand held magnetometer and operator undertaking testing inside stainless steel casings. Method To be confirmed  

Weather constraints remain a safety and financial hazard, no personnel will travel out to the Pontoon if the Pontoon Works personnel report working conditions unsafe. 

Setting up and maintaining floating plant over the duration of the drilling presents a high safety, environmental and commercial risk due to the uncertainty of river bed level and fluctuating water levels at each location. The employer must provide sea levels tables affecting the BH locations relative to a local datum and the offset between local datum and OSD.
The SOCOTEC UK Engineer is to contact the client to confirm the ground conditions when the provisional depth has been achieved to get confirmation that the borehole excavation can be terminated and backfilled with bentonite grout.



	Who or what could be affected?
	Directly – SOCOTEC UK Supervisor, Lead Driller and Assistant/Trainee Driller. 

Indirectly – Visiting personnel from SOCOTEC UK, Client, and Designer etc. 

Environment – Potential spills of fuel / hydraulic oil; potential damage caused by access / egress; leaks from old fuel tanks; Release of excess arising to the river. 

Access – establishment, loading and construction location to be confirmed.


	Key Personnel:


	Office

SOCOTEC UK Project Manager: TBC
SOCOTEC UK Operations Manager: TBC
SOCOTEC UK H&S Manager: TBC
Field crew

SOCOTEC UK Site Agent: TBC

SOCOTEC UK Engineer: TBC

Drilling Crew: TBC

Client Contacts

Client Site Manager: TBC

Client Geo-environmental Engineer: TBC

Supervisor: TBC

	Location:
	Compound expected in the Hafod Copper Works Car park TBC

	Nearest Hospital:
	Singleton Hospital, Sketty Lane, Sketty SA2 8QA TBC

	Frequency and Duration:
	Site hours are 8:00am to 18:00pm TBC


	Personnel 
	Training / Competency Required

	· SOCOTEC Site Agent

· SOCOTEC Fieldwork Supervisor

· Lead Driller
· Assistant Driller
· Other contractors
· UXO Technician
· Pontoon Works Personnel
	All site staff hold CSCS cards appropriate to their role
Site specific safety induction from SOCOTEC

Daily hazard briefing from SOCOTEC

SOCOTEC drill rig induction from Lead Driller.
Lead Driller holds, or is working towards, a Level 2 Diploma in Land Drilling – Lead Driller (Cable Percussion Drilling).  

Assistant Driller holds, or is working towards, a Level 2 Diploma in Land Drilling - Drilling Support Operative. 
Pontoon Works Personnel to hold all relevant training and safety certs to work on water 
For internal drilling crews only 

Practical skills taught in-house by SOCOTEC and operative declared competent by senior management. All staff issued with SOCOTEC Verification of Competence (VOC)


	Plant, Equipment and Materials


	Plant & Work Equipment
· Cable percussion rig – inspected every 12 months under PUWER
· Casing stillages
· Drilling ancillaries e.g. stubbers, chisels, sinker bars 

· CAT and Genny

· Lifting accessories – inspected every 6 months under LOLER
· Drip trays, plant nappy and spill kit 
· Standard Penetration Testing Equipment

· First Aid Kit
· Fire extinguisher 
· Hand tools 
· Trash pump
	Hazardous Materials

· Cement

· Bentonite
· Diesel fuel 

· Lubricants (greases etc.)

· Potential Contaminated ground

See COSHH Assessments
	Personal Protective Equipment 

(Compulsory)
· Safety footwear (lace up boots with Toe tech & midsole).

· Safety Wellington or Waders as required
· Hi-vis vest or jacket (yellow / orange). 
· Hi-vis trousers. 
· Hard hat (If conditions require). 

· Safety glasses (EN166F). 

· Gloves (general handling plus nitrile, Cut 5 if using retractable bladed knives).

· Ear defenders (SNR >25) (If conditions require).
· Wet weather clothing where necessary
· Life jackets. 


	
	Cable Percussion Drilling - Sequence of Tasks 
	Responsibility

	1. 
	General Comments

· COVID 19 currently presents a threat to human health, therefore during all works, the advice given by the government on social distancing and travel must be adhered to. Specific details on working on site with COVID 19 are given in the risk assessment for infection control – COVID 19 (SOCOTEC) and the COVID 19 RAMS.

· Establish rig

· Set up rig on floatation device

· Locate floatation at BH location

· Check bed levels can accommodate float draft at lowest predicted water level during the excavation period

· Relocate floatation or anchor floatation with spud leg and anchor stays tbc

· Contain arisings

· Install conductor casings

· Excavate borehole 

· Ground Investigation works are to be carried out in daylight hours between 08:00 – 18:00.
· Drip trays and plant nappies are to be placed under each item of plant used on site. Any plant found leaking will be isolated and repaired with leaks contained. Plant should not be moved to minimise spreading leaks.

· IBC’s will be provided by Socotec to transport water for the drilling works. No water shall be extracted from water courses without the necessary licence.
· All staff must have the following as a minimum to work on site – CSCS Card, SOCOTEC Induction
	SOCOTEC UK

	2. 
	Prior to work commencing all personnel will receive the site specific induction. A signed record of this will be kept in a register on site. The induction will include:

· A full briefing of relevant RAMS for the task. 

· A mandatory daily activity briefing / daily dynamic risk assessment to be held each morning. 

· Access and egress requirements to main compound and to site entrances.

· Hazard reporting.

· Specific PPE requirements.

· Potential slips, trips and falls.

· Potential interface with 3rd parties including the public & other contractors.

· Site security arrangements.

· Plant movements.

· Any lifting activities required.

· Welfare provision.

If the person is only visiting (not carrying out work) then a visitor’s induction can be carried out.

Check personnel’s training certificates and inspect / review plant / equipment calibration / maintenance records on a weekly basis. This information should be recorded by the Site Agent.
	SOCOTEC Site Agent or nominated deputy

	3. 
	The installation of drilling platform will be in accordance to RAMS provided to SOCOTEC UK Ltd. via the floatation company following their method statement and rams. Any lifting of the pontoon drilling platforms will be completed in accordance with an approved Lift Plan provided by an accredited company. Any necessary stability calculations will be provided by the responsible party and reviewed by SOCOTEC UK Ltd. 
	SOCOTEC UK, Pontoon Works, British Land

	4. 
	Access and egress of personnel to the drilling platform will be controlled by floatation company using appropriate methods based on the distance of the floating platform from shore.
Equipment & spoil will be brought/ removed from the drilling platform to a secure / stable location on the shore on a regular basis to avoid instability of the floatation platform. 
	SOCOTEC Fieldwork Supervisor, Pontoon Works

	5. 
	All the locations will be set out by GPS, the floatation company personnel conducting the movement of the drilling platform. 

	Client Representative, SOCOTEC Fieldwork Supervisor, Pontoon Works

	6. 
	Client to agree service locations and safe stand-off and to issue a ‘Permit to Dig’ to SOCOTEC UK. 
	SOCOTEC Fieldwork Supervisor/ Client

	7. 
	Any crane necessary for construction of the floatation plant will be provided by a bona fide operator and a full lift plan provided. The lift will be supervised by lift operator who will be supplying the, crane operator, slinger and lift supervisor. 


	Ainscough Crane Hire Ltd Lift Supervisor/

SOCOTEC Fieldwork Supervisor/ Lead Driller

	8. 
	Once rig and its corresponding equipment has been unloaded onto the floating platform all equipment stored with the rig will be unloaded on the floating platform. 
	Lead driller

	9. 
	Erect rig using the setup winch
	Lead driller

	10. 
	Level up rig with timbers and fit all retaining pins.
	Lead driller

	11. 
	Secure rig via ratchet straps on lash down points located on the drilling platform.
	Lead driller
Pontoon Works

	12. 
	Place spill protection (plant nappy’s) under all plant within the work area and ensure a tested fire extinguisher and fully stocked spill kit is available within the work area.
	Lead Driller

	13. 
	Create bund around drilling area / rig by laying down visqueen & timbers, to reduce the risk of and spillage of spoil. 
	Lead driller

	14. 
	Upon establishing the pontoon at the borehole install casing through the moonpool placed over the portal of the drilling platform until it is has reached the river bed. 
	Lead driller

	15. 
	Undertake Uxo test inside case if necessary
	

	16. 
	Insert boring tool inside casing. Attach to casing head with surging pin.
	Lead driller

	17. 
	Activate winch and lift tool and casing combination and enter it into the ground vertically.
	Lead driller

	18. 
	Remove surging pin and release winch brake to drop tool to base of the borehole.
	Lead driller

	19. 
	Activate the winch so tools penetrate the ground.
	Lead driller

	20. 
	Remove tool from borehole and clean arisings.
	Lead driller

	21. 
	Bag and contain arisings.
	Lead driller

	22. 
	Reinsert tool and repeat points 16 to 21 until sample or UXO test depth is reached.
	Lead driller

	23. 
	If required, advance casing by surging with casing head and pin or by driving with drop tools.
	Lead driller

	24. 
	Remove casing head and add additional length of casing as required.
	Lead driller

	25. 
	At test/sample depth, carry out SPT / CPT with Magcone (for purpose of magnetometer surveys to identify presence of UXO) or U100.
	Lead driller

	26. 
	Take intermediate bulk (bag), disturbed (tub) or water (bottle) sample as instructed and environmental/ contamination samples as required schedule or if contamination is encountered.
	Lead driller

	27. 
	Proceed to borehole termination depth
	Lead driller

	28. 
	Once the borehole has been drilled to the required depth and backfilled / installed as per the project requirements, remove all casing from the borehole and reinstate as per the drilling instruction and / or installation instruction.
	Lead Driller

	29. 
	Remove casing in lengths using winch. Back hammer with tools if required.
	Lead driller

	30. 
	All spoil / waste can be removed via support plant to the land, a floating skip or equivalent TBC. 
	Lead Driller, Pontoon Works

	31. 
	If any point during the drilling process, the area is found to be contaminated or contamination is found local to the drilling area, stop work immediately. The Field work Supervisor will be informed and if needed additional measures will be put in place.
	Lead Driller

	32. 
	The Rig will remain erect on the Pontoon until the exploratory locations are complete. Once all locations are completed the Pontoon will be brought back to the shore and unloaded using a crane if necessary. 
	Lead Driller, Pontoon Works

	33. 
	The Rig will then be lowered using the reverse of points 11 to 7. Then it will be lifted off the Pontoon using a crane. 
	Lead driller

	34. 
	Remove all spoil and waste to associated skips and observe the requirement to segregate waste. If contaminated, then confirm waste arrangements with the fieldwork supervisor prior to moving any waste. Once the site is clear of all waste and equipment collapse any fencing / exclusion zone and confirm with the field work supervisor that the location is clear.
	SOCOTEC Fieldwork Supervisor /

Lead Driller


	
	Likelihood (L)
	

	Severity (S)
	Score
	1
	2
	3
	4
	5
	Score
	Likelihood (L)
	Score
	Severity
(S)
	Low Risk
	1-6

	
	1
	1
	2
	3
	4
	5
	1
	Very Unlikely
	1
	Minor Injury (No Lost Time)
	No further action – Maintain Control
	

	
	2
	2
	4
	6
	8
	10
	2
	Unlikely
	2
	Minor Injury (Lost Time)
	Medium Risk
	7-12

	
	3
	3
	6
	9
	12
	15
	3
	Likely
	3
	Over 7 Day Injuries (Lost Time)
	Put in place further controls to reduce to Low Risk
	

	
	4
	4
	8
	12
	16
	20
	4
	Very Likely
	4
	Major Injuries
	High Risk
	13-25

	
	5
	5
	10
	15
	20
	25
	5
	Certain
	5
	Death
	Do not carry out work. Review Activities & Improve immediately
	

	

	


	General Activity Assessment

	
	Hazards
	Persons Affected
	Initial Risk
	Control Measures


	Residual Risk (RR)

	
	
	
	L
	S
	Risk Rating
	
	L
	S
	RR

	1. 
	Manual Handling
	Workers:
Injury caused by incorrect lifting heavy tools, samples, plant etc causing muscle strains
	3
	3
	9
	· It is the responsibility of the Lead Driller to set up the work location in such a way that equipment is laid out so that it is accessible and the need for excessive movements of loads minimised. This includes the use of mechanical aids such as FLT and ensuring equipment can be dropped off at the work location.
· Always utilise mechanical lifting assistance where available. Enlist multiple-person lift if mechanical aid is unavailable. If unsure that lift can be completed alone, stop work and seek assistance

· When using multiple person lifts, ensure clear communication is established and maintained at all times.

· Ensure that path is clear prior to lifting. Ensure that lifted item doesn’t visually obscure path during lift.

· Take regular breaks when conducting large volumes of manual handling.

· Wear appropriate gloves for each manual handling task.

· Stretching and warming up muscles prior to commencing lifting operations (particularly when having travelled a significant distance to site) is required to prevent sprains and strains. 
· Any individual with a known health problem should identify this to the Site Supervisor for specific assessment by an H&S Manager or Occupational Health Manager. 
· All personnel to will be encouraged to adopt the Pristine Condition principles of manual handling. Use the Pristine Condition Essential 4:

· INSIDE BASE, BIG ENGINES, TURN NOT TWIST, DIP ‘N’ DRIVE 

· Ongoing training is available by means of the SOCOTEC UK online training modules (via the intranet), toolbox talks and practical demonstrations.

	1
	3
	3

	2. 
	Slips / Trips / Falls etc.
	Workers, Supervisory Staff:

Injury and in extreme cases death from slips / trips / falls.


	4
	5
	20
	· All staff to be briefed on housekeeping & a ‘Don’t Walk By’ policy regarding reporting & removal of potential trip hazards.

· Housekeeping is to be of a high standard and the site team must ensure they employ a ‘tidy as you go’ practice.
· Any trailing hoses and cables to be routed away from pedestrian accessed points. Keep tools suitably stored / out of established walking zones.
· Remove all trip hazards from the work area prior to commencing work.  Trip hazards that cannot be removed should be highlighted / segregated.

· Where water arising from the borehole is anticipated, a slurry trap is to be erected prior to breaking ground.

· Excess water arising from the borehole or entering the work area should be channelled away where possible.

· Use waffle boarding when setting up, on area that have or will become a risk to slips. 
· Plan routes prior to carrying any load.

· Safety footwear to be worn at all times (lace up boots with ankle support, steel toe and sole protection). Alternatives may be considered but only following completion and approval of an activity specific risk assessment. 

	1
	5
	5

	3. 
	Contact with Buried Services
	Workers, Supervisory Staff:
Risk of Serious Injury or Death through damage of underground services by electrocution / explosion etc
	4
	5
	20
	· CCSC are to take full responsibility for service avoidance and setting out.

· All intrusive activities will be carried out in accordance with HSG47 & GS6 Guidelines if applicable.
· Each proposed hole location must be checked against the issued service plans. Service drawings / information to be obtained from the Client.

· Move borehole location if possible, should the proposed borehole be in vicinity of known live service (confirm with client).
· Employ a safety stand off 
· Once all parties are satisfied that the work location is clear of known services, a ‘Permit to Dig’ will be issued to be signed off by the Client. 

· Permit to Dig must be completed, read, understood and signed by all relevant persons involved prior to breaking ground.

· A hard copy of the Permit and issued service plans will be located in the Site File at all times.

· Always treat services as ‘live’.

· If unknown / uncharted services are encountered, report to PM team.

· If damage to a service is found / caused, report IMMEDIATELY 

· Follow industry recommended standards for excavating close to services.

· If at all unsure, stop work and seek advice from site supervisor.
	1
	5
	5

	4. 
	Contact with Overhead Services
	Workers, Supervisory Staff, Visitors, General Public:

Risk of serious Injury or death; electrocution through damage to services.

	3
	5
	15
	· No overhead services have been identified during the site visits, howe ver:

· In the presence of any overhead services in the vicinity of the proposed location, SEEK ADVICE from SOCOTEC UK Project Manager.  
· As a basic rule, NO work will take place within horizontal distances of 10m of overhead lines. This is considered a hold point; should works have to take place within 10m of overhead lines, the service provider will be consulted for advice prior to work in that location.
· Presence of overheads to be covered in site specific induction.
· Where appropriate, GS ‘goalpost’ barriers and blue cones, in accordance with Avoidance of Danger from Overhead Electric Power Lines General Guidance Notes GS6 from the HSE, will be installed on the drilling platform as precautionary measures to ensure sufficient clearance on access routes.  
· Plant and equipment will be manoeuvred under the supervision of the SOCOTEC UK Engineer to ensure that adherence to any exclusion zones are maintained, at all times.
· Exposure to the associated overhead services will be reduced by limiting the number of plant movements along access routes and the number of personnel within each working area of concern.
·   Set out designated passing places beneath overhead cables.

	1
	5
	5

	5. 
	Presence of UXO
	Workers, Supervisory Staff, Visitors, General Public:

Risk of serious Injury or death due to historic UXO presence.
	4
	5
	20
	· Desk study to be provided by CCSC and level of mitigation TO BE CONFIRMED, below details the expected necessary mitigation 
· UXO classification for the site to be included within the project plan.
· UXO specialist to be employed to monitor any excavations for potential UXO. 
· If UXO is encountered during the GI, work will cease immediately. 
· All personnel will be evacuated to a safe area including property / landowners / public that may be in danger. 
· As per UK UXO Reporting Procedures the Police will be contacted immediately on 999.
	1
	5
	5

	6. 
	Injury During Erection / Operation / Lowering
	Workers, Supervisory Staff:
Risk of crushing or trapping injuries

	4
	5
	20
	· Erection and operation of the rig is to be conducted or supervised by trained drilling operative.
· Erection & lowering of Derrek is to be done using the electric winch system.   
· Stay-bars & spreader bar to be properly secured to the Derrek once erected.
· Daily plant condition checks will be conducted by a member of the drill crew prior to each shift with any defects reported.
· Apply grease to grease recharge points as appropriate.

	1
	5
	5

	7. 
	Exposure to Vibration
	Workers:
Risk of long term health problems such as VBF.
	2
	4
	8
	· SOCOTEC drill rigs are regularly monitored for vibration. No rigs have been identified as posing an undue risk to the operator from a HAVS perspective. 
· All work which poses a vibration risk must be planned prior to operation taking place to minimise use of vibration tools.  
· Information on Vibration levels to be assessed by the project lead prior to work commencing. The choice of tool used will be the lowest vibration rating possible commensurate with the work required to minimise exposure. 
· If the operator has not received HAV training or is not in possession of the vibration values of the equipment then they are NOT TO PROCEED and contact their Line Manager for instruction.
· Operator must not exceed 100 points in any given 24 hour period. (Please see procedure GS-SMS-000 2.12 within the Safety Management System). 
· If an operator exceeds 100 points then he / she MUST STOP Work and report this to their line manager.
· Technicians are to keep their hands warm and should take regular breaks. 
· It should be appreciated that smokers are more at risk to the long term effects of vibration.

	1
	4
	4

	8. 
	Noise - Exposure to Harmful Noise Levels
	Workers, Supervisory Staff:
Long term health problems with hearing loss.
	4
	4
	16
	· The hearing protection zone around plant will vary depending on type of plant being used. To that end if it is not possible to hear normal conversation at 2m, that is a rough guide that exposures exceed the second action level and staff must either don suitable ear defenders or withdraw to a distance where this is possible.
· First action level 80dB – Offer hearing protection.

· Second action level 85dB – Wearing of hearing protection and exclusion zones are mandatory.
· If noise generated by the rig during drilling operations is in excess of the second action level, hearing protection will be mandatory for everyone directly involved in the drilling operation. 
· Maximum engine noise levels will be clearly displayed on the rig.
· Mandatory PPE signage should be displayed both on the rig and on the entrance to the work area.

· The hearing protection zone around the rig will vary depending on ground conditions, operations and material being drilled. Specific noise assessment can be arranged on request or as part of ongoing monitoring by the Safety Manager or Occupational Health Manager.

	1
	4
	4

	9. 
	Entrapment / Entanglement 
	Workers, Supervisory Staff:
Risk of crushing or trapping injuries.
	4
	5
	20
	· Lead Driller and Drilling Support Operative to establish an agreed system of hand and verbal signals when pulling or adding to the drill string.
· Lead driller to operate rig only when Drilling Support Operative has indicated that it is safe to do so.
· No personnel should be underneath the legs when being erected or lowered.
· All rotating parts to be fitted with fixed guards at all times.
· Emergency stop control is fitted to the rig adjacent to the controls. 
· Non-authorised personnel are prohibited from entering the working area whilst drilling is being carried out.
· The Lead Driller must be able to see, without any obstruction, the hands and feet of the driller at all times. 
· Hands must be kept clear of the lip of the casing, SPT anvil surface etc. 
· The Lead Driller must ensure that the driller’s hands and feet are clear when lowering tools and casing to the ground.
· All personnel within the segregated work area to have received a rig induction from a member of the drill crew.
· All mobile phones to be left in the vehicle while drill rig is operational.
· All pinch points on the drill rig are highlighted.
· Personnel will not wear loose fitting clothes and long hair will be tied back
· Pins & permanent guide loop are installed around crown wheel to prevent the wire rope from becoming displaced.  
· No personnel should place any parts of their body under suspended loads 
· A second permanent loop & anti whip check bar are installed on the mast to prevent ‘whip action’ on the wire rope.

	1
	5
	5

	10. 
	Overturning of Rig
	Workers, Supervisory Staff:
Risk of crushing or trapping injuries.
	2
	5
	10
	· The rig will be located on a level working surface and will be erected as per SOCOTEC Standard Operating Procedures & the BDA procedural practice. Rig to be erected using fitted electric winch.
· Level mast by placing additional timbers as necessary. 
· Rig can be secured if deemed necessary by the Lead Driller or floatation provider via ratchet straps tied down onto lash down points located on the drilling platform. 


	1
	5
	5

	11. 
	Fall from Height


	Workers:
Risk of serious injury or death.
	4
	5
	20
	· Do not ascend the mast under any circumstances.  
· If the situation can only be resolved by ascending the mast, this should be done under a septate bespoke risk assessment and as the last resort.

	1
	5
	5

	12. 
	Exposure to Hazardous Substances
	Workers, Supervisory Staff, General Public:
Risk of short and long term harm to health.
	3
	4
	12
	· COSHH and SDS data sheets for hazardous substances used during the drilling process are provided in the driller’s safety file.

· Refer to individual COSHH assessments for any hazardous substances used.
· Suitable PPE for handling hazardous substances, used during the drilling process, will be provided.
· Operator must familiarise themselves with the SDS and COSHH assessment prior to handling hazardous materials.
· Eye washes are held within the 1st aid kit which will be present on the drilling platform.
· Wash hands prior to handling food or smoking.

	1
	4
	4

	13. 
	Exposure to Leptospirosis (Weil’s disease).
	Workers, Supervisory Staff:
Short and long term health risks, in extreme cases death to infected persons.
	3
	4
	12
	· The naturally occurring bacteria can get into your body through cuts and scratches and through the lining of the mouth, throat and eyes after contact with infected urine or contaminated water, such as in sewers, ditches, ponds and slow-flowing rivers.
· The following guidance should be given to all staff: 
· Wear impervious gloves.
· Wash your hands and any contaminated clothing regularly. Always wash hands before eating, drinking or smoking.

· Don’t touch rats or livestock with unprotected hands.
· Wash cuts and grazes immediately with soap and running water and cover all cuts and broken skin with waterproof plasters before and during work.

· Signs and symptoms start with a flu-like illness with a persistent and severe headache, which can lead to vomiting and muscle pains and ultimately to jaundice, meningitis and kidney failure. 

· In rare cases the diseases can be fatal. If suffering these signs and symptoms, report to your doctor.  Leptospirosis is much less severe if it is treated promptly. If your doctor decides you have leptospirosis contact the SOCOTEC UK accident helpline immediately on 01327 810666.

	1
	4
	4

	14. 
	Contaminated Land / Made Ground (not asbestos)
	Workers, Supervisory Staff:
Risk of irritation / infection caused by potentially harmful substances in Made Ground spoil / samples
	3
	4
	12
	· Client to provide information of known hazards in Pre-Construction health and safety information (PCI) to describe the potential land contamination constraints considered likely at the site. The SISG classification for the site is 
Yellow
· Where land has been classified as “YELLOW” or “RED” in accordance with the BDA Classification (Contamination or Potentially Contaminated Land BDA 2008), then the specified PPE and decontamination facilities will be used (BS10175). 
· SOCOTEC UK Engineer will monitor all the arisings / samples as a precautionary measure. Exposure to potentially general contaminated soil will be mitigated by:
· Wearing mandatory PPE as standard practice for contaminants anticipated for a ‘YELLOW’ classified site. 
· Maintaining strict hygiene standards i.e. no smoking on site and cleaning hands before eating or drinking whilst progressing through and sampling Made Ground.

· In the event that suspected or potential contaminants are encountered:
· STOP WORK, make safe immediately and report to Project Manager.

· Dynamic Risk Assessments must be carried out and mitigations agreed if work is to proceed, i.e. provision of additional & specific PPE / RPE prior to continuing
· If necessary (dependent on contamination levels / types), the Sample Management Plan will be revised to RED. This must accompany samples when they are collected and transferred from site to the sample store or laboratory.
	1
	4
	4

	15. 
	Contact with Potential Asbestos Containing Materials (ACM)
	Workers, Supervisory Staff, General Public:
Risk of long term respiratory disease caused by inhalation of asbestos fibres
	3
	4
	12
	· If suspected ACM is exposed cease work immediately and contact the Project Manager.
· An assessment will then be made as to whether the remainder of the works in the area of concern constitutes Non Licensed, Notifiable Non-Licensed or Licensed Asbestos work.


	1
	4
	4

	16. 
	Failure of equipment
	Workers, Supervisory Staff:
Risk of serious injury or death
	4
	4
	16
	· All equipment must be checked by the drill team prior to use, this includes hand tools, drill tooling, bowsers, rigs and vehicles. These checks need to be recorded

· All lifting accessories must be in date with their LOLER inspection (6 months inspection regime) and the drill team must ensure they have access to the latest certificates upon request for the items on site

· Rigs must have a valid LOLER certificate (12 month inspection regime)

· Any defective equipment must be taken out of service immediately and reported to line manager.

· Any terminated ends on rope must be done as per BDA recommendations using a torque wrench to the correct setting.
	1
	4
	4

	17. 
	Damage to Environment
	Environment:
Risk from run-off from sediment during wet weather conditions. Damage caused by fuel leaks, spills, split hydraulic hoses etc; access / egress.

	3
	3
	9
	· Drip trays, spill kits will be present and readily available on site. 

· A clean, slip free work area is to be maintained, at all times.
· All plant on site must have valid inspection certification and daily plant checks carried out and recorded.
· Diesel, oils & other hydrocarbons to be stored in bund 1.5 times capacity of the containers within, or temporarily in drip trays – not anticipated to be on the platform.
· Use / store the minimum amount of fuels / chemicals necessary to reduce the risk from spillages.
· Any refuelling of the rig will only take place in the designated area.
· Each drill crew to carry a plant nappy and minimum 20l spill kit.

· Plant nappy to be deployed under engine block prior to erecting rig.
· No refuelling or use of hydraulic oil on ancillary equipment is to occur without first deploying a plant nappy or drip tray.
· Where hydraulic oil is used in ancillary equipment e.g. piston sampler, biodegradable hydraulic oil is to be used.
· Only the agreed and designated routes to the work locations will be used. 
· SOCOTEC UK to report any spillages that do occur and records to be kept.
· A secure bund will be constructed (via the use of visqueen) around the immediate drilling area.
· The final number and location of the boreholes is yet to be confirmed. Boreholes may be required within 10m of the watercourse in such cases all borehole arisings will be managed and controlled so as to avoid any slurries entering the river. The slurries will be stored in suitable containers with transport to relocate the arisings at a suitable controlled storage area before onward transmission to treatment, storage or waste.

	1
	3
	3

	18. 
	Working Over Water

	Workers, Supervisory Staff:

Risk of hyperthermia and death by drowning. 

	5
	5
	25
	· Life Jackets will be provided by SOCOTEC and Pontoonworks to all personnel working over water.
· Edge protection will be present around both the drilling platform and transport barge.
· All personnel associated with overwater works will be briefed as per the Pontoonworks RAMS, and how to carry out access and egress from the platform.
· Safety personnel with Inflatable boats will be present on-site full time to act as rescue personnel if someone falls overboard from the drilling platform / transport barge / inflatable boat etc. 
· No over water work will commence until the floatation platform is approved by the supplier supervisor. 
· Overwater works must be suspended if no floatation platform Personnel are present. 
	1
	 5
	5

	19. 
	Drilling Arisings/Slurries
	Environment:

Risk of drilling waste entering watercourse

	5
	4
	20
	· All slurries will be managed so as to avoid any loss to the environment.
· A bund is to be in place prior to any drilling works taking place.

· If at any point drilling arisings begin to flood the work area then cease works immediately and address.
· Any waste will be removed on floating plant to a suitable disposal point where it will be removed by pumping to waste storage prior to being stored or removed from site to waste.
	1
	4
	4

	20. 
	Migrating Salmon
	Environment:

Risk of disturbance to migrating salmon

	4
	4
	16
	· No percussive drilling should be undertaken two hours before and two hours after high tide.

· No flood lights to be used over the river at any time.

· Working hours to be kept between dawn and dusk.
	1
	4
	4


	Assessor Name & Role

	R Brewer Generic assessment for the City and County of Swansea Council
	Signature & Date
	15/06/22

	Reviewer Name & Role


	Niall Kiernan
	Signature & Date
	20/09/22


	Site Specific Hazards – include site specific hazard not identified in General Activity Assessment above or use to capture change.

	
	Hazards
	Persons Affected
	Initial Risk
	Control Measures


	Residual Risk (RR)

	
	
	
	L
	S
	Risk Rating
	
	L
	S
	RR

	1
	COVID-19
	SOCOTEC Employees, Client, Designer, public 


	3
	5
	15
	Separate site specific RAMS covering the current COVID-19 crisis have been produced and Safe System of Work has been developed by SOCOTEC UK. Ensure these RAMs and the new SSOW have been understood and will be implemented.


	1
	5
	5

	2
	Access / Egress
	SOCOTEC Employees, Client, Designer, public 


	3
	3
	9
	Stick to pre-agreed access routes. SOCOTEC will limit the equipment taken onto the worksites and only mobilise what is essential for the drilling works. 


	1
	3
	3

	3
	Welfare – Hand washing, heating food, hot drinks
	SOCOTEC Employees, family members 


	3
	3
	9
	A welfare unit will be available on site and comprise hot / cold running water, flushing toilet, canteen facilities and separate office. The welfare will be equipped with sanitisers, soaps and cleaning products.

	1
	3
	3

	4
	Inclement Weather 
	SOCOTEC Employees
	4
	4
	12
	Weather constraints remain a safety and financial hazard, no personnel will travel out to the Pontoon if the Pontoon Works personnel report working conditions unsafe. 


	4
	1
	4

	5
	Grounding of the barge and subsequent overturning during tide level changes


	SOCOTEC Employees, floating plant provider employees
	5
	5
	25
	Confirm Bed levels 
Confirm floating plant draft 

The employer must provide sea levels tables affecting the BH locations to a local sea datum 

The employer must provide offset between the local sea datum relative to ordnance survey datum (OSD).

Prepare table of required bed depths at each BH location in advance of establishment.

Compare bed levels prior to anchoring floating plant if margin of safety is small reposition plant in deeper water ensuring plant does not impact on the river bed.

Final safety methods to be refined and confirmed
	2
	5
	10


	Information and Instruction 

	BS5930:1999

BS1377:1990

BDA Health & Safety Manual For Land Drilling – A Code of Safe Drilling Practice (2015)
BDA Guidance For The Safe Operation of Cable Percussion Rigs & Equipment (2016)



	I confirm that I have read and understood the risk assessment and method statement. I will follow the instructions given within, if I feel this cannot be achieved or the work method changes, then I will STOP work and seek further instruction from a supervisor / line manager.

	Confirmation that controls have been implemented
	Y/N
	Name & Role
	
	Signature & Date
	

	Acceptance of Assessment

	Y/N
	Name & Role
	
	Signature & Date
	

	Acceptance of Assessment

	Y/N
	Name & Role
	
	Signature & Date
	

	Acceptance of Assessment

	Y/N
	Name & Role
	
	Signature & Date
	

	Acceptance of Assessment

	Y/N
	Name & Role
	
	Signature & Date
	

	Acceptance of Assessment

	Y/N
	Name & Role
	
	Signature & Date
	

	Acceptance of Assessment

	Y/N
	Name & Role
	
	Signature & Date
	

	Acceptance of Assessment

	Y/N
	Name & Role
	
	Signature & Date
	

	Acceptance of Assessment

	Y/N
	Name & Role
	
	Signature & Date
	

	Acceptance of Assessment

	Y/N
	Name & Role
	
	Signature & Date
	

	Acceptance of Assessment

	Y/N
	Name & Role
	
	Signature & Date
	

	Acceptance of Assessment

	Y/N
	Name & Role
	
	Signature & Date
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