
Permit Number: 	PAN-018186			Operator: 		GFI73 LTD

Facility: Waunarlwydd Generatio    	Form Number: 	 Air1 / 22/11/2022
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY 
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value*
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1 – A48 [6]
	Oxides of nitrogen (NO and NO2 expressed as NO2) [6]
	190 mg/Nm3 [6]
	In line with web guide: Monitoring stack emissions: low risk MCPs and specified generators
	
	In line with web guide: Monitoring stack emissions: low risk MCPs and specified generators
	
	

	A1 – A48 [5]
	Carbon monoxide [5]
	No limit set
	In line with web guide: Monitoring stack emissions: low risk MCPs and specified generators
	
	In line with web guide: Monitoring stack emissions: low risk MCPs and specified generators
	
	



* Monitoring requirements are defined at a temperature of 273.15 K, a pressure of 101.3 kPa and after correction for the water vapour content of the waste gases at a standardised O2 content of 15 % for engines.

[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
[5]    Monitoring frequency for carbon monoxide monitoring is every 3 years from date of acceptance of first monitoring measurements under condition 3.2.3
[6]    Monitoring and limit applies from 01/01/2025 or immediately when the Tranche A Specified Generator becomes a Tranche B Specified Generator whichever comes first

Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)
