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	Permit Reference Number
	BU2357 / AP363455
	
	Operator:
	Warwick Chemicals

	Installation :
	Mostyn, Flintshire
	
	Form Number :
	A2 / (Combustion process)


	Reporting of Emissions to Air for the period:
	From
	1st January 2022
	To:
	30th July 2022


	Emission Point
	Substance/Parameter
	Emission Limit Value
	Result [1]
	Test Method [2]
	Sample Date and Times [3]
	Accreditation/ Certification [4]
	Uncertainty [5]

	A17
	Oxides of Nitrogen
	170mg/m3 [6]
	Nil report 

Plant shut down
	BS EN 14792
	-
	MCERTS
	-

	A18
	Oxides of Nitrogen
	170mg/m3 [6]
	Nil report 

Plant shut down
	BS EN 14792
	-
	MCERTS
	-

	A19
	Oxides of Nitrogen
	170mg/m3 [6]
	Nil report 

Plant shut down
	BS EN 14792
	-
	MCERTS
	-

	A21
	Oxides of Nitrogen
	170mg/m3 [6]
	Nil report 

Plant shut down
	BS EN 14792
	-
	MCERTS
	-

	A17
	Carbon Monoxide
	70mg/m3 [6]
	Nil report 

Plant shut down
	BS EN 15058
	-
	MCERTS
	-

	A18
	Carbon Monoxide
	70mg/m3 [6]
	Nil report 

Plant shut down
	BS EN 15058
	-
	MCERTS
	-

	A19
	Carbon Monoxide
	70mg/m3 [6]
	Nil report 

Plant shut down
	BS EN 15058
	-
	MCERTS
	-

	A21
	Carbon Monoxide
	70mg/m3 [6]
	Nil report 

Plant shut down
	BS EN 15058
	-
	MCERTS
	-


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum - maximum measured values.

[2] Where an internationally recognised standard test method is used the reference number is given; Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given. -

[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.

[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

[6] The emission limit values for oxides of nitrogen and carbon monoxide are expressed as a maximum individual hourly average value and corrected to 273K, 101.3kPa, 3% oxygen, dry.
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	Date:
	30th January 2023

	
	(Authorised to sign as representative of Warwick Chemicals)
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