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1.0 Purpose
The purpose of this procedure is to specify the standard of those parts of the site infrastructure which are required to ensure compliance with other parts of the management system. 
Specifically, the parts of the site infrastructure which has been identified as being significant in ensuring compliance with the management system are: -

· the site surfacing, 

· the drainage systems, 

· the security infrastructure. 
This procedure therefore sets out the construction standard for these items. 
2.0 Scope
Site surfacing, drainage systems, and security infrastructure. 
3.0 Responsibility
Site supervisor

Site operatives
Technically competent manager

4.0 Procedure
4.1 Site office
4.1.1 All day to day control and supervision, administration, management, welfare facilities are provided by way of the site office. 
4.1.2 All records kept under the management system are also stored within the site office.
4.2 Site surfacing

4.2.1 The site surfacing consists of areas of impermeable pavements, areas of permeable hardstanding and some areas of unmade ground. Activities on site should be carried out in areas provided with appropriate surfacing as detailed in SOP-03.
4.2.2 Where ‘impermeable pavements’ are required, these must be areas provided with concrete or tarmac surfacing which are constructed and maintained such that they are impermeable to liquids and which are either laid to fall or provided with kerbs preventing liquids running off the pavement. 
4.2.3 Where significant quantities of materials which are corrosive in nature are stored (such as lead acid batteries), the surfacing must be treated with a chemical resistant coating to ensure that the surface remains impermeable.
4.2.4 Where ‘hardstanding’ is mentioned in this system, this should be areas of compacted hardcore or similar which have sufficient durability to allow clearing by scraping.
4.2.5 Current surfacing details are concrete on the lower waste a handling areas, tarmacadam on the upper pedestrian and recyclates areas and hard standing on peripheral areas. 
4.3 Drainage system
4.3.1 Mess facilities are connected to foul sewer.
4.3.2 Interceptors and filters to be inspected regularly and emptied as required. 
4.3.3 Surfaced areas are laid to fall towards drainage channels and underground drainage pipes connecting up to interceptor and on to storm drains
4.4 Security infrastructure 
4.4.1 The site must be protected with security fencing to prevent unauthorised access. Furthermore, the fencing should be in place to minimise the risk of windblown litter escaping the site.

4.4.2 The site is currently protected by security fencing of a minimum of 1.8 m height around the circumference of the HWRC.
4.4.3 The Site is located on the Ffrwdgrech Industrial Estate, the main entrance is provided with a secure lockable gate. 

4.4.4 The site will also have CCTV cameras in operation.

4.4.5 The gates/entrance will be supervised whenever the site is open. 

5.0 References

· SOP-03: Waste storage and handling 

· SOP-07: Maintenance
· Drawings (within the Site Management System)
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