Appendix 6c
Oil Storage Assessment Form


Site   Silent Valley Landfill Site

Tank


Date


	Item
	Yes/No
	Comments 

	Tank
	
	

	Is the tank in good condition (unlikely to leak or burst in ordinary use)?
	
	

	Is the secondary containment impermeable to water and oil?
	
	

	Is the containment system intact and without openings or valves for drainage?
	
	Ensure any cracks or other damage is carefully repaired.

	Are any draw-off pipes and fill pipes that pass through the containment system sealed adequately?
	
	

	Tank ancillary equipment
	
	

	Are all valves, filters, sight gauges, vent pipes and taps within the secondary containment system?
	
	

	If the tank has a sight gauge, is it supported properly and fitted with a valve that closes automatically when the gauge is not in use?
	
	

	Are fill and draw-off pipes located or protected so that they cannot be damaged by an impact or a collision?
	
	

	And, if applicable, protected from corrosion?
	
	

	And, if above ground, supported properly?
	
	

	Are vent pipes, taps and valves arranged so that any oil lost will be retained within the containment system?
	
	

	Are all taps and valves fixed to the storage tank, through which oil can be discharged to the open, fitted with locks and locked shut when not in use?
	
	

	Deliveries to the tank (filling)
	
	

	Is the fill pipe situated within the secondary containment system, or if not, is a drip tray of adequate capacity provided to contain any oil that may remain in the pipework after filling?
	
	Ensure the drip tray is emptied after the tank is filled.

	Can the tank and vent be seen from the point where the filling operation is controlled, or if not, is the tank fitted with an automatic overfill prevention device?
	
	

	If the tank has a screw fitting or other fixed coupling, is it in good condition?
	
	

	Are fittings/couplings being used when the tank is filled?
	
	

	Flexible draw off pipes
	
	

	Is the flexible draw-off pipe fitted with a tap or valve at the delivery end that closes automatically when the draw-off pipe is not in use?
	
	

	If the tap or valve is capable of being fixed in the open position, it should have an
	
	

	automatic shut-off device.
	
	

	Is the pipe kept within the secondary containment system when not in use or enclosed in a secure cabinet equipped with a drip tray?
	
	

	Is there a lockable valve where the pipe leaves the container which is locked shut when not in use?
	
	

	Pump set draw-off (non gravity draw off)
	
	

	Is the pump set fitted with a non-return valve in the feed line to the pump?
	
	

	Is the pump set protected from unauthorised use (locked or isolated when not in use)?
	
	

	Is the pump set located or protected so that it cannot be damaged by an impact or a collision?
	
	


Inspected by

Signed



