Permit Reference Number : BX3376IG					Operator : Continental UK Teves Limited

Installation : Continental UK Teves Limited					Form Number : S1

Reporting of Emissions to Sewer for the period from 01-01-2018 to 31-12-2018
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Accreditation/ Certification [4]
	Uncertainty
[5]

	S1
	pH
	6-11
	N/A 
	Plant & Lab Meters
	N/A
	N/A
	N/A

	S1
	Chromium and its compounds
	1mg/l
	N/A
	N/A Atomic Absorption
	N/A

	N/A
	0.5%

	S1
	Zinc and its compounds
	2mg/l
	N/A
	N/A Atomic Absorption
	N/A
	N/A
	0.5%

	S1
	Nickel and its compunds
	2 mg/l
	N/A
	N/A Atomic Absorption
	N/A
	N/A
	0.5%

	S1
	Cadmium and its compounds
	0.01 mg/l
	0.01
	Yearly average/dilution
	1st Jan 2018 – 31st Dec 2018
	N/A
	
0.5%

	S1
	Mercury and its compounds
	0.005 mg/l
	0.002
	Yearly average/dilution
	1st Jan 2018 – 31st Dec 2018
	N/A
	0.5%

	S1
	Cadmium and its compounds
	0.60 kg
	0.10
	Mass Balance Calculation
	1st Jan 2018– 31st Dec 2018
	N/A
	N/A

	S1
	Mercury and its compounds
	0.12 kg
	0.02
	Mass Balance Calculation
	1st Jan 2018 – 31st Dec 2018
	N/A
	N/A

	S1
	Total flow
	N/A
	9977m3
	N/A Ultrasonic Flow Meter at Outfall
	1st Jan 2018 – 31st Dec 2018
	M/CERTS
	3.48%


[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. colorimetry.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements, or flow/time proportional samples, the percentage of the process operating time covered by the monitoring is given.   
[4] The accreditation status of the equipment and/or the monitoring organisation, as appropriate, for the methods used for both sampling and analysis.
[5] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated. The following uncertainties are quoted on a different basis (basis as stated) – {The basis of any other uncertainty figure needs to be stated. Where no figure is available the Agency will need to agree an appropriate uncertainty value.} 
Signed [image: ]……………………………….  		Date 14.01.19
……………..			(authorised to sign as representative of the Operator)                      





Permit Reference Number : BX3376IG					Operator : Continental UK Teves Limited

Installation : Continental UK Teves Limited					Form Number : E1


Reporting of Energy Usage for the year …2018……………………….

	
Energy Source
	Energy Usage
	
CO2
Produced
(tonnes)
	
	Trends in Energy Usage

	
	
Quantity
	Primary Energy
(MWh)
	
	
	Year
	Parameter

	
	
	
	
	
	
	Primary Energy usage
	CO2
 produced

	
	
	
	
	
	
	
	

	
	
	
	
	
	2011
	2,280
	1,196

	Electricity *
	MWh
	1798
	910
	
	2012
	2,768
	1,452

	Gas
	tonnes
	Nil
	Nil
	
	2013
	3,460
	1,815

	
	
	
	
	
	2014
	3,566
	1,853

	
	
	
	
	
	2015
	2,246
	1,167

	
	
	
	
	
	2016
	2,063
	1,072

	TOTAL
	-
	
	
	
	2017
	2.049
	1,065

	
	
	
	
	
	2018
	1,798
	910


* Conversion factor for delivered electricity to primary energy = 2.4

	Operator’s comments :  Electricity = total site usage/2.4


[bookmark: _GoBack]
               
[image: ]
Signed …………………………….  		Date: …14.01.19………..		
	(authorised to sign as representative of the Operator)



Permit Reference Number : BX3376IG					Operator : Continental UK Teves Limited

Installation : Continental UK Teves Limited					Form Number : R1


Reporting of Waste Disposal and Recovery for the year …2018…………………….

	Waste
Description
	Disposal
	Recovery
	
	Trends in Waste Disposal and Recovery

	
	Route
	Tonnes
	Tonnes
	
	Year
	Parameter

	
	
	
	
	
	
	Waste 1
	Waste 2
	Total Hazardous Waste (Tonnes)

	(1) Non-Filter Cake Waste
	External treatment/land fill
	34.04
	Nil
	
	2009
	45.16
	9.34
	54.5

	(2) Filter Cake
	Landfill
	32.040
	Nil
	
	2010
	3.79
	36.56
	40.35

	Total hazardous waste
	
	
	
	
	2011
	51.86
	26.60
	78.46

	
	
	
	
	
	2012
	51.074
	42.040
	93.114

	TOTAL WASTE
	
	66.08
	Nil
	
	2013
	35.14
	41.06
	76.2

	
	
	
	
	
	2014
	24.223
	59.6
	83.828

	
	
	
	
	
	2015
	92.801
	44.204
	137.005

	
	
	
	
	
	2016
	74.567
	46.94
	121.502

	
	
	
	
	
	2017
	55.807
	41.2
	97,007

	
	
	
	
	
	2018
	34.04
	32.040
	66.08

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	



	Operator’s comments : Significant volume reduction in plated parts 2018 to 2017 accounts for much of filter cake reduction




[image: ]
Signed ……………………………………….  		Date: 14.01.19…………..
(authorised to sign as representative of the Operator)

Permit Reference Number : BX3376IG					Operator : Continental UK Teves Limited

Installation : Continental UK Teves Limited	Ebbw Vale				Form Number : WU1


Reporting of Water Usage for the year 2018……………………….
	Water Source
	Usage
(m3)
	
	
	
	
	Trends in Water Usage

	
	
	
	
	
	
	Year
	Parameter

	Mains Water supply
	9,977 m3
	
	
	
	
	
	Named 
Water source
	Total 
Water usage
	Water per unit output

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	2009
	Mains water
	6475
	7 litres

	
	
	
	
	
	
	2010
	Mains water
	6337
	7 litres

	
	
	
	
	
	
	2011
	Mains water
	8,597
	8  litres

	
	
	
	
	
	
	2012
	Mains water
	8,427
	7 litres

	TOTAL WATER USAGE
	9,977 m3
	
	
	
	
	2013
	Mains water
	10,056
	7 litres

	
	
	
	
	
	
	2014
	Mains water
	10,948
	6.9 litres

	
	
	
	
	
	
	2015
	Mains water
	14,972
	8.4 litres

	
	
	
	
	
	
	2016
	Mains water
	17,902
	10.3 litres

	
	
	
	
	
	
	2017
	Mains water
	12,095
	7.7 litres

	
	
	
	
	
	
	2018
	Mains water
	9,977
	8.1 litres

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	




	Operator’s comments :  




[image: ]
Signed …………………………………….  		Date…14.01.19
………..			(authorised to sign as representative of the Operator)

Permit Reference Number : BX3376IG					Operator : Continental UK Teves Limited

Installation : Continental UK Teves Limited	Ebbw Vale		2018		Form Number : MR1

	Mass Release 
	
	Trends in Mass Release 

	Parameter
	Limit
	kg
	
	

	
	
	
	
	Year
	Parameter

	Cadmium and its compounds
	0.60 kg
	0.10
	
	
	Mercury
	Cadmium
	

	Mercury and its compounds
	0.12 kg
	0.02
	
	2009
	0.013
	0.051
	

	
	
	
	
	2010
	0.013
	0.044
	

	
	
	
	
	2011
	0.013
	0.044
	

	
	
	
	
	2012
	0.013
	0.044
	

	
	
	
	
	2013
	0.02
	0.13
	

	
	
	
	
	2014
	0.0012
	0.13
	

	
	
	
	
	2015
	0.013
	0.19
	

	
	
	
	
	2016
	0.02
	0.2
	

	
	
	
	
	2017
	0.02
	0.11
	

	
	
	
	
	2018
	0.02
	0.10
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	




	Operator’s comments: Results obtained via mass balance.   Number of parts produced in 2018 = 1.23 million







[image: ]

Signed …………………………………………………………….  		Date …14.01.19……………..		
	(authorised to sign as representative of the Operator)
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