Permit Number: 	WP3231NB                        		Operator: 		Dairy Partners (Cymru Wales) Limited 

Facility:		The Creamery, Aberarad 		Form Number: 	 Water1 / 16/05/2023

Reporting of emissions to water (other than to sewer) and land for the period from DD/MM/YYYY to DD/MM/YYYY

	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	W1

(monitoring location: Flow monitoring meter at NGR: SN 31538 40242)
	Maximum daily discharge volume
	900m3/day
	24-hour total
	
	MCERTS flow meter
	
	

	W1

(Monitoring location: Point M1 as shown on site plan in Schedule 7: M1 NGR: SN 31611 40208)
	Biological oxygen demand (BOD)
	20 mg/L
	24-hour flow proportional composite
	
	BS EN 1899-1
	
	

	
	Chemical oxygen demand (COD)
	110 mg/L
	24-hour flow proportional composite
	
	BS 6068-2.34
	
	

	
	Total suspended solids (TSS)
	30 mg/L
	24-hour flow proportional composite
	
	BS EN 872
	
	

	
	Ammoniacal nitrogen (expressed as N)
	10 mg/L
	Instantaneous (spot sample)
	
	BS EN ISO 11732
	
	

	
	Nitrite (expressed as N)
	1.0 mg/L
	Instantaneous (spot sample)
	
	BS EN ISO 13395
	
	

	
	Total nitrogen
	20 mg/L
	24-hour flow proportional composite
	
	EN 12260 or EN ISO 11905-1
	
	

	
	Total phosphorus
	1.0 mg/L
	24-hour flow proportional composite
	
	EN ISO 6878 or EN ISO 15681-1 or EN ISO 15681-2 or EN ISO 11885
	
	

	
	Total aluminium as Al
	1.0 mg/L
	Instantaneous (spot sample)
	
	BS EN ISO 11885
	
	

	
	Temperature
	
21 °C
	Instantaneous
	
	Standard Thermocouple Sensor
	
	

	
	pH
	Minimum 6,
Maximum 9
	Instantaneous
	
	BS EN 10523
	
	

	
	Mercury and its compounds, expressed as mercury (Total Hg)
	0.5 µg/L

50 g/year
	Compliance based on mass balance calculation 
	
	BS EN 12846

	
	

	
	Cadmium and its compounds, expressed as cadmium (Total Cd)
	0.525 µg/L

50 g/year
	Compliance based on mass balance calculation 
	
	BS EN ISO 5961
	
	

	W2
	Visible oil and grease
	None visible
	Instantaneous (visual examination)
	
	Visual check
	
	

	W3
	Visible oil and grease
	None visible
	Instantaneous (visual examination)
	
	Visual check
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.


Signed …………………………………………………………….  		Date………………………..
	(Authorised to sign as representative of Operator)
