Schedule 6 – Notification
These pages outline the information that the operator must provide.
Units of measurement used in information supplied under Part A and B requirements shall be appropriate
to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions 

and authorized emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential 

information, supplied on a separate sheet and accompanied by an application for commercial confidentiality 

under the provisions of the PPC Regulations.

Part A
	Permit Number / Variation Notice Number
	BR8212IK / (EPR/BR8212IK/V004)

	Name of operator
	Knauf Insulation

	Location of Installation
	Cwmbran

	Time and date of the detection
	22/11/2018 approx 11:00 - 12:05


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	22nd November 2018 approx 09:55 - 12:05

	Reference or description of the location of the event
	A1 – Furnace Stack

	Description of where any release into the environment took place
	To air in the Pontypool /Cwmbran area 

	Substance(s) potentially

released
	Oxides of Sulphur as SO2

	Best estimate of the quantity or rate of release of substance
	Average result of the three taken was 151.9 mg/m3

	Measures taken, or intended to be taken, to stop any emission
	The BOC valve control issue was rectified on 30/11/18 by BOC

	Description of the failure or accident
	Liquid Oxygen was being supplied to the furnace by the sites BOC plant due to poor valve control when operating the furnace burners on VSA. Liquid Oxygen has a higher purity


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	A1

	Parameter(s)
	

	Limit
	Oxides of Sulphur as SO2 of 150 mg/m3

	Measured value and uncertainty
	151.9 mg/m3 and +/- 11.7 mg/m3

	Date and time of monitoring
	22nd November 2018

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection 

	
	

	Substance(s) detected
	Oxides of Sulphur as SO2

	Concentrations of substances detected
	151.9 mg/m3 and +/- 11.7 mg/m3

	Date of monitoring/sampling
	22nd November 2018


Part B – to be submitted as soon as practicable

	Any more accurate information on the matters for notification under Part A.
	BOCs Oxygen blower tripped on genuine high vibrations. This had not long been installed (service exchange on hours) so the stand by unit was in the process of being stripped and overhauled. The spare unit was reinstalled on 30/11/18. During this period BOC supplied liquid Oxygen, of  high purity, to the plant.

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	The spare unit has been overhauled and a second spare unit is on order by BOC therefore three units will be on site to prevent such a reoccurrence leading to the requirement to use liquid Oxygen.

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused be the emission
	If, for any reason, liquid Oxygen use is required again the plant will review the increase in MnO2 additions to the furnace and change Oxy/Gas ratios on the furnace burners. 

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	There have been zero previous unauthorised air emission releases in the previous 24 months.


	Name*
	Warren Christy

	Post 
	HS&E Manager

	Signature
	                             [image: image1.emf]

	Date
	18/04/2019


* authorised to sign on behalf of Knauf Insulation Limited

Permit Number BR8212IK

Variation Notice Number EA/EPR/BR8212IK/V003


