Schedule 6 – Notification
These pages outline the information that the operator must provide.
Units of measurement used in information supplied under Part A and B requirements shall be appropriate
to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions 

and authorized emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential 

information, supplied on a separate sheet and accompanied by an application for commercial confidentiality 

under the provisions of the PPC Regulations.

Part A
	Permit Number / Variation Notice Number
	BR8212IK / (EPR/BR8212IK/V004)

	Name of operator
	Knauf Insulation

	Location of Installation
	Cwmbran

	Time and date of the detection
	16/05/2019 approx 16:00


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or fugitive emission which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	16th May 2019 approx 16:00

	Reference or description of the location of the event
	A3 – Forming Stack

	Description of where any release into the environment took place
	To air in the Pontypool /Cwmbran area 

	Substance(s) potentially

released
	Volatile Organic Compounds as C

	Best estimate of the quantity or rate of release of substance
	Results are varying however initial average reading 167 mg/m3

	Measures taken, or intended to be taken, to stop any emission
	Investigating root cause by sequentially removing potential causes from the process (source of VOC and operation of abatement system)

	Description of the failure or accident
	Investigation ongoing


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	A3

	Parameter(s)
	Volatile Organic Compounds as C

	Limit
	27 mg/m3

	Measured value and uncertainty
	167 mg/m3 

	Date and time of monitoring
	16th May 2019 approximately 16:00

	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection 

	
	

	Substance(s) detected
	Volatile Organic Compounds

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B – to be submitted as soon as practicable

	Any more accurate information on the matters for notification under Part A.
	During the sites bi-annual extractive emission sampling process, it was identified by the sampling contractor, Exova, that the VOC levels from the emission point A3 were above the sites allowed level and significant larger than normally measured.

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	During the in depth investigation into the high VOC levels the root cause was investigated by sequentially removing potential causes from the process. This had minimal effect on changing the VOC readings provided by the sampling equipment. As such the sampling device was changed by Exova to review if it was operating correctly and the monitoring results immediately reduced to the levels expected by the site and below the emission limit for the site.

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused be the emission
	Exova to bring two such VOC monitoring units to ensure both are reading simultaneous results to ensure their validation during the next run of emissions sampling on site.

	The dates of any unauthorised emissions from the installation in the preceding 24 months.
	22/11/18 – Oxides of Sulphur Levels 151.9 mg/m3


	Name*
	Warren Christy

	Post 
	HS&E Manager

	Signature
	                             [image: image1.emf]

	Date
	05/06/2019


* authorised to sign on behalf of Knauf Insulation Limited

Permit Number BR8212IK

Variation Notice Number EA/EPR/BR8212IK/V003


