Permit Number: 	EPR/BV4177IS			Operator: 		Volac International Ltd
Facility:		Volac Felinfach		                          Form Number: 	 Air1 / 04/12/2023
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY 
	Emission Point
	0BSubstance / Parameter
	Emission Limit Value
	Reference Period
	Monitoring frequency
	Result0F[footnoteRef:1] [1:  The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.] 

	Test Method1F[footnoteRef:2] [2:  Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases, the principal technique is stated, for example gas chromatography.] 

	Sample Date and Times2F[footnoteRef:3] [3:  For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   ] 

	Uncertainty3F[footnoteRef:4] [4:  The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.] 


	A15
	Sulphur Dioxide (SO2)
	30 mg/Nm3
	Periodic
	Annual
	
	BS EN 14791
	
	

	
	Oxides of Nitrogen (NO and NO2 expressed as NO2)
	250 mg/Nm3
	Periodic
	Annual
	
	BS EN 14792
	
	

	
	Total Particulate Matter (PM)
	10 mg/Nm3
	Periodic
	Annual
	
	BS EN 13284-1
	
	

	
	Carbon Monoxide (CO)
	150 mg/Nm3
	Periodic
	Annual
	
	BS EN 15058
	
	

	
	Carbon Monoxide (CO)
	150 mg/Nm3
	Hourly average
	Continuous Measurement
	
	BS EN 14181[footnoteRef:5] [5:  CEMs which meet the MCERTS requirements should also follow the principles of EN 14181 (i.e. QAL2/AST and QAL3) but a reduced number of parallel measurements may be acceptable (subject to NRW approval).
* Emission limit value expressed as mass of emitted substances per volume of waste gas under the following conditions: dry gas at a temperature of 273.15 K and a pressure of 101.3 kPa without correction for oxygen content.] 

	
	

	A1
	Dust
	10 mg/Nm3*
	Periodic
	Annual
	
	EN 13284-1
	
	

	A4
	Dust
	10 mg/Nm3*
	Periodic
	Annual
	
	EN 13284-1
	
	

	A8
	Dust
	10 mg/Nm3*
	Periodic
	Annual
	
	EN 13284-1
	
	

	A9
	Dust
	10 mg/Nm3*
	Periodic
	Annual
	
	EN 13284-1
	
	

	A10
	Dust
	10 mg/Nm3*
	Periodic
	Annual
	
	EN 13284-1
	
	

	A11
	Dust
	10 mg/Nm3*
	Periodic
	Annual
	
	EN 13284-1
	
	

	A20
	Dust
	10 mg/Nm3*
	Periodic
	Annual
	
	EN 13284-1
	
	



Signed …………………………………………………………….  		Date………………………...   	
	(Authorised to sign as representative of Operator)
