Polders - Rhymney Great Wharf
Archaeology Plan
1) Survey:
A survey will take place before works commence with the following requirements:
· Walkover survey identifying any archaeological remains. Where walking is not possible due to soft mud, UAV to be used
· Survey only along (5m either side to be included) the design drawing lines, not within the polder area.
· Brief report with map showing location and nature of finds, along with GPS locations

2) Reporting
The report will be shared with RCAHMW when published and a meeting will be organised if necessary to discuss findings and next steps. If the report shows no finds in the affected area, there will be no further action to take, other than an instruction to contractors to remain vigilant during construction for any remains that may have been missed or that emerge during construction. 
3) Mitigation
In line with the Marine Plan principles for archaeological finds of Avoid – Minimise – Mitigate, should archaeological finds be present in the area of the work, the procedure will be as follows:
a) Finds within the vehicle pathway area
An exclusion zone will be created around the remains and contractors will work on the other side of the fencing boundary. Where possible, work will also be undertaken on foot around the exclusion area to ensure that no damage occurs.
b) Finds within the fenceline area
Any remains which lie within the footprint of the fenceline will be recorded, dated and sampled (to be agreed with RCAHMW depending on the nature of the find). If possible, the fenceline will be altered slightly to go around the remains. Further mitigation will be discussed following the production of the survey report.

