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	Site Specific Activity and Control Measures        

                                     (This section must be completed)


	Method
	Hand Fill

	
	Location
	General site area where plant/vehicles operating

	
	Duration
	Duration of contract

	
	Control
	Competency of machine operatives

	Exposure Limits


	5mg/m3 8hr Time Weighted Average value

10mg/m3 15 minutes Short Term Exposure Limit for Oil Mist

	Physical Properties
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	Mineral oil and additives

	Hazard
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	Mildly irritating to eyes

Skin irritation and dermatitis may result from prolonged use

	
	
	May cause skin cancer

	Work Procedures/PPE

[image: image4.wmf]

	Hand protection (Impervious heavy duty knitted wrist gloves) BS EN 374

Eye protection (BS EN166 F3)

	First Aid/Fire
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	Inhalation: remove to fresh air and rest

Ingestion: do not induce vomiting, give plenty of water in sips

Eye Contact: irrigate with water for at least 15 minutes

Skin Contact: wash with soap and rinse with plenty of water

Fire: powder/foam/CO2, DO NOT USE WATER, wear self contained breathing apparatus

	Storage/Disposal
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	Storage: as per manufacturers recommendations

Disposal: as special waste

	Environmental
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	Do not allow to enter mains drain, sewers or watercourses

Clean up spills immediately using the spill kits provided and dispose of material as special waste.
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