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APPLICATION FOR A MARINE LICENCE FOR MARINE WORKS

Marine Works include, but are not limited to, coast defences, beneficial uses of dredged materials, subsea cables, pontoons, jetties, land reclamation, grab samples and outfall pipes under the Marine and Coastal Access Act 2009

Please read the notes carefully before completing the form.
The Marine Licensing Team (MLT) administers Part 4 of the Marine and Coastal Access Act 2009 on behalf of the Licensing Authority, the Welsh Ministers.

The completed application form must be accompanied by a location plan and, where appropriate, descriptive drawing(s) and any supporting environmental assessments. 

Please submit applications to the Permit Receipt Centre via the details at the top of this form. For applications larger than 20MB, we would advise that you contact us to determine the most appropriate method for submitting your application.
 
Please submit marine licence applications, including this form and all supporting documents, at least 4 months before the licence is required.

Some projects may raise matters that require a significantly longer time for consideration. These are most likely to be:

· Projects that fall within The Marine Works (Environmental Impact Assessment) Regulations 2007 – as amended requiring an Environmental Statement
· Large scale projects with substantial volumes of material being deposited or excavated
· Works requiring an Appropriate Assessment to be conducted under The Conservation of Habitats and Species Regulations 2017.

Information should be provided about the anticipated duration of the entire project in respect of works below/seaward of Mean High Water Spring (MHWS). Where appropriate, planned phasing of the work for which consent is sought must be detailed. For projects lasting more than one calendar year, planned phasing details must be given for each 12 month period.

A licence fee is payable in respect of an application. Details of fees can be found on our web pages.

Please note applications will not be processed without the correct relevant fee or invoicing details.  

Payments can be made via Cheque, BACS or credit/debit card. 
· Cheques should be crossed and made payable to Natural Resources Wales. 
· For BACS payments ensure you provide the reference number (not remittance number)

Further information on payment methods can be found on our web pages.

All activities need to comply with the Water Framework Directive (WFD). The framework and guidance can be found on the Natural Resources Wales website, http://naturalresources.wales. The results of your WFD assessment must be attached to your marine licence application.

Please answer all questions. If any information is not available at the time of application please indicate in the relevant section, giving reasoning in a covering letter. Outstanding details must be submitted as soon as possible. Any delay in forwarding details is likely to result in delays in determining your application.

Your application may not be considered complete and therefore not processed until key information has been submitted. Your application may be returned if you fail to submit outstanding information within given timescales.
 
Please note any licence may have conditions that must be discharged before works can commence. This will take additional time. 
If you have any queries with regards to completing this application please contact the MLT: marinelicensing@naturalresourceswales.gov.uk

How your application will be processed by the MLT: 

Submit all application to the Permit Receipt Centre via the details at the top of this form.

Checked and acknowledged by the MLT within 21 days of receipt of application and payment 

If the application is complete and no further information is needed at this time, your application will be placed in a work queue to be assigned a permitting officer

If the application is not complete, further information will be request and need to be provided before the application can be considered as complete

Our 4 months service level for determining non-EIA applications will begin from the date the completed application is received (Please note some projects may take significantly longer than 4 months to determine due to their nature)

EIA projects may take significantly longer due to their scale and complexity. Therefore we encourage early engagement with the MLT

Your application and supporting documents will be sent to for an initial consultation period of 28 days (42 days for EIA projects)

For the majority of projects, a public notice must be advertised. Public consultation will be 28 days (49 days for EIA projects). For EIA projects a second public notice will be required. The MLT will advise on how this should be done.

Responses to consultation will be considered and additional information requested at this time, if necessary.

A decision on your Marine Licence Application will be made

All information submitted may be referred to within a licence, therefore all works must be in accordance with this information, unless otherwise agreed with NRW acting on behalf of the Licensing Authority during the determination process.
It is the responsibility of the applicant to obtain any other consents/authorisations that may be required.

Application Form Structure 
1. Project Description and Cost
2. Applicant Details
3. Details of Agent, Contractor, Vehicles and/or Vessels used to carry out works 
4. Environmental Impact Assessment (EIA)
5. Licensable Period
6. Project Description
7. Methods Statement
8. Materials of Project 
9. Beach Replenishment, Land Reclamation or Salt Marsh Feeding
10. Temporary Works
11. Dredge and Disposal of Dredge Material
12. Protected Sites
13. Other Consents
14. Statutory Powers
15. Public Register
16. Application Fee
17. Declaration

Check List
Please ensure that you have included all the necessary information before you submit your application. If any of the below are not completed in the application form, the application is likely to be considered incomplete and may be returned to you

	Item
	Yes (√)

	The applicant is a legal entity?
	

	The declaration is signed by the applicant?
	

	Is the application fee correct?
	

	Are the grid references/coordinates correct?
	

	Do the coordinates match map locations?
	

	Have all the relevant supporting documents been submitted?
	

	Has a clear methodology been provided in the application form?
	

	Has Protected sites information been included?
	

	Has a Water Framework Directive (WFD) assessment been submitted?
	

	Are all the continuation sheets for application questions appended with correct corresponding numbers?
	


	
Should you have any queries regarding you application please contact the MLT via marinelicensing@naturalresourceswales.gov.uk  

1. Project Description and Cost

1 (a).	Project Name

Brockhole Stream Flood Alleviation Scheme




1(b).	Please provide a brief description of the proposed project, including locationThe Proposed Scheme is situated in Blackpill, Swansea, a small coastal district approximately 5 km southwest of Swansea city centre, positioned along Mumbles Road. The site lies directly on Swansea Beach, with its location recorded at grid reference SS 61954 90510.

The Brockhole Stream Flood Alleviation Scheme (FAS) is situated in Blackpill, Swansea.  The scheme is required to address the long-standing and recurrent flooding associated with the Brockhole Stream, which poses significant risk to residential and commercial properties, the local community and the critical transport link of Mumbles Road.  

The proposed FAS includes a series of integrated works designed to provide flood protection and to improve conveyance capacity to reduce flood risk throughout the Brockhole stream catchment (between Clyne Gardens and Mumbles Road). While the overall scheme involves improvements within Clyne Gardens, Woodman Lane and the upstream channel, only the outfall works below Mean High Water Spring (MHWS) falls within this marine licence application. The works upstream of the existing seawall are above MHWS and have already received planning consent from Swasnea Council.    






















1(c).	Please provide an estimated gross cost of the project (Inc. materials and labour) for works that fall below/seaward of Mean High Water Springs (MHWS)
£100,000





2. Applicant Details
To whom the licence will be issued. This must be a legal entity such as an individual, registered company/ charity or public body. 
Mr
Jack Davies

Title				Full Name

Company or Trading
NameSwansea Council



Company Registration
Number (if applicable)


Name of Contact or 
individual (if different)
Principle Engineer

Position in Company



City and County of Swansea
Civic Centre
Swansea, 
SA1 9DT

Address inc. postcode
(provide registered
Company address if
applicable)


Telephone Number07880 426488


jack.davies@swansea.gov.uk


Email Address
3. Details of Agent, Contractor, Vehicles and/or Vessels used to carry out works 

3(a).	Agent Details 
This is who we will correspond with unless otherwise informed. If no agent we will contact the applicant.
Abbie Jenkins
Miss

Title				Full Name

Company or Trading
NameAtkinsRealis

00688424

Company Registration
Number (if applicable)


Name of Contact or 
individual (if different)

Position in CompanyMarine Environmental Scientist


West Glamorgan House, 
Orchard St, 
Swansea, 
SA1 5AD.

Address 
(Inc. postcode)




02920358019

Telephone Number
abbie.jenkins@atkinsrealis.com


Email Address

3(b).	Does the Applicant wish to be included in all correspondence? Yes ☒	No ☐

3(c).	Contractor Details
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Contractor Company or Trading Name
	Address

	Not currently in place




3(d).	Will the works require the use of vessels?				Yes ☐	No ☒

3(d) (i).Vessel Details (if applicable and available)
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Operator
	Name of Vessel
	Type of Vessel
	Vessel Registration Number
	Country of Registration

	N/A

	
	
	
	




3(e).	Will the works require the use of vehicle?				Yes ☒	No ☐

3(e) (i). Vehicle Details (if applicable and available) to be used below MHWS
In order for contractors to benefit from the licence permission, details must be provided. 
Any details not provided with application must be confirmed before operations commence. 

	Operator 
	Type/Description of Vehicle

	

	6T- 9T Wheeled dumper

	

	Wheeled Telehandler to transport materials

	

	20-25T Tracked excavator with excavation bucket

	

	20–25T Tracked excavator with grab to place blockstone

	
	Lifting apparatus

	
	Small tools such as drills, disc cutters, breakers and whacker plates 

	
	Pumps and settlement tanks for over pumping

	
	Concrete mixer and pumps.

	
	Temporary timber formwork and metal falsework to form the shuttering for the concrete wall.  

	The following plant and Equipment is anticipated to being required to complete the works (The exact sizes of these may vary depending upon the preferred contractor). All plant and equipment will be taken off the beach and stored in the site compound above MHWS at the end of each day.  




3(f).	If the contractor or vessels or vehicles are not known at the application stage, when do you expect to provide these details?
These details will need to be confirmed prior to the licence and operations commencement
A contractor for the works has not been appointed at this stage. Contractor to be appointed prior to the works.





4. Environmental Impact Assessment (EIA)
Certain projects, due to their scale, location and/or nature, may require an EIA under the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended). If a project qualifies under EIA, an Environmental Statement (ES) must be prepared and submitted with the application.

Projects that fall within Annex I of the Directive automatically require an EIA. Projects that fall within Annex II of the Directive are assessed on a case-by-case basis for the requirement for an EIA to be undertaken.

4(a).	Do you consider the works to be under the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended)?				Yes ☐	No ☒									
4(a) (i) If Yes, which Annex does the proposal fall under?	     Annex I☐	   Annex II☐

4(a) (ii) Which number(s) within the Annex does the proposal relate to?

N/A




4(b).	Have you applied for a screening or scoping opinion from the MLT under the Marine Works (Environmental Impact Assessment) Regulations 2007 (as amended)?  									Yes ☐	No ☐
N/A

4(b) (i). If Yes, please provide the reference number

4(c).	Has an Environmental Impact Assessment been undertaken? 	Yes ☐ No ☐											
4(c)(i).If Yes, has an Environmental Statement been submitted to support this Marine Licence application? 						Yes ☐ No ☐	

4(d).	If an Environmental Impact Assessment has been undertaken, but an ES has not been submitted, please provide an explanation

N/A





Please continue on a separate sheet if necessary. Please tick if you have done this ☐


5. Licensable Period

Determination of applications will be based on the works taking place during these dates. Please ensure you have included an adequate contingency period. If works are not completed by the Requested Licence Expiry Date you may be required to submit a new application. Including a contingency period within your original application does not impact on Licence Fee
30/09/2029
01/10/2026

Start Date				Requested Licence Expiry Date


Please ensure you submit your application for a Marine Licence at least 4 months prior to the intended start date. Some projects, such as EIA projects, will take significantly longer to determine.
6. Project Description

6(a).	Please give a description of the proposed project.
This should include the purpose of the project, estimated timescales of construction and operation, and broken down by the phases of works, if applicable. Details should include, but not be limited to, dimensions of project, quantity of material being deposited and removed.
The scope of works will involve:
· Construction of a new 1050mm diameter buried culvert on land behind the existing sea wall, with discharge to Swansea Bay. 
· Excavation and redistribution of existing sediment and sand on the beach to form a new wider channel to accommodate the new outfall pipe 
· Saw-cutting and break-out of the existing concrete sea wall to accommodate the new outfall pipe.  
· In-situ concrete placement to form the sea wall around the new outfall pipe.  
· Installation of 89 1m x 1m x1m blockstones to form the banks of the widened open channel as part of the permanent works.  The blockstone will laid upon geotextile and set within concrete.  
· Installation of 124 0.5m x 0.5m x 0.5m blockstones to the channel invert for a length of 9m to provide scour protection.  
· Associated temporary fencing, access gates and vegetation removal to allow construction of the works.  
The works associated with this marine licence application are likely to take place over a 6 month period. This is dependent on weather and tidal conditions. The full description of the works including construction, phases of works, quatity of material deposited and removed can be found in 5122859-ATK-XX-GEN-RP-C—00003 Brockhole Methodology for Marine Licence_P01






















Please continue on a separate sheet if necessary. Please tick if you have done this ☐

6(b).	Please detail the location of the proposed construction project.
These should be Latitude and Longitude coordinates (WGS84) in decimal degrees to 5 decimal places (e.g. Lat 52.12345 Long -4.12345), defining the extent of the project.
Point 1: 51.596284 , -3.9946009    Point 3: 51.596161 , -3.9940971
Point 2: 51.596741 , -3.9942339    Point 4: 51.596576 , -3.9938316
This area is slightly larger compared to the green line boundary working area shown in 5122859_60_ATK-XX-ZZ-DR-C-0034 P01 to give flexibility for vehicle access.









Please continue on a separate sheet if necessary. Please tick if you have done this ☐
6(c).	The following must be provided with the completed application form:

(i) a suitably scaled extract of an Ordnance Survey Map or Admiralty Chart with location of project, complete with North Arrow and Scale

(ii) construction plans and sectional drawings showing those proposed works below/seaward of MHWS, which should give details of the materials to be used (for beach replenishment the quantity, particle size and source of material to be deposited and deposit location is also required).

(iii) a descriptive schematic drawing and suitably scaled location plan which show the full extent of the project clearly in relation to the surrounding area and features.

Please list below all supporting documents that have been submitted with this application, including suitable documents/maps/drawing titles and reference numbers
· 5122859-ATK-XX-GEN-RP-C-0003 Brockhole Methodology for Marine Licence P01
· 5122859_60-ATK-XX-ZZ-DR-C-0034 P01 – General arrangement of Proposed Works 
· 5122859_60-ATK-XX-ZZ-DR-C-0035 P01 – Sectional arrangement of Proposed Works
· 5122859_60-ATK-XX-ZZ-DR-C-0100-P03 – Key Plan and extent of works (for reference)
· 5122859_60-ATK-XX-ZZ-DR-Z-0200 P03 – Site compound
· Brockhole Flood Alleviation Scheme Water Framework Directive Assessment
· Brockhole Welsh National Marine Plan (WNMP) assessment
· Location of Brockhole Map
· PEA for Brockhole Stream Flood Alleviation Scheme – Car Park Wall and New Culvert to Beach Outfall.


















Please continue on a separate sheet if necessary. Please tick if you have done this ☐

The applicant should note that these drawings/plans may be copied to others as part of the MLT's consultation procedures. If they are subject to copyright, it is the responsibility of the applicant to obtain the necessary approvals to reproduce the documents.

7. Methods Statement

7(a).	Please provide a detailed method statement for the works
This must include methods for all works including temporary structures or deposits such as jetties, cofferdams, moorings or landing stages to be constructed seaward of MHWS
All works below MHWS covered in this marine licence application will be undertaken during suitable low‑tide windows to provide safe access to the beach and to minimise environmental risk and working within the water.

The full method statement can be found in 5122859-ATK-XX-GEN-RP-C-0003 Brockhole Methodology for Marine Licence P01.

Temporary Beach Access and Working Areas
Temporary access to the beach will be achieved via two access ramps constructed from the cycle path down onto the beach on either side of the outfall, as shown on drawing 5122859_60‑ATK‑XX‑ZZ‑DR‑C‑0034. Each ramp will be formed by placing a geotextile layer directly onto the beach surface, overlaid with compacted clean granular stone material to provide a stable and defined access route for plant and equipment.













Excavation and Management of Beach and Channel Sediment  
The existing outfall channel below MHWS will be widened and deepened by means of controlled excavation undertaken using a tracked excavator operating from the beach. Prior to the commencement of these activities, a temporary bypass channel or an over-pumped outfall extension will be installed to divert flows around the excavation and discharge flows further down the bay. Thus, ensuring that plant operates within dry working conditions. Excavation will be carried out using an excavator on the beach and will be in short, sequential sections, progressing in a seaward direction, in order to maintain stability of channel banks and to avoid excessive disturbance of beach material. Sediment, sand and gravel removed during excavation are anticipated to be non-contaminated. This material will be temporarily stockpiled within the working area and subsequently redistributed within the vicinity of the works, thereby retaining sediment within the local coastal system. 

Cutting through the existing sea wall
Concrete cutting will be carried out using disc cutters in controlled stages to prevent uncontrolled breakout. A small cut will be made both vertically and horizontally and all concrete faces.  This will be broken out with a breaker on a excavator to break out the required size to accommodate the 1050mm diameter pipe. All slurry, cutting water and concrete arisings will be fully contained on the protected working surface and collected for removal from site. At no point will cutting residues or debris be permitted to enter the tidally influenced area.

Installation of culvert through the sea wall  
Once the opening through the sea wall has been formed, the culvert outfall will be lifted into position using an excavator fitted with certified lifting equipment. The pipe will be aligned and temporarily supported before localised backfilling is carried out to provide initial stability. Formwork will then be installed around the opening and in‑situ concrete will be placed to reinstate the sea wall around the pipe.

Scour Protection and Channel Reinstatement
Following culvert installation, the outfall channel below MHWS will be reinstated to the design profile. All sand material will be redistributed around the beach. A geotextile separation layer will be placed within the scour protection footprint to limit settlement and to prevent washout of underlying material. 89 blockstone units measuring approximately 1m x 1m x 1m and 124 blockstone units measuring 0.5m x 0.5m x 0.5m will then be installed using an excavator on the beach with a grab attachment to aid placement. The blockstone for the invert will provide long‑term scour and erosion protection at the outfall. Blockstone to the sides will be used to form the new channel sides. The blockstone used will be bed on a layer of concrete to ensure stability over the design life of the scheme. These works will be undertaken at low tide and working in the dry.  

Removal of Temporary Works and Demobilisation
On completion of the works below MHWS, all temporary access ramps, geotextiles, and other temporary works will be removed. The beach will be reinstated to its pre‑construction condition as far as reasonably practicable, and all plant and materials will be removed from the working area.

Access routes
Prior to commencement of construction activities, a temporary site compound will be established above MHWS, located to the south of Mumbles Road as shown on drawing 5122859_60‑ATK‑XX‑ZZ‑DR‑C‑0034 P01. Construction materials, including granular backfill and pipe sections, will be delivered to the site by road via Mumbles Road and temporarily stored within the compound. This arrangement ensures that materials are stored above MHWS and only transferred near to the foreshore when required for the works.  


















































7(b). Do you intend to undertake activities that could generate underwater noise?
								Yes ☐ No ☒


7(b) (i). If Yes, what type(s) of activities will be undertaken?

No – all works below MHWS covered in this marine licence application will be undertaken during suitable low‑tide windows to provide safe access to the beach and to minimise environmental risk and working in the water. Activities will be carefully programmed by the contractor to avoid inundation by the incoming tide.












7(b) (ii). If Yes, approximately how many days will the activity be undertaken for?  
N/A








If Yes, you will be required to complete an additional form that will be provided.

7(c).	Please state the measures to be taken to:
(i) Minimise risk to the marine environment 
· Silt control measures, such as silt fencing, settlement tanks or silt bags, will be deployed as required to limit sediment mobilisation and prevent release into the wider marine environment.
· Geotextile and containment measures will remain in place throughout concreting works to prevent washout or pollution. All concreting activities will be completed within low‑tide windows, and no concrete, wash water or slurry will be permitted to enter the marine environment. The concrete to be used will have special antiwash out additives for use in a marine environment. All concrete poured will be sealed with in the timber formwork and falsework.
· Channel bed and bank levels will be trimmed to achieve a stable tie‑in with the culvert outlet and the widened channel. All works will be completed within low‑tide windows to ensure environmental protection and safe working conditions.
· Pollution prevention and control procedures will be adhered to by the contractor (guidance available at: gpp 5-works-and-maintenance-in-or-near-water.pdf) 
· Spill response kits will be available on all plant. 
· Minimise plant traffic. 
· Designated access and egress routes, marking features of importance. 
· Storage of materials (fuel, chemicals, construction waste) above Mean High Water. 
· All equipment, temporary structures, access tracks, waste and/or debris associated with the works will be removed on completion of the works. 
· Bunding, storage facilities and spill kits will be employed to contain and prevent the release of fuel, oils and chemicals associated with the plant, refuelling and construction equipment into the marine environment. 
· Plant, vehicles and machinery will not be refuelled on the foreshore; this will take place in the site compound above Mean High Water only. 
· All equipment, materials, machinery and Personal Protection Equipment (PPE) used will be in a clean condition prior to their arrival on site, and upon removal from site, to minimise risk of introducing non-native species into the marine environment. 
· Works will commence in daylight hours. 

Information on mitigation measures can be found in Section 9 of 5122859-ATK-XX-GEN-RP-C-0003 Brockhole Methodology for Marine Licence P01.




































(ii) Prevent undue interference to others 


It is anticipated that all construction activities will be limited to daytime hours (for, example 8:00am to 18:00 from Monday to Friday and from 8:00am to 13:00 on Saturday). There will be no nighttime working. There will be no works over Christmas, New Year, Easter public holidays and Bank Holidays. Working times within these time windows will vary as they will need to coincide with the low tide times. 












(iii) Maintain navigational safety, including marking and lighting of works
No additional lighting, work to take place during day time hours only.














Please continue on a separate sheet if necessary. Please tick if you have done this ☐

8. Materials of Project 

8(a).	Description of materials to be deposited seaward of MHWS (Please tick all that apply)
Timber	☐	Iron/Steel	☐	Concrete	☒	Biocides/other chemicals	☐
Silt		☐	Stone/Rock	☒	Gravel		☐	Plastic/Synthetics		☐ 
Sand	☒	Other		☒	

If other, please provide a description of materials.
· 42 m Fencing (Timber post and rail fencing) 
· 1 3m wide field gate
· 89 Blockstone (1m x 1m x 1m) to channel sides  
· 124 Blockstone (0.5m x 0.5m x 0.5m to channel invert
· Concrete (Bed and surround for blockstones– 61m3
· Geotextile (beneath blockstone) – 268m2
· Excavation of channel (sand to be redistributed) - 292 (m3)

Information in Section 4 of  5122859-ATK-XX-GEN-RP-C-0003 Brockhole Methodology for Marine Licence P01.
















8(b).	Delivery method of materials to site
If sea delivery, please include details of vessels to be used with a chart of proposed route and transhipment area. If vehicle delivery, please provide the proposed access route. 
Access to the site and the site compound will be via Mumbles Road then across the pedestrian footpath/ cycle path. Plant and equipment for all works will access the beach via two 
temporary ramps (One to the north east and one to the south west) constructed from the cycle path level and down onto the existing beach on either side of the outfall (As depicted in 5122859_60-ATK-XX-ZZ-DR-C-0034 P01). The access to and from the beach is indicated as a red arrow on the drawing.

Information on access route and vehicle movements in Section 6 of 5122859-ATK-XX-GEN-RP-C-0003 Brockhole Methodology for Marine Licence P01.















Please continue on a separate sheet if necessary. Please tick if you have done this ☐

8(c).	Will the works involve removals seaward of MHWS?		Yes ☒ No ☐

8(c) (i). Description of materials to be removed seaward of MHWS (Please tick all that apply)
Timber	☐	Iron/Steel	☐	Concrete	☐	Biocides/other chemicals	☐
Silt		☐	Stone/Rock	☐	Gravel		☐	Plastic/Synthetics		☐ 
Sand	☒	Other		☐	
8(c) (ii). Description of objects/materials to be removed seaward of MHWS
Including quantities to be removed.
· Excavation of channel (sand to be redistributed) – 292m2. Excavation of approx. 292m2 sand will be undertaken around the existing outfall to create sufficient space for the new channel alignment. The excavated material will be redistributed within the defined working area to maintain sediment balance and avoid the need for off‑site disposal.
· 3m3 concrete from the existing sea wall.














9. Beach Replenishment, Land Reclamation or Salt Marsh Feeding
For works involving any of the above, please provide the following information 

9(a). Is the material to be deposited like for like to existing material? 	Yes ☐ No ☐

9(a)(i) If No for Beach Replenishment please provide justification why?
N/A











9(b).	Description of material to be deposited
Please provide the grading specification of materials to be used, if using a range of grain sizes please state the percentage by weight passing. If unsure, please refer to the Wentworth Scale 
N/A












Please continue on a separate sheet if necessary. Please tick if you have done this ☐

9(c).	Source of the material to be deposited
Including dredged or land based stating the origin of material

N/A







9(d).	Has the material been chemically analysed? 			Yes ☐ No ☐
If material has been analysed, we may request this information to determine the application

9(d) (i) If Yes, is the analysis data been included with the application? Yes ☐ No ☐

10. Temporary Works

10(a).	Will there be any temporary deposits below MHWS? 		Yes ☒ No ☐
This includes construction materials, removed objects/material, jetties or cofferdams
If Yes, please continue with section 10

10(b).	Please provide the location of temporary deposits 
Please include a map/chart displaying the location of temporary deposits, if necessary.
Temporary Beach Access
•	Geotextile (beneath ramps) 70m2 – temporary deposit
•	Stone for ramps 11m3 – temporary deposit












10(c).	Description of temporary deposits
Temporary access to the beach will be achieved via installation of two access ramps constructed from the cycle path down onto the beach on either side of the outfall, as shown on drawing 5122859_60‑ATK‑XX‑ZZ‑DR‑C‑0034 P01. Each ramp will be formed by placing a geotextile layer directly onto the beach surface, overlaid with compacted clean granularstone material to provide a stable and defined access route for plant and equipment.The ramps will be used for the duration of the marine works to allow controlled movement of excavators and materials between the compound and the beach. 
















Please continue on a separate sheet if necessary. Please tick if you have done this ☐


11. Dredge and Disposal of Dredge Material
If you are undertaking Dredge and Disposal activities please also complete the Dredge and Disposal application form and submit together.

11(a).	Do you intend to apply for a marine licence to dispose of dredged material to sea as part of the works in this application? 			Yes ☐ No ☒

12. Protected Sites

Licensing Authorities have a duty to ensure that projects will not have significant adverse environmental impact, particularly on any designated European Site of Conservation Importance - Special Areas of Conservation (SAC) and Special Protection Areas (SPA), listed under the Habitats Directive (Council Directive 92/42/EEC on the conservation of natural habitats and of wild fauna and flora). In addition, it is Government Policy that Wetlands of International Importance (Ramsar sites) are also considered as European Sites.  There is a duty to take reasonable steps to further the conservation and enhancement of nationally designated sites (Sites of Special Scientific Interest (SSSIs).

12(a).	Have you had pre-application correspondence with NRW, its legacy bodies or Natural England? 								Yes ☐ No ☒


12(a)(i). If Yes, please provide copies of correspondence with application and state which team(s) you have contacted? 

N/A











12(b).	Are any part of the works located within or likely to affect a designated conservation site? (SAC, SPA, SSSI or Ramsar)			 Yes ☒ No ☐

12(b)(i). If Yes, which designated site(s) may be affected?
The Proposed Works are located within the Blackpill Site of Special Scientific Interest (SSSI). This SSSI is designated for its nationally important intertidal habitats and the bird species that rely on them, particularly overwintering and migratory waders. The area supports feeding and roosting opportunities for species such as redshank, oystercatcher and ringed plover, which depend on the ecological integrity of the foreshore. Given the sensitivity of these designated features, the Proposed Works incorporates a series of mitigation measures designed to avoid or minimise any potential impacts on the SSSI. These measures aim to protect both the physical habitat and the bird species that utilise the site throughout the year. As a Marine Licence has been applied for, a separate SSSI assent has not been sought, as it is understood that NRW will consider any potential effects on the SSSI through the Marine Licence application process. A Preliminary Ecological Apprasial has been submitted as part of the application. Additional information on constraints and recommendations on the SSSI can be found in Table 3-1 of PEA for Brockhole Stream Flood Alleviation Scheme – Car Park Wall and New Culvert to Beach Outfall.




















12(c).	Please provide a description of all mitigation measures proposed to avoid any 
impact on designated conservation sites.
Works on the shoreline to be avoided during the overwintering period (November to March) to minimise disturbance. If works during winter are required, then any construction activities (e.g. the cutting of block stones) should be undertaken away from the shoreline within the site compound where possible.
In-situ mitigation measures which should be utilised to minimise disturbance to wintering birds within the SSSI will include
· A suitably qualified ECoW with ornithological experience should be employed throughout the works to advise on potential impacts to wading birds and observe bird behaviour during the works.
· Activities should be restricted during sensitive tidal periods, particularly around high tide roosting times.
· Works should be carefully programmed to minimise the duration and spatial extent of disturbance.
· Temporary acoustic and visual barrier fencing should be installed around the works area to minimise noise and visual disturbance.
· Hand tools should be used where possible during construction activities on the shoreline.
· The works should utilise plant and machinery with lower noise outputs where possible for construction activities on the shoreline (e.g. smaller engines or electric alternatives).
· Plant and machinery should be soft started to minimise sudden noise disturbance.





















Additional information on constraints and recommendations  on the SSSI can be found in Table 3-1 of PEA for Brockhole Stream Flood Alleviation Scheme – Car Park Wall and New Culvert to Beach Outfall.






Please continue on a separate sheet if necessary. Please tick if you have done this ☐

12(d).	If the works are not located within or likely to affect a designated conservation site, please indicated the approximate distance to the nearest designated conservation site.
The Proposed Works are not located within, or in close proximity to, any European designated site under the Conservation of Habitats and Species Regulations 2017 (as amended). The nearest SAC, SPA or Ramsar site is Crymlyn Bog, situated approximately 8 km from the Scheme. The closest hydrologically connected designated site is the Carmarthen Bay and Estuaries SAC, located approximately 20 km away. On this basis, a Habitats Regulations Assessment (HRA) is not required.















Please note that if the proposed works are in or within 2km of a European Site of Conservation Importance you will have to provide suitable mitigation measure to avoid any impact on designated conservation sites.

13. Other Consents

Please detail all consents that you have applied for or received for these works

	Type of Consent
	Applied for
	To be applied for
	Reference Number
	Date of Issue and Expiry

	Planning Permission under Town and County Planning Act 1990 – From Local Planning Authority (LPA)

	Planning permission for FAS.
	
	2022/0703/FUL
	20/05/2022 – this is for full FAS and does not cover anything seaward of MHWS.

	Name and Address of LPA for location of works

	




	Land Owners Consent such as The Crown Estate Consent

	
	
	
	

	Port Authority or Local Harbour permissions

	
	
	
	

	Other NRW consents such as Flood Defence or SSSI assent
	
	
	
	

	Details of NRW consent

	

	Other consents such as Transport and Works Act Order, Section 36 Electricity Act, grant/loan sanction
	
	
	
	

	Details of other consents 


	



14. Statutory Powers

14(a).Does the applicant have statutory powers to consent any aspect of the project? 
E.g. coast protection authority, dredging powers, statutory undertakers	Yes ☒ No ☐

14(a)(i).If Yes, please give details and state the relevant legislation that gives these powers
Permitted development rights









15. Public Register

Under The Marine Licensing (Register of Licensing Information)(Wales) Regulations 2011 and the Environmental Impact Assessment Directive (Directive 85/337/EEC – as amended) , all information contained within or provided in support of this application will be placed on the Public Register unless NRW approve of the applicant’s reasons for withholding all or part.	

15.	Is there any information contained within or provided in support of this application that you consider should NOT be included on the Public Register on the grounds that its disclosure:

15(a).	Would be contrary to the interest of National Security? 		Yes ☐ No ☒

15(b).	Would prejudice to an unreasonable degree you, or some other person’s commercial interest of those of a third party? 			Yes ☐ No ☒

If Yes to either (a) or (b), please provide full justification as to why all or part of the information you have provided should be withheld


N/A












Please continue on a separate sheet if necessary. Please tick if you have done this ☐

16. Application Fee

16(a). What are the corresponding fee band for this application? Band 2 ☒ Band 3 ☐

16(b) Band 2 Only
Projects are charged at a fixed fee of £1920. The application will not be processed until the correct fee has been provided.

Please provide the method of payment 

	Method
	Yes (√)
	Reference Number

	Cheque
	
	

	BACS (not remittance no.)
	X


	PRCAPPSWANS105

	World Pay (phone)
	

	



16(c) Band 3 Application only
Band 3 applications are charged at on hourly rate of £120 and are invoiced in arrears. Please complete the details below which will be required for invoicing.


Customer Name




FAO



Purchase order number



Address for invoice





Telephone Number





Email Address




17. Declaration	Comment by Jenkins, Abbie: Jack - can you please sign the declaration, this is required for the named person on the applicant.

I declare that to the best of my knowledge and belief that the information given in this application form and supporting documentation is true.

	WARNING: It is an offence under the Marine and Coastal Access Act 2009, under which this application is made, to fail to disclose information or to provide false or misleading information and can invalidate any licence granted.



[image: ]
Signature														Date	28/05/2026



Name (in capitals)	JACK DAVIES

Position in Company	PRINCIPAL ENGINEER						


Applications cannot be processed unless signed by the Applicant (not agent), the applicant must have appropriate level of authority within the company.

Applications will not be processed unless signed
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