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Authorisation




ENVIRONMENTAL PROTECTION ACT 1990, sect. 37(1)(a)

NOTICE OF MODIFICATION OF
WASTE MANAGEMENT LICENCE




[bookmark: _GoBack]To:	Barrie Lloyd Jones
Of:	Tanygroes Car Dismantlers, Tanygroes, Cardigan

WHEREAS on 1st December 1992 you were granted a Waste Management Licence, licence number 12, by Cyngor Dosbarth Ceredigion relating to land at Tanygroes, Cardigan.

NOTICE is HEREBY GIVEN that the Environment Agency modifies the said conditions as follows:-
Replace the schedule of conditions to the licence with those that are attached to this Notice.

This modification shall take effect from 00.01 hours 14th December 2004.

Dated: 14th December 2004
(Signed)........................................................
	Team Leader Environment Management


N.B.- The person served with this notice may under Section 43 of the 1990 Act appeal against the Agency’s decision to the Secretary of State within six months of the date of the decision or such longer period as the Secretary of State may allow.
Conditions The headings and paragraphs on the following pages have been inserted as examples to show you the intended format of the licence. Please paste in the headings and conditions you require from the waste management library of conditions and delete any headings you do not need.
[bookmark: _Toc462824157][bookmark: _Toc518716106][bookmark: _Toc87330237]Conditions
The headings and paragraphs on the following pages have been inserted as examples to show you the intended format of the licence. Please paste in the headings and conditions you require from the waste management library of conditions and delete any headings you do not need.
[bookmark: _Toc87330238]General considerations
Application of conditions to all waste motor vehicles
The conditions of this licence apply to the recovery (including storage) of all waste motor vehicles as defined by regulation 50 of the End-of-life Vehicles Regulations 2003 and specified waste in section 1.1 working plan.
Technical Requirements for the Treatment and Storage of waste motor vehicles
The storage (including temporary storage) and treatment of waste motor vehicles shall only be carried out at the site if it meets the standards set out in Schedule 5 of the End-of-life Vehicles Regulations 2003. 
Storage and treatment operations of waste motor vehicles shall meet the requirements of Schedule 5 of the ELV Regulations and section 4.4.3 of the working plan. Infrastructure and equipment provided to meet these obligations shall be maintained in working order and shall be used to give effect to their purpose.
The removal of coolants from air-conditioning units shall be in accordance with the “Guidance on the Recovery and Disposal of Controlled Substances Contained in Refrigerators and Freezers” published by the Environment Agency.


[bookmark: _Toc87330239]Specific considerations
Specified waste motor vehicle storage and treatment operations
The Operator is authorised to carry out the activities specified in Table 2.1 

Where discharge to surface water is taking place as part of the site operations the Discharge shall consist solely of surface run off (site drainage) from the treatment and storage areas within the licensed area. The discharge shall be made in the manner and at the place specified as:
discharging via a class 1 interceptor
discharging to the a highways drain 
at National Grid Reference SN 2944 5052
as specified on site drawing in appendix 7 working plan
[bookmark: _Toc465240087]Specified Waste Management Operations & Exempt Waste Management Operations
Where wastes are being brought onto the site for waste management operations which are exempt from licensing under the 1994 Regulations, then the wastes which are subject to the specified waste management operations shall be kept clearly segregated and identified from those wastes which are being kept on the site for the exempt waste management operations.


	Table 2.1   Specified end-of-life vehicle storage and treatment operations

	Specified Operation
	Permitted Waste Types (and European Waste Catalogue number) which may be subject to the Specified Operation
	Limits on Specified Operations

	STORAGE
R13: Storage of wastes pending any of the operations numbered R1 to R12 (excluding temporary storage, pending collection, on the site where it is produced).
D15: Storage of wastes pending any of the operations numbered D1 to D14 (excluding temporary storage, pending collection, on the site where it is produced
	(i) 16 01 04 End of life vehicles **
	Maximum storage capacity 100 vehicles stored on an Impermeable Pavement with a sealed drainage system
Un depolluted vehicles shall only be stored in accordance with section 4.4.1 working plan 

	
	(ii) 16 01 06 End of life vehicles (containing neither liquids nor other hazardous components)
	Maximum storage capacity 1250 vehicles
Depolluted vehicles may only be stored on designated areas as marked in appendix 8 working plan

	
	(iii) Residual wastes produced as a result of depollution or further treatment (see appendix A for full list and EWC codes)
	Maximum storage capacity 50 tonnes, not exceeding 10 tonnes of hazardous waste.
Residual waste arising from depollution of vehicles shall only be stored in areas marked in appendix 8 working plan
Maximum storage time of 1 year prior to disposal or 3 years prior to recovery

	
	
	The overall maximum storage capacity shall not exceed 1250 vehicles and 50 tonnes of residual waste, not exceeding 10 tonnes of hazardous waste removed from depolluted vehicles

	TREATMENT
R3: Recycling / reclamation of metals and metal compounds:
R4: Recycling / reclamation of other inorganic materials
	
(i) 16 01 04 End of life vehicles **
	50 vehicles per week
Treatment of vehicles shall only be carried out in accordance with section 4.4.3 working plan

	
	(ii) 16 01 06 End of life vehicles containing neither liquids nor other hazardous components)
	50 vehicles per week

	
DISCHARGE TO SURFACE WATER



	Surface run off from the treatment and storage areas within the licensed area
	As far as it is reasonably practicable the works               shall be operated so as to prevent the                            Discharge from containing any significant trace               of visible oil or grease

	
	
	The overall annual throughput of the site shall not exceed 2500 tonnes.



EWC entries marked with a **maybe hazardous depending on threshold concentration. Please refer to Agency Technical Guidance WM2 or subsequently guidance for further advice 

2.3		Fit and proper person 
2.3.1	Any changes in the technically competent management of the site, the name of any incoming person and evidence that such a person has the required technical competence, shall be submitted to the Agency in writing within 5 working days of the change in management.
In the event of the Licence Holder being convicted of any relevant offence and which is in addition to any already notified to the Agency, then full details shall be provided to the Agency within 14 days following sentencing, whether or not the conviction or sentence is subsequently appealed. Such details shall include the nature of the offence, the place and date of conviction, and any fine or other penalty imposed.
In the event that the Licence Holder lodges an appeal against any such conviction, the Licence holder shall notify the Agency of this within 14 days of the lodging. The Licence Holder shall notify the Agency of the results of that appeal within 14 days of the appeal being decided.
2.4		Notification of change of operator’s or holder’s details
The following information shall be notified in writing within 5 working days to the Agency: 
any change in the Licence Holder’s name(s) or address(es);
the operator at the time of issue of the licence and of any change in the operator or in the operator’s trading name, address, registered name or registered office address (if different from the Licence Holder);
Notifications and submissions to the Agency
Except where otherwise specified , all notifications and submissions to the Agency under the requirements of these licence conditions:
shall be made in writing to the address specified by the Agency in writing at the time of issue of this licence, or as subsequently specified by written notification to the Licence Holder
shall quote the licence reference number and the name of the Licence Holder. 



[bookmark: _Toc465240116][bookmark: _Toc465240115][bookmark: _Toc473614491][bookmark: _Toc17878228][bookmark: _Toc87330240]Site engineering for pollution prevention & control
Engineering site containment & drainage systems
Provision & maintenance of site containment & drainage systems
No waste shall be deposited, stored, treated or otherwise handled in any area of the site until the engineered site containment and drainage system for that area has been constructed and completed in accordance with condition 3.1.2. Unless authorised in writing by the Agency.
The engineered site containment and drainage systems shall be designed, constructed, inspected, validated and maintained, and shall be fully documented and recorded, to be fit for purpose and meet the standards specified in Table 3.1 below and in accordance with section 2.1 of the working plan.

	Table 3.1 Site containment & drainage standards

	Type of Site Surface & Drainage
	Minimum Specified Standards of Design, Construction & Maintenance


	Hardstanding
	Areas of hardstanding, which include the areas specified in appendix 6 working plan, shall be constructed of granular material (e.g. crushed stone, aggregate, road planings or other similar material) and maintained such that the working surface:
shall remain even
shall not be subject to settlement or differential settlement
shall not be subject to rutting by vehicles even when wet
shall have sufficient durability to allow cleaning for example by scraping
shall remain free of standing water.


	Impermeable pavement, bunding and sills
	Areas of impermeable pavement, which include the areas specified in appendix 6 working plan, bunding and sills shall be constructed and maintained so as to prevent fluids running off the pavement and the transmission of fluids through the pavement or joints.

Where there is a risk of chemical corrosion, areas of impermeable pavement, kerbs, bunds and sills shall be provided with suitable resistance to minimise such corrosion.


	Sealed drainage systems
	Drainage to areas of impermeable pavement shall be provided by a sealed drainage system, that is comprised of a drainage system with impermeable components which does not leak and which will ensure that:-

no liquid will run off the pavement other than via the system; and
except where they may be lawfully discharged, all liquids entering the system are collected in a sealed sump.
Where the discharge is to surface water and is permitted as part of this waste management licence the discharge shall pass through a Class 1 oil interceptor which shall be operated and maintained in accordance with good operational practice.
Sealed sumps shall be inspected no less frequently than daily and after rain, emptied when the collected liquids reach 80% of the capacity of the sump as measured using a dipstick or equivalent gauge, and constructed and maintained so as to collect and contain all liquids which run off the pavement;
Inspections and emptying of sealed sumps shall be recorded in the site diary.
Uncontaminated drainage from clean yard areas shall be kept separate and discharged to either surface water or sewer or watercourse or soakaway.


	Covered buildings or roofed areas

	Where wastes are stored in a building:
the building, which include the areas specified in appendix 8 working plan,  shall be designed, constructed and maintained to prevent ingress of rain and surface water.
roof water shall be kept separate from contaminated water and other liquids and shall be discharged to either surface water or a sewer or a water course or a soakaway.

	Fixed bays
	Fixed bays and other fixed containers used for the storage and treatment of wastes must be constructed and maintained to a standard which is fit for purpose.

	Storage areas for tanks,skips, drums and other containers
	All tanks, skips, drums and other containers which are used for the storage or treatment of wastes shall be constructed and maintained so that they do not leak any liquids contained in them.

All tanks (and their associated inlet and outlet pipes and valves) which are used for the storage or treatment of wastes shall be stored within a bunded or silled area with impermeable pavement, which include the areas specified in appendix 8  working plan,  shall be isolated from the drainage system and shall meet the following specifications:
The bunded or silled area shall be designed and constructed to contain 110% of the volume of the largest container or tank.
The bunded or silled area shall be inspected no less frequently than weekly and after rain and shall be emptied so as to maintain a capacity of 110% of the volume of the largest container or tank.
Rainwater shall be removed by bailing or pumping and shall be treated as contaminated water and disposed of to either an approved discharge or a suitably licensed or permitted facility.


	Inspection and maintenance of engineered containment
	All areas of hardstanding, impermeable pavement, sealed drainage systems, covered buildings, roofed areas, fixed bays and storage areas for tanks, skips, drums and other containers:
shall be inspected no less frequently than monthly, to ensure the continuing integrity and fitness for purpose of their construction, and the inspection and any necessary maintenance shall be in accordance to section 2  working plan and  recorded in the site diary; and
in the event of any damage occurring which breaches the integrity of the engineered containment so that it no longer meets the specified standards, the Licence Holder shall cease importing waste into or treating waste in the affected area, shall notify the Agency immediately, and shall not recommence importing waste into or treating waste in the affected area until it has been repaired to a standard at least as good as the original specification.




Construction quality assurance of new site containment & drainage systems
No wastes shall be deposited, stored, treated or otherwise handled in any area or any fixed tank for which an engineered site containment and drainage system is to be newly constructed to meet the requirements of this condition until:
details of the identities, relevant experience and relevant qualifications of the personnel who will be providing Quality Assurance of the engineered site containment and drainage systems have been submitted in writing to the Agency and acknowledged in writing by the Agency;
the engineered site containment and drainage system has been constructed in accordance with the other requirements of condition 3.1;
the Validation Report on the construction of the engineered site containment and drainage system has been submitted in writing to the Agency, and the Agency has confirmed in writing that it has no objection to the placement of wastes on that containment area.
Construction quality assurance of existing site containment & drainage systems
No wastes shall be deposited, stored, treated or otherwise handled in any area or any fixed tank for which a previously constructed and existing engineered site containment and drainage system is being used to meet the requirements of this condition unless:
details of the identities, relevant experience and relevant qualifications of the suitably qualified Engineer who will be providing inspection and validation of the existing engineered site containment and drainage systems have been submitted in writing to the Agency and acknowledged in writing by the Agency;
the engineered site containment and drainage system for that area has been inspected by the designated Engineer and has been maintained or improved, in accordance with their recorded advice, to be fit for purpose in that:
areas of impermeable pavement are laid to take weight of relevant vehicles, plant and equipment without cracking or breaking; and
areas of impermeable pavement are free from cracks which could increase permeability; and
areas of impermeable pavement are resistant to mechanical, physical and chemical stresses to which they may be subjected; and
areas of impermeable pavement fall towards the drainage system to prevent ponding; and
no liquid will run off areas of impermeable pavement other than via the drainage system; and
the drainage system is sealed so that it does not leak and is capable of collecting and containing liquids draining from the impermeable pavement ; and
liquid from the drainage system is disposed of to an approved discharge.
The existing engineered site containment and drainage system shall be maintained in accordance with the recommendations of the designated engineer and the requirements of Table 3.1.
All discharges from the impermeable pavements shall pass through a Class 1 oil interceptor which shall be operated and maintained in accordance with good operational practice such that
it remains fully operational except at times of unavoidable mechanical or electrical breakdown which shall be attended to, and the Agency informed of the failure, as soon as possible after the failure;
Following a failure all equipment shall be returned to normal operation as soon as practicable.

[bookmark: _Toc473614492][bookmark: _Toc17878229][bookmark: _Toc87330241]Site infrastructure
Site security
Site security shall be provided in accordance with section 3.1 working plan.
Provision of site identification board
No end-of-life vehicles shall be received at the site unless an identification board is provided at or near the site entrance.
The board shall be easily readable from outside the site entrance in daylight hours, and shall display the following information:
Site name and address;
Licence Holder name (company name, not individual name unless justified as necessary);
Operator  name (company name, not individual name unless justified as necessary);
Licence number;
Emergency contact name and telephone number (for security reasons, personal names and home phone numbers should not be used);
Statement that the site is an Authorised Treatment Facility, licensed by the Environment Agency;
Agency national numbers: 08708 506 506 and 0800 807060 (or any other number subsequently notified in writing by the Agency);
[bookmark: _Toc465240122]Days and hours the site is open to receive waste.

[bookmark: _Toc87330242][bookmark: _Toc465240130][bookmark: _Toc465240125][bookmark: _Toc466865947]Site operations
Leaks & spillages
[bookmark: _Toc465240126][bookmark: _Toc466865948]Potentially polluting leaks & spillages from vehicles, plant & equipment
All vehicles used on the site by the operator, and all plant and all equipment used on the site in connection with specified waste management operations, shall be operated and maintained in accordance to section 4.2 working plan, and with the objective of preventing potentially polluting leaks and spillages of wastes or other potentially polluting materials which are to be used in combination with those wastes in the specified waste management operations.
Potentially polluting leaks & spillages from tanks, skips, drums & other containers
Each tank, skip, drum or other container used to hold wastes which consist of or contain end of life vehicle fluids or hazardous residual wastes, or other potentially polluting materials which are to be used in combination with those wastes in the specified waste management operations shall be:
loaded and unloaded in accordance with the handling procedures specified in Table 5.1;
filled and emptied in accordance with the filling and emptying procedures specified in Table 5.1;
clearly and unambiguously labelled regarding its contents, unless the contents are clearly identifiable by visual inspection;
inspected and maintained according to the maintenance schedules and procedures specified in Table 5.1, which shall be fully documented and recorded;
in the event of damage or deterioration to a container that is, or is likely to cause, a leak, that container shall be repaired or replaced immediately.
[bookmark: _Toc465240129][bookmark: _Toc466865951]Control & remediation of leaks & spillages
All areas of impermeable pavement shall be provided with suitable cleanser-degreaser equipment.

In the event of any potentially polluting leak or spillage occurring on site, documented control and remediation procedures shall be implemented immediately and recorded, and shall meet the standards specified in Table 5.1 below.

5.1.5	Control and remediation of mud and debris shall be in accordance with section 4.1 working plan.
	Table 5.1  Standards for prevention & control of leaks and spillages

	Action
	Specified standards

	Loading and unloading skips, drums and other containers
	Loading and unloading of skips, drums and other containers shall be supervised at all times by a member of staff.
Lids/ caps/ bungs or other closures shall be in place during loading/ unloading.
Loading/ unloading shall be carried out in an area provided with engineered containment of the type required for that waste and of the standard of containment specified under condition 3.1

	Filling and emptying, tanks, drums and other containers

	Filling and emptying of tanks, drums and other containers shall be supervised at all times by a member of staff.
Lids/ caps/ bungs or other closures shall be in place at the end of filling
Containers, tanks and drums shall not be filled beyond their operational capacity.
Filling and emptying shall be carried out in a bunded area maintained in accordance with condition 3.1
Measurement of level/ void space shall be by physical dipping prior to loading.

	Inspection, maintenance and repair of skips, tanks, drums and other containers
	Skips, tanks, drums and other containers shall be inspected daily for leaks.
Any fixed tanks found to be leaking shall have their contents immediately transferred to an alternative appropriate tank or container.
Any skips, drums and/or other containers found to be leaking either shall be immediately transferred to a larger appropriate over-container or shall have their contents immediately transferred to an alternative appropriate tank or container.

	Control and remediation of leaks and spillages
	Minor spillages of oil, fuel or other end of life vehicle fluid shall be cleaned up immediately, using sand or proprietary absorbent to clean up liquids and placed in alternative containers.
Major spillages of oil, fuel or other end of life vehicle fluid which are causing or are likely to cause polluting emissions to the environment: 
Immediate action shall taken to contain the spillage and prevent liquid from entering surface water drains, water courses and unsurfaced ground;
the spillage shall be cleared immediately and placed in alternative appropriate containers;
the Agency shall be informed immediately.



Fires on the site
[bookmark: _Toc465240131]Prohibition of fires on site
No wastes shall be burned on the site. 
Actions to be taken in the event of a fire
In the event of a fire on the site, immediately following taking action to suppress and extinguish the fire, the following actions shall be implemented immediately and recorded in the site diary:
the Agency shall be informed of the fire; and
so far as practicable, contaminated site drainage shall be prevented from entering any surface water drain or water course or unsurfaced ground.
Further control measures in accordance with section 4.3 working plan.
[bookmark: _Toc465240133]Waste acceptance & control procedures
[bookmark: _Toc465240134]Waste acceptance procedures
All wastes shall be received, inspected, accepted or rejected, and recorded in accordance with the standards specified in Table 5.3 below and section 4.4.1 working plan.
[bookmark: _Toc465240135]Waste control procedures 
All wastes accepted at the site shall be handled, kept and recorded in accordance with the standards specified in Table 5.3 below and section 4.4.2 working plan.
Waste despatch procedures
All outgoing wastes shall be inspected, despatched and recorded in accordance with the standards specified in Table 5.3 below.
	Table 5.3 Standards for waste acceptance and control procedures

	Stage of Waste Handling
	Specified standards

	Waste inspection
	All vehicles received at the site:
Shall be inspected on receipt to confirm their description and depollution status against the relevant waste transfer note and any other accompanying documentation. 
Shall be kept segregated from depolluted vehicles until they either been confirmed and recorded as previously having been depolluted or alternatively have been depolluted on site in accordance with the standards set out in Schedule 5 of the End-of-life Vehicles Regulations 2003.

	Waste control procedures: quarantine storage and rejection of wastes

	Any items of non-permitted waste which are detected after acceptance at the site, shall be placed immediately in a designated quarantine container and stored as specified in section 4.4.2 working plan
 Where these are or appear to be special wastes, the Agency shall be informed immediately and a risk assessment carried as specified in section 4.4.2 working plan;
In the quarantine area, wastes shall be kept segregated from other wastes which are or are likely to be incompatible;
Quarantined wastes shall be removed from site within 7 days;
A record shall be kept in the site diary of all rejected wastes and all wastes kept in quarantine storage.

	Identification of wastes
	Storage areas, tanks and other containers shall be clearly defined and labelled to identify the wastes stored within them and shall be located in the area specified in appendix 8 working plan.

	Waste despatch procedures
	All wastes despatched from the site shall be inspected prior to despatch to confirm their description and composition.

	Incompatible wastes

	Incompatible wastes that are likely, in combination with each other or with other material at the facility, to give rise to pollution of the environment or harm to human health outside the site, shall be clearly identified and kept physically separate in designated areas.



Handling and storage of residual wastes
Residual wastes shall only be handled and stored on the site in accordance with the standards specified in Table 5.4 below and table 4.2 of the working plan.

	Table 5.4 Standards for handling and/or storage of residual wastes

	Storage requirement
	Specified standards

	End of life vehicle fluids
	Unless otherwise agreed in writing with the Environment Agency, all fluids drained from vehicles shall be segregated by type and stored in separate, appropriate tanks which are fit for purpose. The tanks shall be clearly and unambiguously labelled regarding their contents.
Brake fluids shall be stored segregated from all other wastes.
Fluids shall only be stored in areas provided with an impermeable pavement and a sealed drainage system provided in accordance with condition 3.1 at the location marked in appendix 8 working plan.

	Batteries, oil filters, oil contaminated parts, PCB/PCT containing condensers, components identified as containing mercury and brake pads containing asbestos.

	Once removed from vehicles, these components shall be segregated by type and stored within dedicated appropriate containers which are fit for purpose. The containers shall be clearly and unambiguously labelled regarding their contents and located in the areas marked in appendix 8 working plan. 
Oil Filters and oil contaminated parts shall only be stored in areas provided with an impermeable pavement and a sealed drainage system.
Other components shall be either stored in areas provided with an impermeable pavement and a sealed drainage system or a sealed lockable container at the locations marked in appendix 8 working plan 
Lead acid batteries shall be stored in containers with an impermeable, acid resistant base and a lid to prevent ingress of surface water, located in the area marked in appendix 8 working plan.

	Tyres, air bags and liquefied gas tanks. 
	Once removed from vehicles, these waste types shall be stored in separately designated areas at the location marked in appendix 8 working plan, on hardstanding or impermeable pavement and sealed drainage in accordance with condition 3.1
Tyres shall be stored in stable stacks at the location marked in appendix 8 working plan.  These must be stable stacks with individual capacities of no greater than 50 cubic metres and to a height of no greater than 3 metres Individual tyre stacks shall not be stored within 6 metres of each other or otherwise recommended by the Fire service
Tyre stacks shall not be stored within 1metre of the site boundary or building
Tyre stacks shall not be located within 10 metres of any area used for flame cutting operations.



	Uncontaminated plastic, glass and ferrous and non-ferrous metal wastes arising from the treatment of end of life vehicles
	i)    These materials shall be stored in areas with hardstanding or impermeable pavement as shown in appendix 8 working plan.


[bookmark: _Toc465240141]
[bookmark: spta]
[bookmark: _Toc87330243]Sampling point requirements

6.1		Inspection chamber 
6.1.2	A appropriately labelled inspection chamber shall be provided and maintained in accordance with section 5.1 working plan at National Grid Reference SN 2946 5051, as shown on the attached Plan reference TCD/001.
6.1.3 	Amenity management and monitoring will be in accordance with section 6 working plan.



[bookmark: _Toc87330244]Site operations

A summary of the waste types and quantities accepted and the waste types and quantities removed from the site shall be made for each financial year and shall be submitted to the Agency within 1 month following the end of that year. The summary record shall be in the format specified in Appendix B, and shall include the specified information. 
[bookmark: _Toc465240160][bookmark: _Toc465240159]Site diary
A site diary shall be kept secure and shall be available for inspection at the site when required by an authorised officer of the Agency.  This shall include a record of the following events, in accordance with the other conditions of this licence:
construction work
maintenance
breakdowns
emergencies
problems with waste received and action taken
technically competent management attendance on site: the date and the time onto site and the time left site
complaints about site operations and actions taken
environmental problems and remedial actions

Each record shall be completed within 24 hours of the relevant event.
[bookmark: _Toc17878233][bookmark: _Toc87330245]Interpretation
In this permit the following expressions shall have the following meanings:

“accepted”
for waste being delivered to the site, shall mean accepted as waste input to the site for storage and/or processing and/or disposal under the specified waste management operations;
“authorised officer of the Agency”
means any person(s) authorised in writing by the Agency pursuant to section 108(1) of the 1995 Act to exercise any of the powers specified in subsection (4) of that section;
"chlorofluorocarbons"
(CFCs) means the controlled substances listed in Group I of Annex I of Regulation (EC) No 2037/2000 of the European Parliament and of the Council of 29 June 2000 on substances that deplete the ozone layer, including their isomers.
 “consequences”
for risk assessments carried out within these conditions, means the adverse effects of harm as a result of realising a hazard which cause the quality of human health (other than health and safety of site staff or visitors to the site covered under the Health and Safety at Work Act 1974) or the environment to be impaired in the short or longer term;
“ELV Regulations” 
means the End of Life Vehicles Regulations 2003 SI 2635.
“End-of-life Vehicles Directive” 
means Directive 2000/53/EC on end-of life vehicles.
 “engineer”
for engineering works specified in these conditions, means a person who works in the relevant branch of engineering, as a qualified professional;
“engineered”
for works specified in these conditions, means carried out and completed using the relevant engineering process specified in these conditions;
 “engineered site containment and drainage system”
means all elements relating to engineered containment of activities on the site, other than final disposal to land, and incorporating site surfacing, bunding and drainage systems, buildings and fixed tanks;
“engineering”
for engineering works specified in these conditions, means the relevant process of design, construction or installation, quality assurance or validation or commissioning specified in these conditions;
 “engineering survey”
means a survey carried out in accordance with recognised or approved standards by a suitably qualified competent person;
 “environmental targets or receptors”
for risk assessments carried out within these conditions, shall mean identified human and environmental populations or components, as specified in these conditions or otherwise agreed by the Agency within these conditions;
 “groundwater”
means any water contained in underground strata;
 “hazard”
means a property or situation that in particular circumstances could lead to harm;
"hydrochlorofluorocarbons" 
(HCFCs) means the controlled substances listed in Group VIII of Annex I of Regulation (EC) No 2037/2000 of the European Parliament and of the Council of 29 June 2000 on substances that deplete the ozone layer, including their isomers,
 “immediately”
for carrying out of actions under the conditions, shall mean without delay and within a reasonable time, taking into account any more immediate direct action necessary to prevent or minimise risk to human health and the environment.  For carrying out notifications to the Agency, shall also mean by the fastest effective means available (for example, telephone) and confirmed in writing within 1 working day (or such other time as may be agreed by the Agency within the conditions);
 “inert waste “
means waste which when disposed of in or on land does not undergo any significant physical, chemical or biological transformation;
“Impermeable surface”
 means a surface or pavement constructed and maintained to a standard sufficient to prevent the transmission of liquids beyond the pavement surface, and should be read in conjunction with the term “sealed drainage system”
“List I and List II substances”
means those substances listed in the Annex to Directive 80/68/EEC;
 “maintenance”
for engineering maintenance specified in  these conditions, means the process of inspection, testing, repair of the relevant engineering works specified in these conditions;
“minor spillage”
any potentially polluting leak or spillage less than 100 litres;
“major spillage”
any potentially polluting leak or spillage greater than 100 litres;
 “preparatory works”
means engineering works required prior to the carrying out of the activities authorised by this licence;
 “probability”
means the quantified expression of chance, denoted either as:
the ratio or percentage of the occurrence of a  particular event as one among a number of possible events; 
or as the frequency of occurrence of a particular event in a given period of time;
“received”
for waste being delivered to the site, shall mean delivered to the site and undergoing the waste acceptance procedures specified in the working plan, including storage of those wastes during those procedures prior to acceptance of the waste;
 “release pathways”
for risk assessments carried out within these conditions, shall mean the routes by which defined hazards may potentially realise their consequences, defined in terms of releases or emissions from the site that go beyond the site containment or boundary via one or more of the following routes, either directly or indirectly: Land; Groundwater; Surface water; Atmosphere;
“relevant offences”
are offences within the meaning of regulation 3 of the Waste Management Licensing Regulations 1994 or any statutory provisions or regulations amending or replacing them;
“risk”
means a combination of the probability and consequences of occurrence of a defined hazard;
“risk assessment”
means the systematic identification, analysis, estimation and evaluation within a defined scope of the defined risks of a particular activity, operation, process or design, carried out and reported by suitably qualified or competent persons, using recognised quantified or semi-quantified methods and techniques.
Unless otherwise agreed by the Agency within these conditions, a risk assessment shall include and record the following:
definition of  the hazards associated with an activity, operation, process or design;
assessment of the probability of those hazards occurring;
determination of the potential consequences of those hazards for defined environmental targets or receptors, taking into account defined release pathways and defined protective measures;
evaluation of the potential magnitude of those consequences and the probability of their occurrence;
 “scope of risk assessment”
means the boundaries of the risk assessment and the risks to be assessed within those boundaries, as defined in the conditions or otherwise agreed by the Agency within the conditions;
“Sealed drainage system” 
in relation to an impermeable pavement, means a drainage system with impermeable components which does not leak and which will ensure that: 
no liquid will run off the pavement otherwise than via the system;
except where they may lawfully be discharged, all liquids entering the system are collected in a sealed sump
“Secure”
A place is secure in relation to end-of-life vehicles or waste kept in it if all reasonable precautions are taken to ensure that the end-of-life vehicles, their contents or waste cannot escape from it.
“special waste”
has the meaning as defined by regulation 2 of the Special Waste Regulations 1996 or any statutory provisions or regulations amending or replacing them;

 “surface water management system”
means all elements relating to collection of rain water or surface water from individual landfill phases and the landfill site as a whole, and incorporating methods of water collection, containment and the subsequent treatment and/or disposal system, either on or off the site;
“surface water”
means any lake, pond, river or watercourse whether natural or artificial;

“Technically competent management”, “technical competence” and “relevant person” 
shall be as defined under Section 74, Environmental Protection Act 1990.
“the 1994 Regulations”
 means the Waste Management Licensing Regulations 1994 and any statutory provisions or regulations amending or replacing them.
 “the Agency”
means the Environment Agency;
 “the Licence Holder”
means the Licence Holder specified in this licence or other person to whom the licence has been transferred in accordance with section 40 of the Environmental Protection Act 1990;
“the operator”
means a person who is in occupation of the site and has responsibility for carrying out day to day activities at the site;
“the site”
means the land, structures, plant and equipment to which this licence relates;
 “time periods, e.g. annually, quarterly, monthly, per year, etc. “
Where periods are referred to in conditions, they shall be calculated in the following way:
annually or per year: 1 April to 31 March;
quarterly: 1 April to 30 June, 1 July to 30 September, 1 October to 31 December, 1 January to 31 March;
monthly: calendar month;
weekly:  Monday to Sunday.
Where the issue of the licence does not coincide with the start of any of these periods, then any relevant limits for the first period shall apply pro rata;
 “waste”
means controlled waste as defined in section 75(4) of the 1990 Act and the Controlled Waste Regulations 1992 or any statutory provisions or regulations amending or replacing them;

"waste motor vehicle" 
means a motor vehicle of any type that is waste and includes an end-of-life vehicle.
“waste oil”
means any mineral-based lubricating or industrial oil which has become unfit for the use for which it was originally intended and, in particular, used combustion engine oil, gearbox oil, mineral lubricating oil, oil for turbines and hydraulic oil;
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Appendix A: EWC Catalogue Numbers (Condition 2.1)

	Residual wastes as a result of depollution or subsequent treatmentTable 4.7.   Permitted quantities of residual waste

	Waste type
	Waste Categories and European Waste Catalogue No.

	Vehicle batteries
	16 06 01 lead batteries *
16 06 05 other batteries and accumulators *

	Oil filters
	16 01 07 oil filters *

	PCB/PCT containing condensers
	16 01 09 components containing PCBs **
16 01 21 hazardous components (other than those mentioned in 16 01 07 to 16 01 11 and 16 01 13 and 16 01 14) **

	Components identified as containing mercury
	16 01 08 components containing mercury **

	Brake pads
	16 01 11 brake pads containing asbestos **
16 01 12 brake pads other than those mentioned in 16 01 11

	Tyres
	16 01 03 end-of-life tyres

	Air bags
	16 01 10 explosive components (for example air bags) *

	Liquefied gas tanks
	16 01 16 tanks for liquefied gas

	End of life vehicle fluids:
Hydraulic Oils




Engine, gear and lubricating oils



Fuel


Air conditioning fluids


Brake fluids
Antifreeze fluids

Any other fluid contained in the end of life vehicle
	

13 01 09 Mineral based chlorinated hydraulic oils *
13 01 10 Mineral based non-chlorinated hydraulic oils *
13 01 11 Synthetic hydraulic oils *
13 01 12 Readily biodegradable hydraulic oils *
13 01 13 Other hydraulic oils *
13 02 04 Mineral based chlorinated engine, gear and lubricating oils *
13 02 05 Mineral based non-chlorinated hydraulic oils *
13 02 06 synthetic engine, gear and lubricating oils *
13 02 07 readily biodegradable engine, gear and lubricating oils *
13 02 08 other engine, gear and lubricating oils *
13 07 01 Fuel oil and diesel *
13 07 02 Petrol *
13 07 03 Other fuels (including mixtures) *
14 06 01 Chloroflurocarbons, HCFC, HFC *
14 06 02 Other halogenated solvents and solvent mixtures *
14 06 03 Other solvents and solvent mixtures *
16 01 13 Brake fluids *
16 01 14 Antifreeze fluids containing dangerous substances ** 
16 01 15 Antifreeze fluids other than those mentioned in 16 01 14
16 01 22 Components not otherwise specified

	Plastic, glass and ferrous and non-ferrous metal wastes arising from the treatment of end of life vehicles 
	16 01 17 Ferrous Metal
16 01 18 Non-ferrous metal
16 01 19 Plastic
16 01 20 Glass



EWC entries marked with a * are hazardous wastes
EWC entries marked with a ** may be hazardous depending on threshold concentrations. Please refer to Agency Technical Guidance WM2 or subsequent guidance for further advice
Waste management licence
General considerations 
Waste management licence
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Appendix B: Format for summary records of wastes accepted and removed (Condition 6.1)
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Section 43(1) of the Environmental Protection Act 1990 provides that, where except in pursuance of a direction given by The National Assembly For Wales,
a licence is granted subject to conditions
the applicant may appeal from the decision to The National Assembly For Wales.
Therefore if you feel aggrieved by the decision or any of the conditions to the licence as granted you may obtain the appropriate form on which to give written notice of an appeal from:

The Planning Inspectorate
Crown Buildings
Cathays Park
Cardiff
CF10 3NQ

Tel: 02920 823859
Fax 02920 825150

This notice of appeal should be accompanied by the following information:
a statement of the grounds of appeal
a copy of the licence
a copy of any correspondence relevant to the appeal
a copy of any other document relevant to the appeal including, in particular, any relevant consent, determination, notice, planning permission, established use certificate or certificate of lawful use or development
a statement indicating whether you wish the appeal to be in the form of a hearing or on the basis of written representations.
You are also required to serve a copy of your notice of appeal together with copies of any of the above documents that have accompanied your notice of appeal, to the Environment Agency. You should appeal within 6 months of the date that this notice takes effect but The National Assembly For Wales may allow notice of appeal to be given after the expiry of this time period.
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