Permit Number: 	EPR/XP3830UR			Operator: 		The First Milk Cheese Company Limited

Facility:		Haverfordwest Creamery		Form Number: 	 Air1 / 17/07/2026
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2][5]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	200 mg/Nm3
	Periodic
	
	MCERTS 
BS EN 14792
	
	

	
	Carbon monoxide
	No limit set
	Periodic
	
	MCERTS BS EN 15058
	
	

	A2
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	200 mg/Nm3
	Periodic
	
	MCERTS
BS EN 14792
	
	

	
	Carbon monoxide
	No limit set
	Periodic
	
	MCERTS BS EN 15058
	
	

	A3
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	200 mg/Nm3
	Periodic
	
	MCERTS
BS EN 14792
	
	

	
	Carbon monoxide
	No limit set
	Periodic
	
	MCERTS BS EN 15058
	
	

	A4
	Oxides of nitrogen (NO and NO2 expressed as NO2)
	95 mg/Nm3
	Periodic
	
	MCERTS BS EN 14792
	
	

	
	Carbon monoxide
	No limit set
	Periodic
	
	MCERTS BS EN 15058
	
	



Notes:
[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
[5] At reference conditions of a temperature of 273.15 K, a pressure of 101.3 kPa and after correction for the water vapour content of the waste gases at a standardised O2 content of 6 % for solid fuels, 15 % for engines and gas turbines and 3 % for all other MCPs

Signed …………………………………………………………….  		Date…………..
	(Authorised to sign as representative of Operator)
