Ynys y Big
      Precautions and Mitigating Measures
Precautions
1. We will select Contractors with the right skills attitudes and track records

2. The Contractors will be comprehensively briefed and closely supervised.

3. All plant will be modern and to a high specification

4. All plant will be inspected for leaks before being allowed on site every day

5. A contingency plan to extract plant will be in place in case of break downs

6. Spill kits will be available close to the plant,

7. No re fuelling will be permitted on beach or within 20m of beach

8. Scaffolds will be man portable and will not be left in place.

9. When it is feasible to use cordless power tools they will be used

Mitigation measures

1. Mud movement will be minimised

2. Re located mud will be spread over existing mud

3. Re located mud will be placed so it is always covered by tide

4. Concrete will be supplied in water proof sacks and will be stored above high tide level and off the beach.

5. Concrete will be laid dry to prevent the formation of concrete liquor

6. Concrete sacks will be bagged immediately to prevent contamination.

7. Excavations will be filled to a level 20mm below top of excavation

8. Concrete will only be laid at times when tide will not return within 1 hour. Cure time is 40 minutes

9. Once cure time has been met a layer of 200mm of mud will be manually placed over concrete to reduce risk of tidal scour.
